(footprint "MR60PB-M_Board_Edge"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(locked yes)
	(layer "F.Cu")
	(property "Reference" "J5"
		(at -8.6 0.85 90)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "d41adf34-3283-45fc-ad8b-bd623ce2de1b")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "MOTOR"
		(at 0 -2.35 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "33071552-6b91-440b-b671-e06e7f5aba51")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Connector_AMASS:MR60PB-M_Board_Edge"
		(at 0 2.75 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c00e1ab2-4ea5-4faa-8bf7-f7103589c49a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 2.75 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "9aa144b2-d104-4b3c-a173-9b3270d868be")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
		(at 0 2.75 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "72bac694-502b-419e-bc7d-a93a21761ff2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Dielectric" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ee5cb7d4-719e-46e4-9b0b-a9dcd3bf60cc")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint_Density" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "56cb771c-121a-404c-887e-3c27b48b8470")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint_Library" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d622c1ff-45a5-420d-9b13-e0f1eadf005e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "JLCPCB Part" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "bc06fec3-8371-47dd-8b4e-7be6c5f98a15")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Mouser" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "99d8bd94-c597-4125-ad65-8942ef4cb2f9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole exclude_from_pos_files exclude_from_bom)
	(fp_poly
		(pts
			(xy -8.3 1.6) (xy -8.15 1.6) (xy -8.15 3.5) (xy -8.3 3.5)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "3e9c0111-d366-4fcf-8d04-4171c5987387")
	)
	(fp_line
		(start -8.45 0)
		(end 8.45 0)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "021e1186-46f6-49c9-ad49-e0e47a12870c")
	)
	(fp_line
		(start -8.45 3.5)
		(end -8.45 0)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "0422c56f-e438-41d1-9c68-57ef1593584f")
	)
	(fp_line
		(start 6.95 5)
		(end -6.95 5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "ad451b74-9a51-40bf-9c87-fd133f4cb495")
	)
	(fp_line
		(start 8.45 0)
		(end 8.45 3.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "c072a71b-fe7c-4158-9b5f-33c6a1741f61")
	)
	(fp_arc
		(start -6.95 5)
		(mid -8.01066 4.56066)
		(end -8.45 3.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "c807037a-ef54-4261-a777-7c5d93d43ab4")
	)
	(fp_arc
		(start 8.45 3.5)
		(mid 8.01066 4.56066)
		(end 6.95 5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "278d00f2-f0e2-43e7-aca1-c915df298028")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -0.85 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "be57b5e6-1c6c-4808-ae99-f0bb91401b28")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" connect roundrect
		(at -5.5 2.4)
		(size 4.9 4.2)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2142857143)
		(chamfer_ratio 0.01)
		(chamfer top_left top_right)
		(uuid "3e898c2f-9eaf-4abe-9a8f-707cacb9612c")
	)
	(pad "2" connect roundrect
		(at 0 2.4)
		(size 4.9 4.2)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2142857143)
		(chamfer_ratio 0.01)
		(chamfer top_left top_right)
		(uuid "4c595786-14ba-470f-8521-ef5a624fc4f0")
	)
	(pad "3" connect roundrect
		(at 5.5 2.4)
		(size 4.9 4.2)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2142857143)
		(chamfer_ratio 0.01)
		(chamfer top_left top_right)
		(uuid "6a131474-bea3-4fdb-8a11-7cf8906564cc")
	)
	(model "${KICAD6_3DMODEL_DIR}/Connector_AMASS.3dshapes/User Library-MR60PB-M.STEP"
		(offset
			(xyz 0 2.2 1.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 0 0)
		)
	)
)
