(footprint "2012_C"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(tags "0805 2012 Capacitor")
	(property "Reference" "C16"
		(at 1.25 0 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "eec4cc20-c382-470f-b099-2541f861f096")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
			(justify left)
		)
	)
	(property "Value" "0.1uF 100V"
		(at 1.25 0.65 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "952d5736-48ca-424b-a548-700cf71d6e67")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.0625)
			)
			(justify left)
		)
	)
	(property "Footprint" "2012_C"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "45798a82-e3e6-4ab8-8aa8-224663ace5d6")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "51c43d6d-0b64-4488-ae34-b2c74cef8c40")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "bffc996f-eea1-4de5-b657-8fa009851966")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Dielectric" "X7R"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "b2f6da93-48c0-498c-b619-5a529950bb55")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint_Density" "C"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "8948fca7-4a77-472a-ae0e-46bec1a8e491")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint_Library" "Capacitor_SMD"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "99b3b5de-2a99-420d-9d80-f84b319f1afd")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Package" "2012"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "7fc403f5-e477-40aa-8de2-63367e5464d3")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Spice_Model" "100n"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "82b4d8fc-5f37-437c-bf29-3e26962d7fd1")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Spice_Netlist_Enabled" "Y"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "796e02af-787c-4b32-8b02-0fac2468e1ca")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Spice_Primitive" "C"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "e9b541ff-160d-4a81-a9d3-c6b1df1280e9")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Tolerance" "10%"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "28a147c5-c248-489b-a04b-311f341cbb04")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Voltage" "100V"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "547280ec-f0ce-4d0b-b3da-3da5dcbeece0")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(solder_mask_margin 0.05)
	(solder_paste_margin -0.05)
	(attr smd)
	(fp_poly
		(pts
			(xy 0.325 -0.65) (xy -0.325 -0.65) (xy -0.325 -0.8) (xy 0.325 -0.8)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "17705a12-89f0-4f03-b789-868753af09cc")
	)
	(fp_poly
		(pts
			(xy 0.325 0.8) (xy -0.325 0.8) (xy -0.325 0.65) (xy 0.325 0.65)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "7c7de7d7-8ed6-437c-ac80-65c9efc1ff35")
	)
	(fp_line
		(start -1.3 -0.45)
		(end -1.3 0.45)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "eb4ea098-e117-4cc8-b2cd-4fc8a18c6e83")
	)
	(fp_line
		(start -1 0.75)
		(end 1 0.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "28a1f598-0b22-411d-929c-0c42f67cd2fe")
	)
	(fp_line
		(start 1 -0.75)
		(end -1 -0.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "044914ef-aca4-4b21-83a1-d099d09a6ed7")
	)
	(fp_line
		(start 1.3 0.45)
		(end 1.3 -0.45)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "76349b9c-36a0-47c6-8df4-2210bd51fd02")
	)
	(fp_arc
		(start -1.3 -0.45)
		(mid -1.212132 -0.662132)
		(end -1 -0.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "e204fb79-6673-4fe3-8c24-054d5f6639e7")
	)
	(fp_arc
		(start -1 0.75)
		(mid -1.212132 0.662132)
		(end -1.3 0.45)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "92f30e65-dbb2-4da3-be57-47c7f8d0e58d")
	)
	(fp_arc
		(start 1 -0.75)
		(mid 1.212132 -0.662132)
		(end 1.3 -0.45)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "d11247f8-8013-41dc-a207-eefc6eff8b36")
	)
	(fp_arc
		(start 1.3 0.45)
		(mid 1.212132 0.662132)
		(end 1 0.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "977b0bda-fa80-4bf9-8970-6666e57596c6")
	)
	(fp_rect
		(start -1 -0.6)
		(end 1 0.6)
		(stroke
			(width 0.025)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "adc23b07-fb14-4e28-9b98-b2645b09abb6")
	)
	(pad "" smd oval
		(at -0.825 0)
		(size 0.5 1)
		(layers "F.Paste")
		(uuid "684493f2-b9d1-44e8-bdef-b9976e57b08f")
	)
	(pad "" smd oval
		(at 0.825 0)
		(size 0.5 1)
		(layers "F.Paste")
		(uuid "fdc4f54e-1052-493d-acdb-d95759715bc1")
	)
	(pad "1" smd roundrect
		(at -0.825 0)
		(size 0.65 1.2)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(chamfer_ratio 0.01)
		(chamfer top_right bottom_right)
		(uuid "041cdd6b-0b0b-4e5c-847c-5aee4d4c6d7f")
	)
	(pad "2" smd roundrect
		(at 0.825 0)
		(size 0.65 1.2)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(chamfer_ratio 0.01)
		(chamfer top_left bottom_left)
		(uuid "37f6a9b6-c340-45a5-a85b-53bca3a9fc84")
	)
	(model "${KICAD7_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
