(module "SSOP-16_3.9x4.9mm_P0.635mm" (layer F.Cu) (tedit 5F33BD87)
  (descr "SSOP16: plastic shrink small outline package; 16 leads; body width 3.9 mm; lead pitch 0.635; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot519-1_po.pdf)")
  (tags "SSOP 0.635")
  (attr smd)
  (fp_text reference "U1" (at 0 -3.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 63435604-5ec1-439a-af94-c3d521ccd632)
  )
  (fp_text value "Genesys_Logic_GL823K-HCY04" (at 0 3.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 3ce7c963-a315-4e4d-9323-12e13de166fa)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer F.Fab)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 0c9d8c3a-aa05-4240-a6c1-9a7544ab662d)
  )
  (fp_line (start -2 2.675) (end 2 2.675) (layer F.SilkS) (width 0.15) (tstamp 1b394364-722b-46a9-a5c4-6b5ae79f2e16))
  (fp_line (start -3.275 -2.725) (end 2 -2.725) (layer F.SilkS) (width 0.15) (tstamp e27ee76d-cae9-4b56-b25e-dc5e78b2ba8f))
  (fp_line (start -3.45 -2.85) (end 3.45 -2.85) (layer F.CrtYd) (width 0.05) (tstamp 02e95ecc-c2f5-4c4e-beb5-eff99d3bf372))
  (fp_line (start -3.45 2.8) (end 3.45 2.8) (layer F.CrtYd) (width 0.05) (tstamp 040ef399-a7c1-4ede-8732-a1314fdbcbb3))
  (fp_line (start -3.45 -2.85) (end -3.45 2.8) (layer F.CrtYd) (width 0.05) (tstamp 94899b9c-4644-4053-9624-e3b46c82bcba))
  (fp_line (start 3.45 -2.85) (end 3.45 2.8) (layer F.CrtYd) (width 0.05) (tstamp bfff6847-027f-47e0-8a6c-c2cb5fb61c88))
  (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.15) (tstamp 80d186cf-2bf5-47ab-9f44-e526bb8dbcab))
  (fp_line (start -0.95 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.15) (tstamp 932dde1b-936f-48b0-8f1a-9a0c775a4b33))
  (fp_line (start -1.95 -1.45) (end -0.95 -2.45) (layer F.Fab) (width 0.15) (tstamp 9e88b61f-0d15-4053-a1e8-a290c407ddbb))
  (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.15) (tstamp a39f56c5-4327-4a5f-992b-5ad899f233cd))
  (fp_line (start -1.95 2.45) (end -1.95 -1.45) (layer F.Fab) (width 0.15) (tstamp bd38c444-673b-4865-8161-5e6f2a68c4d8))
  (pad "1" smd roundrect (at -2.6 -2.2225) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 6184952c-e6eb-4b35-a598-bc660a60287e))
  (pad "2" smd roundrect (at -2.6 -1.5875) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 76124fbf-6c99-430e-8a78-104fc1d1c2a4))
  (pad "3" smd roundrect (at -2.6 -0.9525) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 758d2e61-f8b1-4936-bed9-78430969fbfa))
  (pad "4" smd roundrect (at -2.6 -0.3175) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 059b39b0-af53-43c2-9536-84852e9cb543))
  (pad "5" smd roundrect (at -2.6 0.3175) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 30e98ca6-9240-4703-9d64-1b864c8eccc1))
  (pad "6" smd roundrect (at -2.6 0.9525) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp fb8df69b-de30-41f1-bd30-0ab26055f42e))
  (pad "7" smd roundrect (at -2.6 1.5875) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 20639c15-ce22-4b5e-b983-20c64898d9fb))
  (pad "8" smd roundrect (at -2.6 2.2225) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 1c9b71b5-3b97-4b39-b826-e73719d30530))
  (pad "9" smd roundrect (at 2.6 2.2225) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e15cc51d-0c3c-42f3-ae96-f8fcb5b1fb3c))
  (pad "10" smd roundrect (at 2.6 1.5875) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d76262ee-91b5-42a8-b945-de7986274b18))
  (pad "11" smd roundrect (at 2.6 0.9525) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 51bda433-a0ee-417d-bb18-b079716cb2a4))
  (pad "12" smd roundrect (at 2.6 0.3175) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c3b97059-ede1-47f8-9d5f-8002659aa3e2))
  (pad "13" smd roundrect (at 2.6 -0.3175) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c6302380-0e45-48fa-b3f5-1b8b4eaa094e))
  (pad "14" smd roundrect (at 2.6 -0.9525) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f19102fb-8e99-4029-a338-169da4c24c92))
  (pad "15" smd roundrect (at 2.6 -1.5875) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 72f69e8b-4b30-4266-9f20-7f7e56f09c3a))
  (pad "16" smd roundrect (at 2.6 -2.2225) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 436fdad4-9976-4d0d-bddd-c36cceaa28cc))
  (model "${KICAD7_3DMODEL_DIR}/Package_SO.3dshapes/SSOP-16_3.9x4.9mm_P0.635mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
