(footprint "XT30-PB_Dual_Mount" (version 20220427) (generator pcbnew)
  (layer "F.Cu")
  (property "Dielectric" "")
  (property "Footprint_Density" "")
  (property "Footprint_Library" "")
  (property "JLCPCB Part" "")
  (property "LCSC" "")
  (property "MFG" "")
  (property "MPN" "DO NOT POPULATE")
  (property "MPN_ALT1" "")
  (property "Mouser" "")
  (property "Note" "")
  (property "Package" "")
  (property "Sheetfile" "ESC_Dual_10A.kicad_sch")
  (property "Sheetname" "")
  (property "Spice_Model" "")
  (property "Spice_Netlist_Enabled" "")
  (property "Spice_Primitive" "")
  (property "Tolerance" "")
  (property "USD_per_1" "")
  (property "USD_per_1000" "")
  (property "Voltage" "")
  (property "exclude_from_bom" "")
  (property "ki_description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
  (property "ki_keywords" "screw terminal")
  (zone_connect 2)
  (attr through_hole exclude_from_bom)
  (fp_text reference "J1" (at 0 3.25 unlocked) (layer "Cmts.User")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 4fb5a237-5acb-4b80-ba9e-0666a4f1b448)
  )
  (fp_text value "Vin" (at 4.85 -2.15 90 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp 310b81cc-310a-4f75-a56d-b49eca746a3e)
  )
  (fp_text user "${REFERENCE}" (at -4.7 -2.25 90 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp 07872799-bb0e-474f-9510-4dbc5de6888d)
  )
  (fp_text user "+" (at -4.8 0 unlocked) (layer "F.Fab")
      (effects (font (size 1.5 1.5) (thickness 0.375) bold))
    (tstamp 7dffee09-6f2a-4cb0-a718-1c39d5669b70)
  )
  (fp_line (start -5.05 -2.55) (end -5.05 -1.55)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 8be44c45-f5e2-4d0b-a214-6a9baf9c2482))
  (fp_line (start -5.05 2.55) (end -5.05 1.55)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp f3867c8f-1cc1-4b48-be63-150c7cbce304))
  (fp_line (start -5.05 2.55) (end -4.25 2.55)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp a1a7a71d-0ab4-452d-bbe8-6d3ce3c82fbd))
  (fp_line (start -4.25 -2.55) (end -5.05 -2.55)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 006bb8be-e247-488c-a7b2-cadceddc9154))
  (fp_line (start 5.05 -2.05) (end 5.05 -1.55)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 76f23493-98f7-4822-91d9-3302fd19672e))
  (fp_line (start 5.05 1.55) (end 5.05 1.75)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 36425299-b498-4781-b7fb-eb32065bb42d))
  (fp_arc (start 4.55 -2.55) (mid 4.903553 -2.403553) (end 5.05 -2.05)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp e65ee7ec-7bea-49fb-95db-765f857a5182))
  (fp_arc (start 5.05 1.75) (mid 4.815685 2.315685) (end 4.25 2.55)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp fbb81d2c-b5a2-4eda-b936-b807fa852120))
  (fp_line (start -5.35 2.6) (end -5.35 -2.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4d3a5703-dc79-434e-8061-cb568b5db544))
  (fp_line (start -5.1 -2.85) (end 5.1 -2.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 382c188f-45fa-4a2a-980a-3d389f6763f2))
  (fp_line (start 5.1 2.85) (end -5.1 2.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 08d43e0e-3e94-4ad6-950d-83fbb31ff00c))
  (fp_line (start 5.35 -2.6) (end 5.35 2.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 89d226d7-50f4-4fad-9629-7e04691ae913))
  (fp_arc (start -5.35 -2.6) (mid -5.276777 -2.776777) (end -5.1 -2.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f3ab40cd-ed8b-4671-bcbe-5f75105f4345))
  (fp_arc (start -5.1 2.85) (mid -5.276777 2.776777) (end -5.35 2.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 418d08c3-b067-44c9-9d06-26965781a01a))
  (fp_arc (start 5.1 -2.85) (mid 5.276777 -2.776777) (end 5.35 -2.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp fc80ca06-e55e-4dda-8828-8923f1ea1408))
  (fp_arc (start 5.35 2.6) (mid 5.276777 2.776777) (end 5.1 2.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 01e959f2-d744-4b8b-b396-54db034cb848))
  (fp_line (start -5.1 -13.3) (end 5.1 -13.3)
    (stroke (width 0.05) (type dash)) (layer "F.Fab") (tstamp 085ba9d0-1d9f-477a-93a7-5d1217cc2168))
  (fp_line (start -5.1 -2.6) (end -5.1 -13.3)
    (stroke (width 0.05) (type dash)) (layer "F.Fab") (tstamp 1ae990bf-919e-456e-9ad3-ce647693fcfc))
  (fp_line (start 5.1 -13.3) (end 5.1 -2.6)
    (stroke (width 0.05) (type dash)) (layer "F.Fab") (tstamp a5838a99-2094-427d-9f9f-fda2c76df4e9))
  (fp_rect (start -5.1 -2.6) (end 5.1 2.6)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.Fab") (tstamp 9dc8ef5d-5837-4600-8605-e646a77b8be7))
  (pad "1" thru_hole circle (at -4.3 -2.1) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 6631683d-72ea-45da-b4d1-cd44a2effa71))
  (pad "1" thru_hole circle (at -4.3 -1.5) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp da6bba99-5066-40c4-9276-78829fa3a207))
  (pad "1" thru_hole circle (at -4.3 -0.9) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp c0337c02-917a-4e7f-8150-fb5c27616791))
  (pad "1" thru_hole circle (at -4.3 -0.3) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 5ab2f674-8217-47c6-b3e6-4a76a3e4c8ec))
  (pad "1" thru_hole circle (at -3.9 0.9) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp d1d7bfe2-e62e-4011-97b9-5bb7a839926f))
  (pad "1" thru_hole circle (at -3.7 -2.1) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 9bdd41fc-be5e-4a74-89d0-3c20a1e9378d))
  (pad "1" thru_hole circle (at -3.7 -1.5) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 06b2f24b-4fd0-4af3-849b-744e9e4998b5))
  (pad "1" thru_hole circle (at -3.7 -0.9) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 90faddd6-8a9e-49a9-9997-afbd56b9e7a6))
  (pad "1" thru_hole circle (at -3.7 -0.3) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 615623e7-fe22-4d48-9072-300959496189))
  (pad "1" thru_hole circle (at -3.7 0.3) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp b17f604e-4288-4758-89ff-78863cd88bc9))
  (pad "1" thru_hole circle (at -3.3 0.9) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 51b4f10c-ef89-4fb6-8ff0-8282d68ab4b4))
  (pad "1" thru_hole circle (at -3.3 1.5) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp b4106d0b-5b20-4b88-9e77-5a14e47ee553))
  (pad "1" thru_hole circle (at -3.1 -2.1) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 7f0052db-9b57-43e5-859f-8c84488ef993))
  (pad "1" thru_hole circle (at -3.1 -1.5) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 1ea0c77b-a56d-410e-9b3c-0713c58daa68))
  (pad "1" thru_hole circle (at -2.8 1.2) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp c1632080-5de5-401b-8812-ea14f7ea34cb))
  (pad "1" thru_hole circle (at -2.5 -2.1) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 5c1f2bbd-79e9-4583-a080-4be65513dc66))
  (pad "1" thru_hole circle (at -2.5 -1.5) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp e7be3c22-dd6a-48ce-bf57-b8231867217d))
  (pad "1" connect rect (at -2.5 -1.2) (size 4.1 2.4) (layers "F.Cu" "F.Mask") (tstamp b5fe4887-77ba-4a5c-b229-c20db8a357fb))
  (pad "1" thru_hole circle (at -2.5 0) (size 4.1 4.1) (drill 1.7) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp 57b3b2d3-2eab-4a73-afe8-371345260a2d))
  (pad "1" thru_hole circle (at -2.5 1.7) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 8bad3637-cd01-46a8-a959-e9a491afeb19))
  (pad "1" thru_hole circle (at -2.2 1.2) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 76f1bdf1-c4af-4fe7-97af-fd7615e19689))
  (pad "1" thru_hole circle (at -1.9 -2.1) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp fbf1874b-8e3f-48ec-aa0e-677d77104913))
  (pad "1" thru_hole circle (at -1.9 -1.5) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 790d2aa9-0743-40fe-afcc-4011433a6611))
  (pad "1" thru_hole circle (at -1.7 0.9) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp b1f84516-6101-4a1c-985e-6f2f60bc9082))
  (pad "1" thru_hole circle (at -1.7 1.5) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 651586db-7465-4b86-8aaa-c9838e5fc4e2))
  (pad "1" thru_hole circle (at -1.3 -2.1) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 3ff073f2-b746-4630-9d6d-08a6ef9b7ba1))
  (pad "1" thru_hole circle (at -1.3 -1.5) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp e40c2667-9d3d-415d-8797-db5cc33c8ef8))
  (pad "1" thru_hole circle (at -1.3 -0.9) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 831e38d2-0c5e-4936-8602-b1b7a3dd8006))
  (pad "1" thru_hole circle (at -1.3 -0.3) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 6f422604-1196-4792-8cc2-cbb8149745cd))
  (pad "1" thru_hole circle (at -1.3 0.3) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp a41f19b7-81eb-40e0-94e1-7af0cc34589f))
  (pad "1" thru_hole circle (at -1.1 0.9) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 69aea374-d214-4d72-892b-de61ebac35c6))
  (pad "1" thru_hole circle (at -0.7 -2.1) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp dedde551-cb23-4465-b0b2-989f78817548))
  (pad "1" thru_hole circle (at -0.7 -1.5) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 4ad7eeed-8d4e-44c5-a2d0-505e60545a74))
  (pad "1" thru_hole circle (at -0.7 -0.9) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 54b4d448-a4ba-4926-bccf-6a24db782841))
  (pad "1" thru_hole circle (at -0.7 -0.3) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 629e5fdc-63b7-42f4-a58e-c9956dc2dffe))
  (pad "2" thru_hole circle (at 0.7 -2.1) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 3a27c2c0-275a-4deb-929d-fd736982c0f5))
  (pad "2" thru_hole circle (at 0.7 -1.5) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp fad5a859-3317-4e39-a74a-64f89bd25e34))
  (pad "2" thru_hole circle (at 0.7 -0.9) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 002ff9f9-cbeb-47f7-a5ac-a9531658d040))
  (pad "2" thru_hole circle (at 0.7 -0.3) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 40820f9a-a2c9-4001-b672-35f40d4bf5a2))
  (pad "2" thru_hole circle (at 1.1 0.9) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp fe49a665-70ec-4a36-8e49-46a59486c4c5))
  (pad "2" thru_hole circle (at 1.3 -2.1) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp d6546c41-a6e2-4348-a3b2-65d20ec9baf3))
  (pad "2" thru_hole circle (at 1.3 -1.5) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp d31f62da-b1dc-44a8-8d7f-7be03d3c70b6))
  (pad "2" thru_hole circle (at 1.3 -0.9) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 902665de-8af9-4f6a-9c6e-0dacef1d7a55))
  (pad "2" thru_hole circle (at 1.3 -0.3) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 7e6b001b-7af0-4c39-9532-e0275ddf9b43))
  (pad "2" thru_hole circle (at 1.3 0.3) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 6296e565-feb6-474a-af3b-ff709bf6a6ea))
  (pad "2" thru_hole circle (at 1.7 0.9) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 3bf6b104-3b18-4bc8-8366-6a2efc3ebbfe))
  (pad "2" thru_hole circle (at 1.7 1.5) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 492c73c0-a189-41f6-9c80-5ac5c07a0bb4))
  (pad "2" thru_hole circle (at 1.9 -2.1) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 8026d646-8b68-459a-a85a-4bc42f8a134f))
  (pad "2" thru_hole circle (at 1.9 -1.5) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 500942ef-8f75-49e3-b277-d78459d37139))
  (pad "2" thru_hole circle (at 2.2 1.2) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 60cdfb98-3502-4bea-a090-0b87eda5319f))
  (pad "2" thru_hole circle (at 2.5 -2.1) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp c9f8e757-d230-4f45-8554-2f9ed79f1b2f))
  (pad "2" thru_hole circle (at 2.5 -1.5) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 0c6974db-2a66-4b6c-ad1d-d8f1609dee82))
  (pad "2" connect rect (at 2.5 -1.2) (size 4.1 2.4) (layers "F.Cu" "F.Mask") (tstamp 80769803-3419-4230-91ed-de14e27da4d8))
  (pad "2" thru_hole circle (at 2.5 0) (size 4.1 4.1) (drill 1.7) (layers *.Cu *.Mask) (remove_unused_layers) (keep_end_layers) (tstamp a9f88e1f-2ca9-4ae9-9e44-bc4c4a18ee35))
  (pad "2" thru_hole circle (at 2.5 1.7) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 31ea685c-c19f-4f3c-ab55-22c6f08b3a4f))
  (pad "2" thru_hole circle (at 2.8 1.2) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 4c32bf0b-e67c-4fe3-82fb-c2dd204eee83))
  (pad "2" thru_hole circle (at 3.1 -2.1) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 68b70e33-0444-4a04-8615-5ee402cd8ff2))
  (pad "2" thru_hole circle (at 3.1 -1.5) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 6c957e16-17f2-4ce4-8042-56fe60f9e0c9))
  (pad "2" thru_hole circle (at 3.3 0.9) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp d1d9b401-e87e-4b8d-83d7-f5931058ce26))
  (pad "2" thru_hole circle (at 3.3 1.5) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 015d94db-5548-4779-b8da-f890f8cf4d5a))
  (pad "2" thru_hole circle (at 3.7 -2.1) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 350f9aa8-cd79-405b-8d92-bf6578c05c09))
  (pad "2" thru_hole circle (at 3.7 -1.5) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp d2a547e5-df33-4732-a7bb-3244bf34fffb))
  (pad "2" thru_hole circle (at 3.7 -0.9) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 53104a91-7b51-46e4-8922-da8546d15a3d))
  (pad "2" thru_hole circle (at 3.7 -0.3) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp dad8f752-f244-45b4-ab36-629f45aa7e8d))
  (pad "2" thru_hole circle (at 3.7 0.3) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp cc1bdd03-0b6f-49e3-ae64-6bd07fa6fda9))
  (pad "2" thru_hole circle (at 3.9 0.9) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp a5a7bf84-5c29-4952-8edb-a5aadc68b4b4))
  (pad "2" thru_hole circle (at 4.3 -2.1) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 44b726fe-fe63-4d5b-adf2-b66f55040fb7))
  (pad "2" thru_hole circle (at 4.3 -1.5) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 53c798d9-f50f-49c5-8ca4-6f9863257926))
  (pad "2" thru_hole circle (at 4.3 -0.9) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 7cd2b356-8529-4c19-8210-7f3aea4a8f15))
  (pad "2" thru_hole circle (at 4.3 -0.3) (size 0.5 0.5) (drill 0.25) (layers *.Cu "F.Mask") (remove_unused_layers) (tstamp 83afeb62-aef0-45d6-8f32-3e66f8e97916))
  (model "${KICAD7_3DMODEL_DIR}/Connector_AMASS.3dshapes/Amass_XT30UPB-M.wrl"
    (offset (xyz 0 2.6 0.7))
    (scale (xyz 1 1 1))
    (rotate (xyz 90 -180 0))
  )
)
