(module CUI_CSS-95B30-SMT (layer F.Cu) (tedit 57EFE16B)
  (solder_mask_margin -0.04)
  (solder_paste_margin -0.05)
  (attr smd)
  (fp_text reference SP1 (at 0 5.5 180) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value BEEP (at 0 1) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_line (start -5 5) (end -5 4) (layer F.SilkS) (width 0.125))
  (fp_line (start 5 5) (end 5 4) (layer F.SilkS) (width 0.125))
  (fp_line (start 5 -5) (end 5 -4) (layer F.SilkS) (width 0.125))
  (fp_line (start -5 -5) (end -5 -4) (layer F.SilkS) (width 0.125))
  (fp_line (start -4 5) (end -5 5) (layer F.SilkS) (width 0.125))
  (fp_line (start 5 5) (end 4 5) (layer F.SilkS) (width 0.125))
  (fp_line (start 4 -5) (end 5 -5) (layer F.SilkS) (width 0.125))
  (fp_line (start -5 -5) (end -4 -5) (layer F.SilkS) (width 0.125))
  (fp_line (start -1 -3) (end 1 -3) (layer F.SilkS) (width 0.125))
  (fp_line (start -2 -5) (end 2 -5) (layer F.SilkS) (width 0.125))
  (fp_line (start 2 -5) (end 1 -3) (layer F.SilkS) (width 0.125))
  (fp_line (start 1 -3) (end 1 -2) (layer F.SilkS) (width 0.125))
  (fp_line (start 1 -2) (end -1 -2) (layer F.SilkS) (width 0.125))
  (fp_line (start -1 -2) (end -1 -3) (layer F.SilkS) (width 0.125))
  (fp_line (start -1 -3) (end -2 -5) (layer F.SilkS) (width 0.125))
  (fp_line (start -5.5 -5.5) (end 5.5 -5.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5.5 -5.5) (end 5.5 5.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5.5 5.5) (end -5.5 5.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.5 5.5) (end -5.5 -5.5) (layer F.CrtYd) (width 0.05))
  (fp_circle (center -5.7 -4.6) (end -5.6 -4.6) (layer F.SilkS) (width 0.125))
  (fp_line (start -5 4) (end -4 5) (layer F.SilkS) (width 0.125))
  (pad 4 smd roundrect (at -5 3) (size 1.8 1.8) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (pad 3 smd roundrect (at 5 3) (size 1.8 1.8) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (pad 2 smd roundrect (at 5 -3) (size 1.8 1.8) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (pad 1 smd roundrect (at -5 -3) (size 1.8 1.8) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (model ${KICAD7_3DMODEL_DIR}/Buzzer_Beeper.3dshapes/CUI_INC_CSS-95B30-SMT.step
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 180))
  )
)
