(footprint "Crystal_4-SMD_2.5x2mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Sheetfile" "QuadCameraCarrier.kicad_sch")
  (property "Sheetname" "")
  (solder_mask_margin 0.001)
  (solder_paste_margin -0.025)
  (attr smd)
  (fp_text reference "Y2" (at 0 -1.675 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 49c876d4-7ed5-409a-962c-978a3028fb9c)
  )
  (fp_text value "Crystal_small_4P" (at 0 0.75) (layer "F.Fab") hide
      (effects (font (size 0.6 0.6) (thickness 0.15)))
    (tstamp ea17fcb9-b209-4f80-9b23-f9239bace994)
  )
  (fp_rect (start -1.65 -1.05) (end -1.5 -0.8)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 825907cd-5018-43dd-a96e-ab55ab11235c))
  (fp_rect (start -1.25 -1.3) (end -1 -1.45)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 2d67a4bc-ef22-430e-ac69-f7cb7dddba36))
  (fp_rect (start 1.25 -1.45) (end 1 -1.3)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp d8260ffe-ca47-45b3-9168-7f4cd294ba2b))
  (fp_rect (start 1.25 1.3) (end 1 1.45)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 1d4a5987-1348-4240-9383-dc55e3af790e))
  (fp_rect (start 1.5 -1.05) (end 1.65 -0.8)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 22cc034f-086e-43c8-b22e-94e00cf44ee9))
  (fp_rect (start 1.65 1.05) (end 1.5 0.8)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 0564c342-2dd5-487f-bf13-1a5067f1af47))
  (fp_arc (start -1.575 -1.05) (mid -1.47981 -1.27981) (end -1.25 -1.375)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp b535a853-5568-47dc-b05b-71e25e2b8d84))
  (fp_arc (start 1.25 -1.375) (mid 1.47981 -1.27981) (end 1.575 -1.05)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp c9fb5af2-2806-480f-a3ba-e2fdee39fea9))
  (fp_arc (start 1.575 1.05) (mid 1.47981 1.27981) (end 1.25 1.375)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp c94a3835-75f3-496c-ad0b-2c8dc4c14e41))
  (fp_poly
    (pts
      (xy -1.5 1.3)
      (xy -1 1.3)
      (xy -1 1.45)
      (xy -1.65 1.45)
      (xy -1.65 0.8)
      (xy -1.5 0.8)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 0677920b-d8ac-404c-8584-aa222b70f376))
  (fp_line (start -1.6 1.05) (end -1.6 -1.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d5e34274-6259-41fd-8ecd-ea9a0b51029b))
  (fp_line (start -1.25 -1.4) (end 1.25 -1.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 96cb09cd-a786-4186-840e-1736ebc0f5a6))
  (fp_line (start 1.25 1.4) (end -1.25 1.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ebc316e9-ca49-445b-a9fc-7a8cd8605d12))
  (fp_line (start 1.6 -1.05) (end 1.6 1.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 5599cfe4-7444-4ece-a8a0-8a091ebc0591))
  (fp_arc (start -1.6 -1.05) (mid -1.497487 -1.297487) (end -1.25 -1.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f20c1261-8fe0-4ced-9e8c-bb3a9623e1bf))
  (fp_arc (start -1.25 1.4) (mid -1.497487 1.297487) (end -1.6 1.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6e9c99c5-ddad-4141-8312-57a455ae5bfe))
  (fp_arc (start 1.25 -1.4) (mid 1.497487 -1.297487) (end 1.6 -1.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f1b9ebed-c999-414c-8ca3-225e2d667b34))
  (fp_arc (start 1.6 1.05) (mid 1.497487 1.297487) (end 1.25 1.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 85e0884b-7da3-43ac-99e0-f73f682dcb11))
  (fp_line (start -1.25 -1) (end -1.25 -1)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 5b69352f-ff87-4184-87ce-b3b353ef34b7))
  (fp_line (start -1.25 -1) (end 1.25 -1)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 805f7ae7-e7d2-45c4-be63-26c8340386a2))
  (fp_line (start -1.25 1) (end -1.25 -1)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp ff8471d0-6506-4ea6-abd7-604c2bc12c41))
  (fp_line (start 1.2 -1.05) (end 1.2 -1.05)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 16656b85-f7c9-4de5-80ff-39bf2d28b4ad))
  (fp_line (start 1.25 -1) (end 1.25 1)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 2e362fc9-a019-4752-8e7f-4c2c01f3b843))
  (fp_line (start 1.25 1) (end -1.25 1)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 9be09cf2-ce44-4dc2-92b3-14aadd4ec842))
  (fp_line (start 1.25 1) (end 1.25 1)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 822d22c4-fdf3-4e13-a855-d512b88cd158))
  (pad "" smd roundrect (at -0.85 -0.7) (size 1 1) (layers "F.Paste") (roundrect_rratio 0.33) (tstamp 33d633cf-da6e-4309-b2a4-a32729996841))
  (pad "" smd roundrect (at -0.85 0.7) (size 1 1) (layers "F.Paste") (roundrect_rratio 0.33) (tstamp 3ded0a3b-58bc-49c3-ab8d-fede8294eed8))
  (pad "" smd roundrect (at 0.85 -0.7) (size 1 1) (layers "F.Paste") (roundrect_rratio 0.33) (tstamp b701c8b9-d51e-42de-89c3-b45b59219b53))
  (pad "" smd roundrect (at 0.85 0.7) (size 1 1) (layers "F.Paste") (roundrect_rratio 0.33) (tstamp 2e2c3db8-53ec-4107-817e-07b6b77256f3))
  (pad "1" smd roundrect (at -0.85 0.7) (size 1.2 1.1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1818181818)
    (chamfer_ratio 0.05) (chamfer top_right) (tstamp cdaca02f-8ed3-451e-92b2-374a26a18dce))
  (pad "2" smd roundrect (at 0.85 0.7) (size 1.2 1.1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1818181818)
    (chamfer_ratio 0.05) (chamfer top_left) (tstamp 76383879-f136-4df6-a982-7a7fc5db5cfd))
  (pad "3" smd roundrect (at 0.85 -0.7) (size 1.2 1.1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1818181818)
    (chamfer_ratio 0.05) (chamfer bottom_left) (tstamp a84fbfec-9867-4f89-8d0a-5866961a30ff))
  (pad "4" smd roundrect (at -0.85 -0.7) (size 1.2 1.1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1818181818)
    (chamfer_ratio 0.05) (chamfer bottom_right) (tstamp 84630631-d5bc-4293-8146-6056ffb3cc0c))
  (model "${KICAD7_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_4P_2520.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
