(module JP-12_2R_2mm (layer F.Cu) (tedit 56E868DC)
  (fp_text reference JP (at -5 -2.5) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text value VAL** (at 0 -2.5) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_line (start -4 -2) (end -4 0) (layer F.SilkS) (width 0.125))
  (fp_line (start -4 0) (end -6 0) (layer F.SilkS) (width 0.125))
  (fp_line (start -6 2) (end 6 2) (layer F.SilkS) (width 0.125))
  (fp_line (start 6 2) (end 6 -2) (layer F.SilkS) (width 0.125))
  (fp_line (start 6 -2) (end -6 -2) (layer F.SilkS) (width 0.125))
  (fp_line (start -6 -2) (end -6 2) (layer F.SilkS) (width 0.125))
  (pad 1 thru_hole rect (at -5 -1) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -5 1) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -3 -1) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at -3 1) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at -1 -1) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at -1 1) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at 1 -1) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 1 1) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at 3 -1) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
  (pad 10 thru_hole circle (at 3 1) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
  (pad 11 thru_hole circle (at 5 -1) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
  (pad 12 thru_hole circle (at 5 1) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
  (model 3D/walter/pin_strip/pin_strip_2mm_6x2.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
