(footprint "HSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.1mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "HSOP, 8 Pin (https://www.st.com/resource/en/datasheet/l5973d.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
  (tags "HSOP SO")
  (property "LCSC" "C90665")
  (property "MFG" "TI")
  (property "MPN" "LMR16030PDDAR")
  (property "Sheetfile" "../../library/blocks/60 to 10V 0.5A Buck Converter.kicad_sch")
  (property "Sheetname" "60V to 10V buck")
  (attr smd)
  (fp_text reference "U1" (at 0 -3.4) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 39e700e1-aece-4763-a4a7-117225c61da1)
  )
  (fp_text value "LMR16030P" (at 0 3.4) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 87561161-21bf-4cfd-b36e-78c0d30ce422)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.98 0.98) (thickness 0.15)))
    (tstamp 7a762919-872e-4559-8c46-c1911cefbf36)
  )
  (fp_line (start 0 -2.56) (end -3.45 -2.56)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 83bb0a51-86c9-46ae-8cdd-48a2881ef9a6))
  (fp_line (start 0 -2.56) (end 1.95 -2.56)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 200f6ca8-374d-4474-a605-af5057fcdfb2))
  (fp_line (start 0 2.56) (end -1.95 2.56)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 124bdc8a-a3b8-41c7-b534-3e0069a4c647))
  (fp_line (start 0 2.56) (end 1.95 2.56)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5a9a1486-7eff-44a0-89e2-0d36ce5cacb6))
  (fp_line (start -3.6 2.05) (end -3.6 -2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp fd3640c6-29ca-4032-bbec-b907d97c9c0d))
  (fp_line (start -3.3 -2.35) (end -2.2 -2.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b9b76489-e96d-4c0a-bf59-1f100f4561e4))
  (fp_line (start -3.3 2.35) (end -2.2 2.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ab0dd6c2-cec1-4738-a61c-f76799cf66a2))
  (fp_line (start -2.2 -2.35) (end -2.2 -2.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp cd7965ed-70fd-4822-b6c6-4f396e845e00))
  (fp_line (start -2.2 2.35) (end -2.2 2.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 94b5d4cb-51b6-45b5-8f04-79174dd86591))
  (fp_line (start -1.95 -2.7) (end 1.95 -2.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 93f3bf60-8d48-465e-9e24-695ff3a04a27))
  (fp_line (start 1.95 2.7) (end -1.95 2.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1effeb75-f2aa-4b8f-978b-b1c60612d01d))
  (fp_line (start 2.2 -2.35) (end 2.2 -2.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ec51a582-a100-464b-9ee7-9554c15cdbd1))
  (fp_line (start 2.2 2.35) (end 2.2 2.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp bbc488df-2952-49dd-89c7-2e48442af0b0))
  (fp_line (start 3.3 -2.35) (end 2.2 -2.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 52efd9aa-fe70-4bc6-88b0-00e3cd72e676))
  (fp_line (start 3.3 2.35) (end 2.2 2.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 57e4e891-f354-4a43-be9f-19331719d052))
  (fp_line (start 3.6 -2.05) (end 3.6 2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp dc282cf4-0dd5-4ecc-915c-3595b7fca163))
  (fp_arc (start -3.6 -2.05) (mid -3.512132 -2.262132) (end -3.3 -2.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6ac65b04-6d8a-4e90-9a0f-122667e03ac6))
  (fp_arc (start -3.3 2.35) (mid -3.512132 2.262132) (end -3.6 2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e40f3f9d-f164-411e-91fe-540f090488c5))
  (fp_arc (start -2.2 -2.45) (mid -2.126777 -2.626777) (end -1.95 -2.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 06daed0f-75ad-42c1-a4ee-e2bde4ad54d3))
  (fp_arc (start -1.95 2.7) (mid -2.126777 2.626777) (end -2.2 2.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 7544c1bf-6dd9-4611-97b9-78f868cb704f))
  (fp_arc (start 1.95 -2.7) (mid 2.126777 -2.626777) (end 2.2 -2.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e7862ee5-11d5-47aa-9104-0b719c8403a1))
  (fp_arc (start 2.2 2.45) (mid 2.126777 2.626777) (end 1.95 2.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e677db83-81c2-4e60-96b3-486a00c4fd56))
  (fp_arc (start 3.3 -2.35) (mid 3.512132 -2.262132) (end 3.6 -2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4a1fb430-643b-42d4-955d-9124e44bfc4c))
  (fp_arc (start 3.6 2.05) (mid 3.512132 2.262132) (end 3.3 2.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 487a6f01-555a-4f52-8aef-8a3f3e303570))
  (fp_line (start -1.95 -2.45) (end 1.95 -2.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 76176654-1d9b-4394-adeb-0f0f76813883))
  (fp_line (start -1.95 -1.475) (end -0.975 -2.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b7e5433c-debc-486d-a9c6-31e4e93e560c))
  (fp_line (start -1.95 2.45) (end -1.95 -2.475)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8040da0b-a8de-4256-9aa7-02aed4c133b1))
  (fp_line (start 1.95 -2.45) (end 1.95 2.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3cda820d-22d7-4948-a8d4-95360c7a9327))
  (fp_line (start 1.95 2.45) (end -1.95 2.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ccaed27c-26aa-42cb-b304-3b1984be314a))
  (pad "" smd roundrect (at -0.6 -0.775) (size 0.97 1.25) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp 435c0665-c989-4e30-b8d0-d32f770f1e87))
  (pad "" smd roundrect (at -0.6 0.775) (size 0.97 1.25) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp 6c70c606-e463-4959-bd69-8e03674e5485))
  (pad "" smd roundrect (at 0.6 -0.775) (size 0.97 1.25) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp 2e9f4b70-3e4d-4c37-9185-b40fac3d37af))
  (pad "" smd roundrect (at 0.6 0.775) (size 0.97 1.25) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp 91f5d015-6459-4cae-8d8b-a2f3461603ca))
  (pad "1" smd roundrect (at -2.65 -1.905) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4a17bd27-5ea5-491e-bdd9-26fb427b5be7))
  (pad "2" smd roundrect (at -2.65 -0.635) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9aa76c49-8846-4408-bf11-fd22d34fcc4a))
  (pad "3" smd roundrect (at -2.65 0.635) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9a1d812b-38e4-475c-8f2c-eb744a3e844d))
  (pad "4" smd roundrect (at -2.65 1.905) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 3605638c-2856-49ac-b018-3169892be6b8))
  (pad "5" smd roundrect (at 2.65 1.905) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 26023e95-01d3-499f-ab06-7b395e35ac9d))
  (pad "6" smd roundrect (at 2.65 0.635) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c3ca1eee-7dd2-4eff-af7d-380ea0c9b835))
  (pad "7" smd roundrect (at 2.65 -0.635) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8cd57a19-357c-40bc-b0ae-b06ad8549a65))
  (pad "8" smd roundrect (at 2.65 -1.905) (size 1.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 07522085-4983-4a02-bafc-8fd467a6c1f5))
  (pad "9" smd rect (at 0 0) (size 2.41 3.1) (layers "F.Cu" "F.Mask") (tstamp d62cc9ad-3309-4497-a0d4-dfa6ed955467))
  (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/HSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.1mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
