(module "DIP-8_1.27mm_J-hook_(CHS-08TA)" (layer F.Cu) (tedit 5B499AA3)
  (solder_mask_margin 0.025)
  (solder_paste_margin -0.025)
  (attr smd)
  (fp_text reference REF** (at -6.4 0 90) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value "DIP-8_1.27mm_J-hook_(CHS-08TA)" (at 0 1) (layer F.Fab)
    (effects (font (size 0.4 0.4) (thickness 0.1)))
  )
  (fp_circle (center -5.75 3) (end -5.85 3) (layer F.SilkS) (width 0.125))
  (fp_line (start 5 -2.7) (end 5.85 -2.7) (layer F.SilkS) (width 0.125))
  (fp_line (start 5.85 -2.7) (end 5.85 2.7) (layer F.SilkS) (width 0.125))
  (fp_line (start 5.85 2.7) (end 5 2.7) (layer F.SilkS) (width 0.125))
  (fp_line (start -5 -2.7) (end -5.85 -2.7) (layer F.SilkS) (width 0.125))
  (fp_line (start -5.85 -2.7) (end -5.85 2.7) (layer F.SilkS) (width 0.125))
  (fp_line (start -5.85 2.7) (end -5 2.7) (layer F.SilkS) (width 0.125))
  (fp_line (start 6.35 3.85) (end -6.35 3.85) (layer F.CrtYd) (width 0.05))
  (fp_line (start -6.35 3.85) (end -6.35 -3.85) (layer F.CrtYd) (width 0.05))
  (fp_line (start -6.35 -3.85) (end 6.35 -3.85) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.35 -3.85) (end 6.35 3.85) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5.85 -2.7) (end 5.85 2.7) (layer F.Fab) (width 0.05))
  (fp_line (start 5.85 2.7) (end -5.85 2.7) (layer F.Fab) (width 0.05))
  (fp_line (start -5.85 2.7) (end -5.85 -2.7) (layer F.Fab) (width 0.05))
  (fp_line (start -5.85 -2.7) (end 5.85 -2.7) (layer F.Fab) (width 0.05))
  (pad 1 smd roundrect (at -4.445 2.4) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 2 smd roundrect (at -3.175 2.4) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 3 smd roundrect (at -1.905 2.4) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 4 smd roundrect (at -0.635 2.4) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 5 smd roundrect (at 0.635 2.4) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 6 smd roundrect (at 1.905 2.4) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 7 smd roundrect (at 3.175 2.4) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 8 smd roundrect (at 4.445 2.4) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 9 smd roundrect (at 4.445 -2.4) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 10 smd roundrect (at 3.175 -2.4) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 11 smd roundrect (at 1.905 -2.4) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 12 smd roundrect (at 0.635 -2.4) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 13 smd roundrect (at -0.635 -2.4) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 14 smd roundrect (at -1.905 -2.4) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 15 smd roundrect (at -3.175 -2.4) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 16 smd roundrect (at -4.445 -2.4) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (model ${KICAD7_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/CHS-08TA.step
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
