(footprint "51338-1074 100P P0.4_Odd-Even_Mirror" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Sheetfile" "SoM Headers.kicad_sch")
  (property "Sheetname" "SoM Headers")
  (attr smd)
  (fp_text reference "J21" (at 0 -2.45 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 9d3f00bc-a67d-460f-9c73-58bdf2ffb8e4)
  )
  (fp_text value "Forlinx_FET3588-C_Bottom-Left" (at -11.4 -0.2 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)) (justify left))
    (tstamp 884be8f8-dc20-4868-9476-1e591d9750e8)
  )
  (fp_text user "Own signals only" (at 0 0.55 unlocked) (layer "Dwgs.User")
      (effects (font (size 0.2 0.2) (thickness 0.05)))
    (tstamp 0f0089e3-f656-4a9d-85dd-17740b897ac5)
  )
  (fp_text user "${REFERENCE}" (at -11.4 0.3 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)) (justify left))
    (tstamp f23c1b31-531a-44ae-be0b-19fc92931293)
  )
  (fp_arc (start -11.775 -1.85) (mid -11.753033 -1.903033) (end -11.7 -1.925)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp eda1e2ba-7be1-4595-a733-9fb25f9b734b))
  (fp_arc (start -11.7 1.925) (mid -11.753033 1.903033) (end -11.775 1.85)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 95fe0b28-fced-4ba3-944c-7bbb304a8492))
  (fp_arc (start 11.7 -1.925) (mid 11.753033 -1.903033) (end 11.775 -1.85)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 5078e992-df46-4b27-9f95-0eeea4d21027))
  (fp_arc (start 11.775 1.85) (mid 11.753033 1.903033) (end 11.7 1.925)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp bf010f14-ed86-4deb-b3a3-bcec098251e1))
  (fp_poly
    (pts
      (xy -9.8 -2.05)
      (xy -9.6 -2.35)
      (xy -10 -2.35)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 0f1552f5-4104-4843-b9e7-2d4ffd97ca4d))
  (fp_poly
    (pts
      (xy -10.25 -1.85)
      (xy -11.7 -1.85)
      (xy -11.7 1.85)
      (xy -10.25 1.85)
      (xy -10.25 2)
      (xy -11.7 2)
      (xy -11.85 1.85)
      (xy -11.85 -1.85)
      (xy -11.7 -2)
      (xy -10.25 -2)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp aff1c19e-4939-40f1-b6c6-efe4b9f1ab98))
  (fp_poly
    (pts
      (xy 10.25 1.85)
      (xy 11.7 1.85)
      (xy 11.7 -1.85)
      (xy 10.25 -1.85)
      (xy 10.25 -2)
      (xy 11.7 -2)
      (xy 11.85 -1.85)
      (xy 11.85 1.85)
      (xy 11.7 2)
      (xy 10.25 2)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp fde7efd4-1638-42e0-b0e8-a346884d7453))
  (fp_rect (start -9.95 -1.25) (end 9.95 -0.8)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp f19e449e-783e-402b-a4ea-6dd36695c53f))
  (fp_rect (start -9.95 0.75) (end 9.95 1.2)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp c84e801a-2a75-4651-bd98-b089a7be2c34))
  (fp_line (start -11.7 -1.7) (end -11.7 1.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 303f9099-3f9a-4688-9bcf-8b2a7460eace))
  (fp_line (start -11.35 2.05) (end 11.35 2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 39b6056f-30ae-48f5-b54c-4613c620b455))
  (fp_line (start 11.35 -2.05) (end -11.35 -2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f07e4f64-c9f9-45ba-a36e-f7494138dab1))
  (fp_line (start 11.7 1.7) (end 11.7 -1.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b3a9a83e-6f14-4b17-8319-8192faf7cb9e))
  (fp_arc (start -11.7 -1.7) (mid -11.597487 -1.947487) (end -11.35 -2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp da0eef9c-6e1c-4e04-a961-8597932cdb0c))
  (fp_arc (start -11.35 2.05) (mid -11.597487 1.947487) (end -11.7 1.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp da025524-5ba8-4aa8-b5e5-3912ecf81317))
  (fp_arc (start 11.35 -2.05) (mid 11.597487 -1.947487) (end 11.7 -1.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e6c8594a-28f5-4ec0-9bf0-edf15d312043))
  (fp_arc (start 11.7 1.7) (mid 11.597487 1.947487) (end 11.35 2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2cea9fa6-4bf0-4416-86d4-d939d5b3e197))
  (fp_rect (start -11.55 -1.7) (end 11.55 1.7)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp b00dab52-3f24-4b09-b0f8-ac545a1cf355))
  (pad "" smd oval (at -9.8 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp fee44202-f94f-487e-a980-e1281cda4883))
  (pad "" smd oval (at -9.8 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 711b450a-c3bd-4772-82e0-9eb481109aeb))
  (pad "" smd oval (at -9.4 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp fd681a10-fe3b-4422-a89f-bdf0d042e500))
  (pad "" smd oval (at -9.4 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 2833442b-73a3-4ccf-983a-339cb1e5990c))
  (pad "" smd oval (at -9 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 397878a9-3c03-4e44-8fbb-d7af1dbb229a))
  (pad "" smd oval (at -9 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 25e44380-6ce7-4034-99d6-77909cd48fd3))
  (pad "" smd oval (at -8.6 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 5e2d2803-a53a-4c6c-99a8-940abbb81a2b))
  (pad "" smd oval (at -8.6 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 67616198-131c-4594-960c-93d913f56e11))
  (pad "" smd oval (at -8.2 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 7b048074-8937-450f-a338-6c68f5512d1c))
  (pad "" smd oval (at -8.2 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp e5a47a62-814b-4350-8288-62c63b05fc05))
  (pad "" smd oval (at -7.8 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 19cb4255-3b77-4229-bb20-3476753b4ceb))
  (pad "" smd oval (at -7.8 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 19104386-df64-48f2-a04f-ae46c5fd24df))
  (pad "" smd oval (at -7.4 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 8fbb7adb-578d-435c-940b-df964395ce48))
  (pad "" smd oval (at -7.4 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp a81d6e23-ebfc-41fc-a479-c5c2d659178a))
  (pad "" smd oval (at -7 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 9348cf7c-60a2-4fa0-a710-a5186776abd3))
  (pad "" smd oval (at -7 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 8278b7c0-3498-4d99-a726-a6ac7bc81fab))
  (pad "" smd oval (at -6.6 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 7614fd10-67f4-427e-83c5-87e93f86702a))
  (pad "" smd oval (at -6.6 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 18ff065f-21d1-4b46-a8d5-73438eb9535a))
  (pad "" smd oval (at -6.2 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 622981ed-6761-4629-9e72-64a1ddc776f8))
  (pad "" smd oval (at -6.2 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp a67d6edb-e02f-437d-ad9f-fa7c67d19742))
  (pad "" smd oval (at -5.8 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp f1f0c906-17bd-4773-b18f-3e9440438ab1))
  (pad "" smd oval (at -5.8 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp cda6c7d4-1722-4816-8d6b-7afc486a446f))
  (pad "" smd oval (at -5.4 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 1fcb182a-de52-4e1f-94af-ace9e69b9f02))
  (pad "" smd oval (at -5.4 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 212a595b-e761-4fc5-aa18-3931c264bd23))
  (pad "" smd oval (at -5 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 3bbd331a-22ae-41f7-879b-a3f9859ba2df))
  (pad "" smd oval (at -5 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 17f28888-3610-4293-b2e5-e25c7483a5c6))
  (pad "" smd oval (at -4.6 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp d00004bb-3407-4a8c-a51c-c35798dc6b9d))
  (pad "" smd oval (at -4.6 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 83a77b39-4240-4c55-9789-376169581de6))
  (pad "" smd oval (at -4.2 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp fd288cec-0eb0-4a16-8d1c-f9b37d11610d))
  (pad "" smd oval (at -4.2 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 2be97c33-eac7-4339-9679-401c5fc43136))
  (pad "" smd oval (at -3.8 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp b5f4accc-ee0d-4795-a373-366d04c56e84))
  (pad "" smd oval (at -3.8 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp b2016744-a548-4168-9561-e68d396745e4))
  (pad "" smd oval (at -3.4 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp cb03227c-e426-4545-b1b1-f8970d1bf90d))
  (pad "" smd oval (at -3.4 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 3f54a038-7502-4c74-ab52-f72f8592e097))
  (pad "" smd oval (at -3 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 6f7e6162-368c-4c84-a911-eab97510fcdc))
  (pad "" smd oval (at -3 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp ff56a61c-e3f4-4816-8aff-228d54263286))
  (pad "" smd oval (at -2.6 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 6d579a4f-5f44-47bf-8904-d5d57fa20f7d))
  (pad "" smd oval (at -2.6 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp e31a4d01-d3ef-4045-9a87-5223d443e853))
  (pad "" smd oval (at -2.2 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp fb7cc630-1003-4b26-a42a-5b46d6a65ecd))
  (pad "" smd oval (at -2.2 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 2a925e1a-99ba-4b8d-9b7b-cc02acb923db))
  (pad "" smd oval (at -1.8 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp fe5f2d23-aee3-4ae3-8502-f461726a4193))
  (pad "" smd oval (at -1.8 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 17f3b7a0-5b63-4150-8455-4665c00b1c53))
  (pad "" smd oval (at -1.4 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 0ede95ae-e278-413f-9990-5d51d49c805b))
  (pad "" smd oval (at -1.4 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp ba30115d-f5ef-4baf-9686-c48151a1544c))
  (pad "" smd oval (at -1 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp c0bbcb0f-112e-4c55-8b6a-aca768d8b4d9))
  (pad "" smd oval (at -1 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 4eade796-9f68-4ae7-9d99-8841ece3320a))
  (pad "" smd oval (at -0.6 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 827e01ab-a99a-453c-8f06-2b252de09647))
  (pad "" smd oval (at -0.6 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp cc430e96-517f-474a-93c8-5799766f856f))
  (pad "" smd oval (at -0.2 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 56eee58d-b5da-421b-b0d5-b2e57ab73717))
  (pad "" smd oval (at -0.2 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 7e01f36a-8270-4736-a37f-f6e66b9cc804))
  (pad "" smd oval (at 0.2 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 4a4c55e6-7480-41aa-8c80-bbcfa8838fbf))
  (pad "" smd oval (at 0.2 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 01f0c6ad-5b63-4f42-a949-2e4292471ded))
  (pad "" smd oval (at 0.6 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 246f9200-8380-4bc6-99d4-b15b88897e7d))
  (pad "" smd oval (at 0.6 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 0f64ceac-abf3-437a-be3f-717d418e0ee4))
  (pad "" smd oval (at 1 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 6b1eb570-6b09-4c28-8fd3-dd47cb41686a))
  (pad "" smd oval (at 1 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 48e72c34-4921-4bb5-81df-83c1e8e1e107))
  (pad "" smd oval (at 1.4 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 0fd2a0f8-23cd-4bd7-b240-84b4c916194f))
  (pad "" smd oval (at 1.4 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 24069efb-b504-43ac-9630-5ee1e8570dc1))
  (pad "" smd oval (at 1.8 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 11fe8c67-5f18-4550-acc7-4a95e5220969))
  (pad "" smd oval (at 1.8 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 4f248ec2-95a0-423e-95b9-39a3356bed5f))
  (pad "" smd oval (at 2.2 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp b0733140-1ba9-49e6-b5a9-a43ae9f973c8))
  (pad "" smd oval (at 2.2 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp e51f2616-0b1a-41c1-ae78-a05a3682cd68))
  (pad "" smd oval (at 2.6 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 5dd1900b-a7fa-449d-9452-906984e81cee))
  (pad "" smd oval (at 2.6 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp a8834501-b43d-4c6d-af36-dff818c6e2d5))
  (pad "" smd oval (at 3 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp c25e7a29-1322-4480-8d4d-44d2de1fcb4d))
  (pad "" smd oval (at 3 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 1b9ceb55-d411-48c9-88e9-f8b693d5b600))
  (pad "" smd oval (at 3.4 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 0d593066-e8b1-4802-8824-8985e484cdb8))
  (pad "" smd oval (at 3.4 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 2248373f-0ece-4e65-9602-768024848388))
  (pad "" smd oval (at 3.8 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp a608f9a0-1e22-4f38-9509-af3e941cd464))
  (pad "" smd oval (at 3.8 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp c12a3ed9-f40f-4cf4-a155-ac746fdaf23c))
  (pad "" smd oval (at 4.2 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 63d4e4b4-1d3e-46b2-9096-8b28f4ce1f83))
  (pad "" smd oval (at 4.2 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 93abe592-b6b0-4bc5-93d1-5cef8b6212a5))
  (pad "" smd oval (at 4.6 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 00632bf1-8115-464e-9128-874d9c77324b))
  (pad "" smd oval (at 4.6 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 34b49ecf-ea05-41fc-b538-501a741f6c4b))
  (pad "" smd oval (at 5 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 40112a55-1359-486a-9be7-6a944e2a4bb0))
  (pad "" smd oval (at 5 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp e9e8b9e9-a903-40ed-865f-5fd4b6b79e98))
  (pad "" smd oval (at 5.4 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 4f54e645-8387-4fd6-b190-a81d601eb31d))
  (pad "" smd oval (at 5.4 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 99cfaf12-42dc-4349-9900-8333f22541a2))
  (pad "" smd oval (at 5.8 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 88bdddca-1c41-4286-9703-f1ea6e58f13f))
  (pad "" smd oval (at 5.8 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 50ab7e50-de46-44df-814c-ac8760b4a054))
  (pad "" smd oval (at 6.2 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp f91aa569-99f0-4f28-ab34-d45505186910))
  (pad "" smd oval (at 6.2 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 8595e397-e78c-43cf-a0a8-f1f7a40c8466))
  (pad "" smd oval (at 6.6 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp daf04597-af5f-4d91-bf30-897b6a7515bb))
  (pad "" smd oval (at 6.6 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp d3fa5c4a-f1c5-4cf4-9663-579c38358c36))
  (pad "" smd oval (at 7 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 3cd3dd9d-e0de-4311-ab28-33d6fdbfd8c8))
  (pad "" smd oval (at 7 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 60175bb7-7b23-452b-81c8-12b0ffddce8f))
  (pad "" smd oval (at 7.4 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 1e6fea1d-4820-4a86-bd5a-ce5330c05ea0))
  (pad "" smd oval (at 7.4 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp d78a1044-05bc-4887-b09c-a66c7b5941c1))
  (pad "" smd oval (at 7.8 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 5cd4d8a1-d09e-4e02-b86a-ddb9cf0aed82))
  (pad "" smd oval (at 7.8 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 4b6415e6-8b72-4b4a-9957-76a9ab7a7b81))
  (pad "" smd oval (at 8.2 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp b935a706-ea2f-4906-9014-285ccb740e6a))
  (pad "" smd oval (at 8.2 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 27a198e9-ed4c-4b96-a48a-668016d47410))
  (pad "" smd oval (at 8.6 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp f678bf91-2a00-4d7c-b3c5-9fbda6724f04))
  (pad "" smd oval (at 8.6 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp f11d7716-6977-4322-a243-37edd6dda171))
  (pad "" smd oval (at 9 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 86548cb6-5b74-4b07-bc03-3ee305938533))
  (pad "" smd oval (at 9 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp b47c1505-830b-49bb-a931-82adab1f2b54))
  (pad "" smd oval (at 9.4 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp fdf100ab-5453-4d62-9767-2a881f4e5512))
  (pad "" smd oval (at 9.4 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 62c1abde-3c54-4103-8cec-4d8c8b23f9e5))
  (pad "" smd oval (at 9.8 -1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp c9205677-a95d-4fac-a253-b46fd01ceafa))
  (pad "" smd oval (at 9.8 1.55) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 46bf2602-2fd1-48a5-8433-85ec025c2aae))
  (pad "1" smd roundrect (at -9.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 2f33ee57-bcd7-4f43-ab2f-a3ebcdf5770f))
  (pad "2" smd roundrect (at -9.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 1c5cad77-ad3c-4efe-9c85-3f45151a3ed8))
  (pad "3" smd roundrect (at -9.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 1d1995df-4453-4a17-97c1-a48e0fd9f54f))
  (pad "4" smd roundrect (at -9.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 2f13d6fb-4553-4f90-b68f-c29e912e7e3c))
  (pad "5" smd roundrect (at -9 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 281eb05a-9434-4722-8d2b-e67556dddbb6))
  (pad "6" smd roundrect (at -9 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 6f1a6b8b-f115-4349-ad0e-b0b64e128a61))
  (pad "7" smd roundrect (at -8.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 0e463ad7-710b-4db3-865c-de5e5ede30ee))
  (pad "8" smd roundrect (at -8.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 0a05cc74-e875-47e9-bcdb-0557befb18fe))
  (pad "9" smd roundrect (at -8.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 583beba4-9349-4fb4-a29b-2f8e2eb9b207))
  (pad "10" smd roundrect (at -8.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 3c47b0c8-16c3-4d56-9f17-9f7f8493963d))
  (pad "11" smd roundrect (at -7.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 5057e9ad-7c89-416d-a81c-134dab75d215))
  (pad "12" smd roundrect (at -7.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp e8267229-c622-4454-bbce-edf6f1e3fb99))
  (pad "13" smd roundrect (at -7.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp f08e86ca-b156-4d42-9047-66ba87f1850c))
  (pad "14" smd roundrect (at -7.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 6fb35fc0-c13b-4e62-81db-6a3d1f959edd))
  (pad "15" smd roundrect (at -7 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 760212f1-aaf9-47bd-8c6f-416fb17152d2))
  (pad "16" smd roundrect (at -7 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 90ae0d1d-c5c2-40a7-9984-61c3d7fb9b1c))
  (pad "17" smd roundrect (at -6.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp be14a7b2-8bf2-4245-bdaf-4ee0ecae9273))
  (pad "18" smd roundrect (at -6.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 292fb1de-9e86-4151-a99f-6bf83b8ab5ef))
  (pad "19" smd roundrect (at -6.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 1291ada9-6fd1-41dd-bed3-931f58f259a5))
  (pad "20" smd roundrect (at -6.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 3521dddc-f0ab-43d9-ab8e-56f7bc85ae56))
  (pad "21" smd roundrect (at -5.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp db77de9c-72fe-4b54-a6b1-bf5c5cd77ffc))
  (pad "22" smd roundrect (at -5.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 6b45115b-a735-47f8-aa1e-fb03334a8e89))
  (pad "23" smd roundrect (at -5.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp cbc3baf4-22f3-4e32-9d5a-b9864dbc7913))
  (pad "24" smd roundrect (at -5.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp cbfa6dd9-4c1d-49cb-8d73-be5d06c07ef3))
  (pad "25" smd roundrect (at -5 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp a43aeca7-0c9a-4000-a40c-dd44b50c35a3))
  (pad "26" smd roundrect (at -5 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 435d8dd9-a1a3-4be8-a90e-bafd8f6bf9df))
  (pad "27" smd roundrect (at -4.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 337c1f33-1d4a-4bf4-8643-70043a799791))
  (pad "28" smd roundrect (at -4.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp c6865dee-6b0b-4559-bd57-351d800504ec))
  (pad "29" smd roundrect (at -4.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp d6fd0ce5-3618-45c9-aab1-5237a884dc09))
  (pad "30" smd roundrect (at -4.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 58f314f9-c7fb-42ae-91e8-63c2a5a3862b))
  (pad "31" smd roundrect (at -3.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 6d84a20a-e754-45a2-add6-d19f5d99d70a))
  (pad "32" smd roundrect (at -3.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp f8e46b55-6239-4976-bd99-f538a0d032c4))
  (pad "33" smd roundrect (at -3.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 4976d94b-87c6-45a4-a2e4-7692f69cc651))
  (pad "34" smd roundrect (at -3.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 92705b10-997e-4ecd-9c4a-5e61ecebb123))
  (pad "35" smd roundrect (at -3 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 5cd586d9-aade-4780-8b19-b4957b92b6f3))
  (pad "36" smd roundrect (at -3 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 32704293-39d7-4345-836b-56e909f7b9d9))
  (pad "37" smd roundrect (at -2.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp a4fee287-082c-4d9b-8c8d-cb8e9060dfc2))
  (pad "38" smd roundrect (at -2.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp b84969ac-02f2-4991-95ca-d0da4109a670))
  (pad "39" smd roundrect (at -2.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp c86d194b-0362-43c7-ba82-744f4b47b4c8))
  (pad "40" smd roundrect (at -2.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 97f637b6-64b0-4a66-98aa-f5e2cb2faf02))
  (pad "41" smd roundrect (at -1.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 12160e97-c3ab-45ea-b85c-71454567299e))
  (pad "42" smd roundrect (at -1.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp c3fd3e79-a58f-4425-b4b4-1d381735567c))
  (pad "43" smd roundrect (at -1.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 5a4e011e-666c-44a3-8289-d2da112d679b))
  (pad "44" smd roundrect (at -1.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 43b2d9cd-9d74-4cbf-8e46-44039ecec0ff))
  (pad "45" smd roundrect (at -1 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp a0028778-0d97-4d7c-84c0-246331a00a8a))
  (pad "46" smd roundrect (at -1 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 4e46e3cd-f545-4c74-8975-6a3fcb34415e))
  (pad "47" smd roundrect (at -0.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 0075947f-eef9-4a00-819a-42390372e085))
  (pad "48" smd roundrect (at -0.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 5cb468ac-4a19-4554-a35c-0006d0b61238))
  (pad "49" smd roundrect (at -0.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 502c753c-e0db-4152-9d32-f7414bf4ec39))
  (pad "50" smd roundrect (at -0.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 2f5f08d2-4230-4532-9a59-1a91777f46bf))
  (pad "51" smd roundrect (at 0.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 6bb3eec9-752b-4f26-9400-14112fbd906b))
  (pad "52" smd roundrect (at 0.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp ca8457e4-5b3b-4ad8-a38c-4d4719292bab))
  (pad "53" smd roundrect (at 0.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 98e3224f-2d8c-49dd-81e2-1955da85a384))
  (pad "54" smd roundrect (at 0.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 26066bb5-7dc7-4782-be5d-68cd3f1b41ff))
  (pad "55" smd roundrect (at 1 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 190bd5c4-6edd-4907-b20e-f099f25eff0c))
  (pad "56" smd roundrect (at 1 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 527ea168-156f-4b02-a3c6-7f9e6655039b))
  (pad "57" smd roundrect (at 1.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 66916875-f489-492d-b2fd-2b31acbd784d))
  (pad "58" smd roundrect (at 1.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 013b4c0c-08cc-49ea-b7e2-b73aafe3ee26))
  (pad "59" smd roundrect (at 1.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 0bea3e4d-9dee-41b3-9cd2-277997f0f1b0))
  (pad "60" smd roundrect (at 1.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp b0aee988-4619-4428-b754-279b9bf8cf8f))
  (pad "61" smd roundrect (at 2.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp c470d0ba-5085-4e1b-8593-11aaa69856cd))
  (pad "62" smd roundrect (at 2.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 9e88f68e-5307-4003-84ea-d748fd2c5444))
  (pad "63" smd roundrect (at 2.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 290b6975-10c6-4bd8-9ac1-cf57a8fb1c33))
  (pad "64" smd roundrect (at 2.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 55ff4ee7-ef62-4a55-8de4-e7a57bf2be46))
  (pad "65" smd roundrect (at 3 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 7b36c4d8-4fdc-4562-b09c-337875f7ad46))
  (pad "66" smd roundrect (at 3 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 9e6fd8e5-62be-4301-ab86-743e1423e25d))
  (pad "67" smd roundrect (at 3.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp d2ac5876-4e59-47ab-95d1-67bb1ec9e3e9))
  (pad "68" smd roundrect (at 3.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 19d2a6bf-a96f-4a68-bbad-713192d0740a))
  (pad "69" smd roundrect (at 3.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 8bf90fec-e4aa-409e-acf8-44dfad9e47d7))
  (pad "70" smd roundrect (at 3.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 29313684-5193-411b-ac22-b9b60f69a73f))
  (pad "71" smd roundrect (at 4.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 6a60b258-1e03-48f6-b168-8da20af12522))
  (pad "72" smd roundrect (at 4.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 8cbbaf6d-a205-4ab4-9cbb-fa3ba3a39247))
  (pad "73" smd roundrect (at 4.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 88628645-62bf-4981-af46-10b4bdd98630))
  (pad "74" smd roundrect (at 4.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 75525fb6-0cac-418c-9c32-ac9bbf4a27b5))
  (pad "75" smd roundrect (at 5 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 28fcda10-344f-4e56-9728-04d136d57878))
  (pad "76" smd roundrect (at 5 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 2e38a83e-38ea-436d-a0c3-dd6dedd979f9))
  (pad "77" smd roundrect (at 5.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 3f76e7db-3fa9-4836-9d25-f9851f57b094))
  (pad "78" smd roundrect (at 5.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 0e634e35-7920-444b-85bc-1d5f42927c25))
  (pad "79" smd roundrect (at 5.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp ff87bfdb-568d-4e1b-875b-8edf8617a388))
  (pad "80" smd roundrect (at 5.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 486f06c2-d208-4105-a579-bca3182e8b11))
  (pad "81" smd roundrect (at 6.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp b8c3fe01-259f-4b75-99d3-ee658953b371))
  (pad "82" smd roundrect (at 6.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp c73d145d-9981-4fc6-b0a1-074e2f03303c))
  (pad "83" smd roundrect (at 6.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 39a457b1-2b7f-42c3-808f-126b00aa727b))
  (pad "84" smd roundrect (at 6.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp e65cf099-98ef-47e4-9062-8f5d6ad44923))
  (pad "85" smd roundrect (at 7 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp a6498b81-2c30-40eb-b34a-3b85760e9f61))
  (pad "86" smd roundrect (at 7 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp cbaa3fe4-a3fc-4a5e-8aea-f8b9619058ab))
  (pad "87" smd roundrect (at 7.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp b5c300ba-17ae-40a4-9ab1-92444502ec3c))
  (pad "88" smd roundrect (at 7.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp b9c55630-e9c1-44a2-9d66-2384e7ffa290))
  (pad "89" smd roundrect (at 7.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 04141113-7356-4310-9afb-4681f51bce51))
  (pad "90" smd roundrect (at 7.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp ea660c15-a33f-4f41-9e88-8dabbd637e3b))
  (pad "91" smd roundrect (at 8.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 55d30a35-e774-40a6-9901-02c8f507c53c))
  (pad "92" smd roundrect (at 8.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 02d1a912-43c4-418f-8cc5-a4d50f2c259e))
  (pad "93" smd roundrect (at 8.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 7213b881-b204-43d0-9ea1-8e7645a07d62))
  (pad "94" smd roundrect (at 8.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 62d639d2-30bd-4714-bf5b-5e4c96efd7b2))
  (pad "95" smd roundrect (at 9 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 3240a9fb-cc0c-4aaa-9491-d7b3fb3f867c))
  (pad "96" smd roundrect (at 9 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 01775c40-4df5-44e3-b0a7-c75cdd0380cd))
  (pad "97" smd roundrect (at 9.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 9f664841-8685-42a5-938b-9db2cafb6701))
  (pad "98" smd roundrect (at 9.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp bec347b6-556e-4740-84a1-4cbfb1c6c9c5))
  (pad "99" smd roundrect (at 9.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 31663969-8871-4467-b1ce-df7cbfbca4d4))
  (pad "100" smd roundrect (at 9.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 2c1ba925-e962-4188-9618-1bcb5e5addd5))
  (pad "MP" smd roundrect (at -10.75 -1.5) (size 1 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp bd88c42c-0e75-4a55-b8b2-9be032534e59))
  (pad "MP" smd roundrect (at -10.75 1.5) (size 1 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp 92ba717e-17c1-47fa-85a8-ac0d415cd490))
  (pad "MP" smd roundrect (at 10.75 -1.5) (size 1 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp 7f8d4ded-d7cb-46b5-b16a-51378dcf3c44))
  (pad "MP" smd roundrect (at 10.75 1.5) (size 1 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp 6f9de69f-93eb-4389-9c30-1cd95b631d12))
  (model "${KICAD7_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex 51338-1074.stp"
    (offset (xyz 0 0 0.64))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
