(footprint "51338-1074 100P P0.4" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -2.45 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 598e4510-d210-4eea-be4e-c5076d1f5952)
  )
  (fp_text value "51338-1074 100P P0.4" (at -11.4 -0.2 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)) (justify left))
    (tstamp 5505bb43-5d37-458c-905e-366e56548e59)
  )
  (fp_text user "Own signals only" (at 0 0.55 unlocked) (layer "Dwgs.User")
      (effects (font (size 0.2 0.2) (thickness 0.05)))
    (tstamp 532401cc-c582-4c04-a0c5-1b0719346492)
  )
  (fp_text user "${REFERENCE}" (at -11.4 0.3 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)) (justify left))
    (tstamp f66b9741-06a7-41f1-850f-6a7a32ea1c19)
  )
  (fp_arc (start -11.775 -1.85) (mid -11.753033 -1.903033) (end -11.7 -1.925)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 81e5e44c-0df7-44e3-8106-422ca1bc98f9))
  (fp_arc (start -11.7 1.925) (mid -11.753033 1.903033) (end -11.775 1.85)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 84d6b8f3-0a67-47a3-b6fb-610bc7507391))
  (fp_arc (start 11.7 -1.925) (mid 11.753033 -1.903033) (end 11.775 -1.85)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 118aebe5-1d8f-4409-982b-529459ef8534))
  (fp_arc (start 11.775 1.85) (mid 11.753033 1.903033) (end 11.7 1.925)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp edb724a3-9415-4289-bf58-338b90d07c8d))
  (fp_poly
    (pts
      (xy -9.8 2.05)
      (xy -9.95 2.35)
      (xy -9.65 2.35)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp e4c59198-8d9e-4803-82b5-7e2ad81f23c8))
  (fp_poly
    (pts
      (xy -10.25 -1.85)
      (xy -11.7 -1.85)
      (xy -11.7 1.85)
      (xy -10.25 1.85)
      (xy -10.25 2)
      (xy -11.7 2)
      (xy -11.85 1.85)
      (xy -11.85 -1.85)
      (xy -11.7 -2)
      (xy -10.25 -2)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 69a4c7ad-0722-4ba8-89b6-0512724d171c))
  (fp_poly
    (pts
      (xy 10.25 1.85)
      (xy 11.7 1.85)
      (xy 11.7 -1.85)
      (xy 10.25 -1.85)
      (xy 10.25 -2)
      (xy 11.7 -2)
      (xy 11.85 -1.85)
      (xy 11.85 1.85)
      (xy 11.7 2)
      (xy 10.25 2)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 912ecbd4-ace5-4bde-b8eb-90f18ee5d9c6))
  (fp_rect (start -9.95 -1.25) (end 9.95 -0.8)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 58fb423d-cb90-4f87-ae9d-9bc2ad53b0a6))
  (fp_rect (start -9.95 0.75) (end 9.95 1.2)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 20937b88-081e-4c03-83b7-9d7b5d6338a5))
  (fp_line (start -11.7 -1.7) (end -11.7 1.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1bd71c3c-f553-410d-a73e-a4f70e58716e))
  (fp_line (start -11.35 2.05) (end 11.35 2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 62c2f4e6-1271-474e-b372-dfc7dd7ebf8f))
  (fp_line (start 11.35 -2.05) (end -11.35 -2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp bc906930-f108-4525-9878-819e2808e24a))
  (fp_line (start 11.7 1.7) (end 11.7 -1.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 68a4bea8-5bf6-4f9d-a425-446a07d44fef))
  (fp_arc (start -11.7 -1.7) (mid -11.597487 -1.947487) (end -11.35 -2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1ca789b3-a4b4-44e6-aa4f-3d4960a4e6a0))
  (fp_arc (start -11.35 2.05) (mid -11.597487 1.947487) (end -11.7 1.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp cc86db10-3f11-49c8-870a-9c1c29aa5895))
  (fp_arc (start 11.35 -2.05) (mid 11.597487 -1.947487) (end 11.7 -1.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4b403886-2b49-472d-9490-08d6e0bad4dd))
  (fp_arc (start 11.7 1.7) (mid 11.597487 1.947487) (end 11.35 2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp fe2c3498-d6d1-4668-9e9d-7af51d36ca8c))
  (fp_rect (start -11.55 -1.7) (end 11.55 1.7)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 5d82f5eb-0a47-4c18-9728-6dc9339c219d))
  (pad "1" smd roundrect (at -9.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 32285edc-46d1-41db-a949-538a9858ead1))
  (pad "2" smd roundrect (at -9.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 72492c2a-0ad5-48d7-bc57-5cc16645c56b))
  (pad "3" smd roundrect (at -9 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 026c8300-832a-46f3-bf9a-ed9b0d08e0bd))
  (pad "4" smd roundrect (at -8.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 11bf7b46-d7c3-442e-80c6-d00958eeda90))
  (pad "5" smd roundrect (at -8.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 0c73e30f-f1b5-480a-a263-2551a0cb1c61))
  (pad "6" smd roundrect (at -7.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 887933c1-857b-492e-b337-8c9767b1f1a5))
  (pad "7" smd roundrect (at -7.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 12e1213f-071f-42ff-b1dc-2dd53334ce52))
  (pad "8" smd roundrect (at -7 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 13495f1c-1781-4fff-9c0f-38c7637b5d2f))
  (pad "9" smd roundrect (at -6.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp bbe91466-e76e-471d-8634-bf63ae26d287))
  (pad "10" smd roundrect (at -6.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 7db24340-2efa-471e-9c4c-3663c0cb0bc3))
  (pad "11" smd roundrect (at -5.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 07e2eb71-5bc9-4b08-b97d-a82244f886da))
  (pad "12" smd roundrect (at -5.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 6bcb5169-1c0e-48a2-b2bd-59b80dff6419))
  (pad "13" smd roundrect (at -5 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 1cdd1c8d-a259-482a-b363-5ecc6cc3fc72))
  (pad "14" smd roundrect (at -4.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 78d9cdb7-2bf2-4477-9c49-62bf84b9edda))
  (pad "15" smd roundrect (at -4.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 1b7059ed-c3a0-4166-b303-fe961d7734b2))
  (pad "16" smd roundrect (at -3.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 626d025a-4e28-4adf-aeb8-fb4d9ee50f12))
  (pad "17" smd roundrect (at -3.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 3dfc4cad-ba3a-4ef2-ba38-99802b0e5981))
  (pad "18" smd roundrect (at -3 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 5d700a8f-ec6e-43e0-bc98-a623159e8121))
  (pad "19" smd roundrect (at -2.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp ceb2e04c-af3b-4243-9bce-9ab8410d1f8b))
  (pad "20" smd roundrect (at -2.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 98e9a969-9a23-42cc-867f-5f9e0b007491))
  (pad "21" smd roundrect (at -1.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp e537778e-33d1-4cad-b0d0-8736853d0dc5))
  (pad "22" smd roundrect (at -1.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 9f8f05bb-a1e4-42df-b123-dfdd1c20a5b3))
  (pad "23" smd roundrect (at -1 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp c3268a68-a417-4a8b-9ab4-a761e53e5542))
  (pad "24" smd roundrect (at -0.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp ef151a35-e8db-4c94-86d6-d9da21a16b85))
  (pad "25" smd roundrect (at -0.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 8e0e71e9-18fe-4f0a-a5dc-4e2170dce073))
  (pad "26" smd roundrect (at 0.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 30156fac-6826-4613-abe7-cadcacc343d8))
  (pad "27" smd roundrect (at 0.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 6972d916-8732-4049-8945-60299f0807bd))
  (pad "28" smd roundrect (at 1 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 5aedd05d-a7e2-4f65-b37c-95fc8a64ac36))
  (pad "29" smd roundrect (at 1.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 98d2e04e-634d-46a0-9345-405f3fd7ab6f))
  (pad "30" smd roundrect (at 1.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 4283787a-ae53-4465-aac0-34d7e88388c9))
  (pad "31" smd roundrect (at 2.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 58fba016-708d-4a66-bbb8-2463c3c0754a))
  (pad "32" smd roundrect (at 2.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp e55a7260-883a-483c-b211-115aa6af90d8))
  (pad "33" smd roundrect (at 3 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 6255b726-5a70-4ae5-94ec-e6dd1ee6bac0))
  (pad "34" smd roundrect (at 3.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp ce4bef50-c7b8-45b2-98f7-4aadb65b5703))
  (pad "35" smd roundrect (at 3.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 23dcae25-32d0-4c09-84f3-05bd739e2219))
  (pad "36" smd roundrect (at 4.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 1d5e9dc7-205b-44fd-80d5-03ec77bde084))
  (pad "37" smd roundrect (at 4.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp c1fce3e0-5d37-49f2-8665-30478ab05072))
  (pad "38" smd roundrect (at 5 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 4782a42e-e901-4b6f-a3ef-300d202a327e))
  (pad "39" smd roundrect (at 5.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp a8f3075d-d1c9-4917-85f5-ed873727710f))
  (pad "40" smd roundrect (at 5.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 4f8194ca-9242-40e5-b3c0-eaa27f5dd5b3))
  (pad "41" smd roundrect (at 6.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp e624edda-2f62-46bc-9e76-fe49749e92c7))
  (pad "42" smd roundrect (at 6.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 192ecad3-3ebf-45aa-bb4a-9ad60a4d80fd))
  (pad "43" smd roundrect (at 7 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 9327e5fc-37d4-4241-95a6-9d06646271a7))
  (pad "44" smd roundrect (at 7.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 6fdd67f6-ed5e-4b66-b02b-dd687d705535))
  (pad "45" smd roundrect (at 7.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 5b06e315-8719-4414-aa12-1e4178c4a148))
  (pad "46" smd roundrect (at 8.2 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 5f750227-39eb-47a4-ba8c-58f6d6718680))
  (pad "47" smd roundrect (at 8.6 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 00f9fb2f-5706-4032-a520-330c34d714a7))
  (pad "48" smd roundrect (at 9 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 83e98803-29c9-41cb-aa3b-838d7e510fc9))
  (pad "49" smd roundrect (at 9.4 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 0d966c2e-763c-4bc1-8e7b-2760af1d3cc3))
  (pad "50" smd roundrect (at 9.8 1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 8c6e4e39-e87b-440b-88a5-92b167a201dd))
  (pad "51" smd roundrect (at 9.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp cbec15a5-50c6-4dc7-adb5-fe8257f896d5))
  (pad "52" smd roundrect (at 9.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 7823d19a-c8ab-4598-8d67-87abd5740d9b))
  (pad "53" smd roundrect (at 9 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 310d0b33-b384-4cea-9918-e902a0ddd2e8))
  (pad "54" smd roundrect (at 8.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 7b034b49-00a4-4ddc-900a-0bfcb588389e))
  (pad "55" smd roundrect (at 8.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 25f8ad83-9cd8-4356-843a-9628500a7b5b))
  (pad "56" smd roundrect (at 7.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 74001145-52a3-4641-8090-5be7a509efb1))
  (pad "57" smd roundrect (at 7.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 9acfbbf0-516a-4f81-b6cc-620442eb09b4))
  (pad "58" smd roundrect (at 7 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 35d55bb4-161d-4082-9243-9da6f44bfcb1))
  (pad "59" smd roundrect (at 6.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 98fb8897-1743-48c8-b112-9b8ab11d83bf))
  (pad "60" smd roundrect (at 6.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp c2954530-e87b-4435-8075-f4799385bdc3))
  (pad "61" smd roundrect (at 5.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp f7f9c80c-9a33-4638-8ce8-78c49e42aea4))
  (pad "62" smd roundrect (at 5.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 8be0a3a3-fe92-4a4b-a5eb-41cccd581d0d))
  (pad "63" smd roundrect (at 5 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 8586cbd8-89d8-4643-9eb2-bc1550a51da2))
  (pad "64" smd roundrect (at 4.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 0eb71153-5bc7-4628-a6d3-75124c594a2a))
  (pad "65" smd roundrect (at 4.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 5a4af8bf-42d7-46d3-8a82-fe2102cf1050))
  (pad "66" smd roundrect (at 3.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp ad3d1ef9-5b92-46ce-aed8-b87ad469a4ca))
  (pad "67" smd roundrect (at 3.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp b7dbd0b0-4126-4e40-b586-6cbbecf7e6ea))
  (pad "68" smd roundrect (at 3 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp afd2fd0c-4566-4d7f-a18f-4a947233dd16))
  (pad "69" smd roundrect (at 2.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 829aa5ac-9292-4d30-9524-a78c8758a2a3))
  (pad "70" smd roundrect (at 2.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp b3aca725-0ea5-4190-a499-4438c47db898))
  (pad "71" smd roundrect (at 1.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 06222bff-0a44-492d-aaad-cc692c90daeb))
  (pad "72" smd roundrect (at 1.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 18799320-e192-4ff9-951d-f027028673b9))
  (pad "73" smd roundrect (at 1 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp efeaea70-b105-4a0b-b1b0-8921baae3cd4))
  (pad "74" smd roundrect (at 0.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp f24c57d3-fb1f-4555-ba68-fbf3aed939f3))
  (pad "75" smd roundrect (at 0.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp cf33b3ba-4a19-4694-a30f-7ae6d1f84da2))
  (pad "76" smd roundrect (at -0.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 361aaa62-b704-40f5-b8bd-4120590bcc97))
  (pad "77" smd roundrect (at -0.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 975bf8b2-2811-480e-833c-8bd5fbc49a5c))
  (pad "78" smd roundrect (at -1 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp ae12b341-2190-4314-8373-8d6c93f3376f))
  (pad "79" smd roundrect (at -1.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp d6482551-d91b-4857-ac3a-a5822ffd94d6))
  (pad "80" smd roundrect (at -1.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 6a940c27-f29e-4c30-a6b8-cb7bbb459730))
  (pad "81" smd roundrect (at -2.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 1d848324-e1ef-46c9-af53-41df85faee48))
  (pad "82" smd roundrect (at -2.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp da3be0d0-4159-47ca-b399-a4c36715b4e9))
  (pad "83" smd roundrect (at -3 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp e964136e-fb8b-4561-a581-77a705b916c0))
  (pad "84" smd roundrect (at -3.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 547bf706-6b3d-485c-a17d-8c9607f33e45))
  (pad "85" smd roundrect (at -3.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 2eb83c5a-8989-494e-8212-545c566b11d5))
  (pad "86" smd roundrect (at -4.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 4710dfd1-1c94-4eb2-ae8a-8ef7e418299e))
  (pad "87" smd roundrect (at -4.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 2cb07bd8-7d35-4967-8c3d-24592c0efef6))
  (pad "88" smd roundrect (at -5 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 7d43cd98-97bf-4475-9249-4a2808c41d5d))
  (pad "89" smd roundrect (at -5.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp f7355c91-9891-4f49-bec2-9e2992481a6d))
  (pad "90" smd roundrect (at -5.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp ba9a82d6-0b4e-4b93-8951-9362f3abf53c))
  (pad "91" smd roundrect (at -6.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp eded8277-d502-45ea-b0df-3e46796401fa))
  (pad "92" smd roundrect (at -6.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 4963c4a4-430a-4ace-92b6-c4e3a945fe8f))
  (pad "93" smd roundrect (at -7 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 2d4ba0fa-824f-45e1-b65d-59dc2655f12e))
  (pad "94" smd roundrect (at -7.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 497f0f77-fa5e-4c0d-aed7-ff144299f8f9))
  (pad "95" smd roundrect (at -7.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 78c5e6a3-d171-42f2-9121-e59f7af21dff))
  (pad "96" smd roundrect (at -8.2 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp d02041eb-c172-40c9-baf3-4642860f65f3))
  (pad "97" smd roundrect (at -8.6 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 9f1ed388-cbca-4a67-9afa-e6c66b6aea69))
  (pad "98" smd roundrect (at -9 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp 90527f54-7288-40cc-982f-e35d0f09f797))
  (pad "99" smd roundrect (at -9.4 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp cffa7534-b5d9-4edd-81df-8d5e07de9a11))
  (pad "100" smd roundrect (at -9.8 -1.55) (size 0.22 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
    (thermal_bridge_angle 45) (tstamp f4470e3b-56df-4e04-b386-ced02a51022a))
  (pad "MP" smd roundrect (at -10.75 -1.5) (size 1 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp 6bad2ce4-57c7-482a-bfc6-540ba0c54ea1))
  (pad "MP" smd roundrect (at -10.75 1.5) (size 1 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp 1bc3996f-839b-4c9c-9c37-d13161a4588f))
  (pad "MP" smd roundrect (at 10.75 -1.5) (size 1 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp f6edce7a-234b-4b4d-8aa6-f45d01033939))
  (pad "MP" smd roundrect (at 10.75 1.5) (size 1 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp f6689ba3-4553-49ff-a346-93eacbd9a27f))
  (model "${KICAD7_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex 51338-1074.stp"
    (offset (xyz 0 0 0.64))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
