(footprint "WSON-10-1EP_2x2mm_P0.4mm_EP0.9x1.5mm" (version 20220331) (generator pcbnew)
  (layer "F.Cu")
  (property "MFG" "TI")
  (property "MPN" "INA2181A2IDSQR")
  (property "Sheetfile" "ESC_Dual_10A.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Bidirectional, Low- and High-Side Voltage Output, Current-Sense Amplifier, SOT-23-6")
  (property "ki_keywords" "current monitor shunt sensor bidirectional")
  (attr smd)
  (fp_text reference "U6" (at 0 -1.9 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp d96b3a17-8150-4105-a6cc-12697c33a06b)
  )
  (fp_text value "INA2181" (at 0 2.2 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1712a8c6-e929-4783-a2b1-4722777ffddc)
  )
  (fp_text user "${REFERENCE}" (at 0 3.7 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 51c4778c-453f-4444-b8dc-baede6524ed2)
  )
  (fp_arc (start -1.225 -1.15) (mid -1.203033 -1.203033) (end -1.15 -1.225)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp f853a8fd-16b3-469c-8cb3-540258c9e3ce))
  (fp_arc (start -1.15 1.224999) (mid -1.203033 1.203032) (end -1.225 1.149999)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp bfb83ee6-d06d-41be-ab0f-1c6773281995))
  (fp_arc (start 1.15 -1.224999) (mid 1.203033 -1.203032) (end 1.225 -1.149999)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp d5a8d683-e796-42a9-a8a9-82572b68170a))
  (fp_arc (start 1.225 1.15) (mid 1.203033 1.203033) (end 1.15 1.225)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 1b04d75d-ffaa-46d2-b67c-4b24318247ef))
  (fp_poly
    (pts
      (xy -1.25 -0.8)
      (xy -1.375 -0.675)
      (xy -1.375 -0.925)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 0a997615-80ce-4792-84ca-85a2ed95a579))
  (fp_poly
    (pts
      (xy -1.3 1.15)
      (xy -1.3 1)
      (xy -1.15 1)
      (xy -1.15 1.15)
      (xy 1.15 1.15)
      (xy 1.15 1)
      (xy 1.3 1)
      (xy 1.3 1.15)
      (xy 1.15 1.3)
      (xy -1.15 1.3)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 9f38befe-a07c-41e4-95d9-ed093da620fb))
  (fp_poly
    (pts
      (xy 1.3 -1.15)
      (xy 1.3 -1)
      (xy 1.15 -1)
      (xy 1.15 -1.15)
      (xy -1.15 -1.15)
      (xy -1.15 -1)
      (xy -1.3 -1)
      (xy -1.3 -1.15)
      (xy -1.15 -1.3)
      (xy 1.15 -1.3)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp ed4a9063-f1b5-4621-96a1-0a7d4fa67ba7))
  (fp_rect (start -1 -1) (end 1 1)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp fbc7c6f0-0b5f-4051-ba68-826a24b21709))
  (pad "1" smd roundrect (at -0.95 -0.8) (size 0.5 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp e117f2b4-6053-48bf-a38a-340c4ac99766))
  (pad "2" smd roundrect (at -0.95 -0.4) (size 0.5 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 2c6f3909-ae02-4558-bc11-2de876532eb6))
  (pad "3" smd roundrect (at -0.95 0) (size 0.5 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp c2f46c5c-a703-4670-9450-99ee66fea98f))
  (pad "4" smd roundrect (at -0.95 0.4) (size 0.5 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp c0bce34c-0a39-4b09-b6e9-d291b60adcba))
  (pad "5" smd roundrect (at -0.95 0.8) (size 0.5 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 0f58ae7a-e2dc-4c1f-b5e6-44448f71c560))
  (pad "6" smd roundrect (at 0.95 0.8) (size 0.5 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp d378da9e-2cfd-47c5-9e11-22b405354071))
  (pad "7" smd roundrect (at 0.95 0.4) (size 0.5 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp c97f75f1-8dc9-4866-975a-0eb73995fe21))
  (pad "8" smd roundrect (at 0.95 0) (size 0.5 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 6d139cfc-9986-4950-b2ff-f3d7fcc85bb6))
  (pad "9" smd roundrect (at 0.95 -0.4) (size 0.5 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 2461d350-dd46-45fc-812b-eaf399db81df))
  (pad "10" smd roundrect (at 0.95 -0.8) (size 0.5 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 3afb4675-16b3-4613-a66e-82a19ac645cc))
  (pad "11" smd roundrect (at 0 0) (size 0.9 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05555555556)
    (thermal_bridge_angle 45) (tstamp fc4a9afa-aff1-4a6e-abde-a003fa7d44f2))
  (model "${KICAD7_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/DFN-10_2x2mm_P0.4mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
