(footprint "Raspberry-Pi-4-Compute-Module_Board" (version 20210126) (generator pcbnew) (layer "F.Cu")
  (tedit 60340DAF)
  (descr "Raspberry Pi 4 Compute Module")
  (tags "Raspberry Pi 4 Compute Module")
  (property "Field4" "Hirose")
  (property "Field5" "2x DF40C-100DS-0.4V")
  (property "Sheetfile" "PiCoral.kicad_sch")
  (property "Sheetname" "")
  (attr exclude_from_pos_files)
  (fp_text reference "Module1" (at 18.38 -5.08 -90) (layer "F.SilkS") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 5985c070-37d2-4377-966f-286e18fe7aa6)
  )
  (fp_text value "ComputeModule4-CM4" (at 16.52 0.19 -180) (layer "F.Fab") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 7bd30356-abe1-4ef2-8b8b-5597873bc529)
  )
  (fp_line (start 0 3.5) (end 33 3.5) (layer "F.SilkS") (width 0.12) (tstamp 0b96ae17-34b9-4591-a84b-8dea994ba552))
  (fp_line (start -3.5 -48) (end -3.5 0) (layer "F.SilkS") (width 0.12) (tstamp 95b013d2-cd4e-442d-94f9-5af6e8c5414e))
  (fp_line (start 36.5 0) (end 36.5 -48) (layer "F.SilkS") (width 0.12) (tstamp cb796acb-b65f-42f9-9fc8-ccfca93e8656))
  (fp_line (start 33 -51.5) (end 0 -51.5) (layer "F.SilkS") (width 0.12) (tstamp fc8a283b-9ebd-43d9-991a-8dedd34bf3e0))
  (fp_arc (start 33 -48) (end 36.5 -48) (angle -90) (layer "F.SilkS") (width 0.12) (tstamp 2aa61511-a7dd-4bf1-91a3-3cf7f2621a30))
  (fp_arc (start 0 0) (end -3.5 0) (angle -90) (layer "F.SilkS") (width 0.12) (tstamp b1d16cbd-7b9f-445c-9f7c-845f807cadfe))
  (fp_arc (start 0 -48) (end 0 -51.5) (angle -90) (layer "F.SilkS") (width 0.12) (tstamp df36e5f4-25bf-4f15-bd38-15314c65acb9))
  (fp_arc (start 33 0) (end 33 3.5) (angle -90) (layer "F.SilkS") (width 0.12) (tstamp e75628b0-c157-41a7-b3ee-f04418baa20d))
  (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask)
    (solder_mask_margin 1.7) (clearance 1.7) (tstamp 4477391f-a295-4853-b3f8-b7c4309e1410))
  (pad "" np_thru_hole circle (at 33 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask)
    (solder_mask_margin 1.7) (clearance 1.7) (tstamp 5a085fd5-e3e6-4775-8949-25b9c7d54561))
  (pad "" np_thru_hole circle (at 33 -48) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask)
    (solder_mask_margin 1.7) (clearance 1.7) (tstamp 5b1c01b2-4796-4fca-803d-c7762c6cc148))
  (pad "" np_thru_hole circle (at 0 -48) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask)
    (solder_mask_margin 1.7) (clearance 1.7) (tstamp fe99c07a-397e-43ec-be8a-0894c2c49219))
  (model "${KICAD7_3DMODEL_DIR}/Connector_Hirose.3dshapes/DF40C-100DS.stp" hide
    (offset (xyz -0.46 15.38 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
  (model "${KICAD7_3DMODEL_DIR}/Connector_Hirose.3dshapes/DF40C-100DS.stp" hide
    (offset (xyz 33.46 15.38 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
  (model "${KICAD7_3DMODEL_DIR}/Module.3dshapes/Raspberry_Pi_Compute_Module_4.step"
    (offset (xyz 52.5 -3.5 1.5))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 -90))
  )
)
