(module Fairchild_DFB2060_Bridge_Rectifier (layer F.Cu) (tedit 57E106A5)
  (fp_text reference REF** (at -7.5 3.7) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Fairchild_DFB2060_Bridge_Rectifier (at 0 -1) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -15 0) (end -15 4.6) (layer F.Fab) (width 0.05))
  (fp_line (start -15 4.6) (end 15 4.6) (layer F.Fab) (width 0.05))
  (fp_line (start 15 4.6) (end 15 0) (layer F.Fab) (width 0.05))
  (fp_line (start 15 0) (end -15 0) (layer F.Fab) (width 0.05))
  (fp_line (start -15 3.6) (end 15 3.6) (layer F.Fab) (width 0.05))
  (fp_line (start -1.5 3.6) (end -1.5 0) (layer F.Fab) (width 0.05))
  (fp_line (start 1.5 3.6) (end 1.5 0) (layer F.Fab) (width 0.05))
  (fp_line (start -15 0) (end -15 4.6) (layer F.SilkS) (width 0.125))
  (fp_line (start -15 4.6) (end -14 4.6) (layer F.SilkS) (width 0.125))
  (fp_line (start -15 0) (end 15 0) (layer F.SilkS) (width 0.125))
  (fp_line (start 15 0) (end 15 4.6) (layer F.SilkS) (width 0.125))
  (fp_line (start 15 4.6) (end 14 4.6) (layer F.SilkS) (width 0.125))
  (fp_line (start 11 4.6) (end 6.5 4.6) (layer F.SilkS) (width 0.125))
  (fp_line (start 3.5 4.6) (end -1 4.6) (layer F.SilkS) (width 0.125))
  (fp_line (start -4 4.6) (end -11 4.6) (layer F.SilkS) (width 0.125))
  (fp_line (start -10 0.75) (end -10 1.75) (layer F.SilkS) (width 0.125))
  (fp_line (start -10.5 1.25) (end -9.5 1.25) (layer F.SilkS) (width 0.125))
  (fp_line (start 10.5 1.25) (end 9.5 1.25) (layer F.SilkS) (width 0.125))
  (fp_arc (start -5.25 1.25) (end -5.5 1.25) (angle 180) (layer F.SilkS) (width 0.125))
  (fp_arc (start -4.75 1.25) (end -4.5 1.25) (angle 180) (layer F.SilkS) (width 0.125))
  (fp_arc (start 7.25 1.25) (end 7 1.25) (angle 180) (layer F.SilkS) (width 0.125))
  (fp_arc (start 7.75 1.25) (end 8 1.25) (angle 180) (layer F.SilkS) (width 0.125))
  (pad 1 thru_hole roundrect (at -12.5 3.025) (size 2.5 4) (drill 1.6 (offset 0 -0.5)) (layers *.Cu *.Mask)(roundrect_rratio 0.25))
  (pad 2 thru_hole roundrect (at -2.5 3.025) (size 2.5 4) (drill 1.6 (offset 0 -0.5)) (layers *.Cu *.Mask)(roundrect_rratio 0.25))
  (pad 3 thru_hole roundrect (at 5 3.025) (size 2.5 4) (drill 1.6 (offset 0 -0.5)) (layers *.Cu *.Mask)(roundrect_rratio 0.25))
  (pad 4 thru_hole roundrect (at 12.5 3.025) (size 2.5 4) (drill 1.6 (offset 0 -0.5)) (layers *.Cu *.Mask)(roundrect_rratio 0.25))
)
