(footprint "JST_PH_S2B-PH-SM4-TB_1x02-1MP_P2.00mm_Horizontal" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "JST PH series connector, S2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
  (tags "connector JST PH top entry")
  (property "Sheetfile" "Servo_Controller.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Fan")
  (property "ki_keywords" "Fan Motor")
  (attr smd)
  (fp_text reference "M2" (at 0 -5.8) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6ad02d50-b5ad-41f0-b574-1973995c5c49)
  )
  (fp_text value "Fan" (at 0 4.1) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp 5e97314a-dd85-4114-8d6b-0033b5128567)
  )
  (fp_text user "${REFERENCE}" (at 0 3.7) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp adcadca2-ee2d-4ef8-aece-191d0abfc32d)
  )
  (fp_line (start -4.06 -3.31) (end -3.04 -3.31)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b7cf5423-8a84-4928-aa76-768920d67e78))
  (fp_line (start -4.06 0.94) (end -4.06 -3.31)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ea8831fe-f149-4aad-abfd-d702bd97f5f1))
  (fp_line (start -3.04 -3.31) (end -3.04 -1.71)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 96009ce7-0c87-48a2-8a8f-b22b0d3ac6d6))
  (fp_line (start -3.04 -1.71) (end -1.76 -1.71)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 11ffdb90-e2ee-4b9a-830c-d181469a4920))
  (fp_line (start -2.34 4.51) (end 2.34 4.51)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp be550e85-9c78-4f48-8a6e-dc473df5d2b3))
  (fp_line (start -1.76 -1.71) (end -1.76 -4.6)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c53632ef-d605-40bf-a79f-66d52a8f77b5))
  (fp_line (start 3.04 -3.31) (end 3.04 -1.71)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ddb511ba-c78d-4764-a94e-195cad612791))
  (fp_line (start 3.04 -1.71) (end 1.76 -1.71)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cf0dcd16-1476-43bb-a22e-75cba5f1cd63))
  (fp_line (start 4.06 -3.31) (end 3.04 -3.31)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c82758ca-7dc4-449a-8b81-5035eaffddd0))
  (fp_line (start 4.06 0.94) (end 4.06 -3.31)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fb934ede-549e-4bab-91a9-a4c766e57efc))
  (fp_line (start -4.25 1.45) (end -4.25 4.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 582bd89f-8db7-4184-b7e8-3ba218aed00f))
  (fp_line (start -4.2 -3.2) (end -4.197297 1.251544)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 538b2903-d525-4b45-bb73-b5425a596f69))
  (fp_line (start -3.95 -3.45) (end -1.65 -3.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d59207da-3017-451b-b947-0dad5bb8f2c0))
  (fp_line (start -3.85 4.75) (end 3.85 4.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f6f39a34-b8de-4383-a0a0-46d41b118dc3))
  (fp_line (start -1.65 -3.45) (end -1.65 -4.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f8447b49-abd2-4d04-bbc6-403b338e809d))
  (fp_line (start -1.25 -4.75) (end 1.25 -4.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 274d94ee-efd6-40b5-b808-66f272232090))
  (fp_line (start 1.65 -3.45) (end 1.65 -4.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f5a30a87-621b-4c3c-8ee7-fb9fc6822f01))
  (fp_line (start 3.95 -3.45) (end 1.65 -3.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3e9e9643-16ee-44cc-8e08-1424a5f7487c))
  (fp_line (start 4.2 -3.2) (end 4.197297 1.251544)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6b720508-ef6d-4b34-bd5d-3caad47061d0))
  (fp_line (start 4.25 1.45) (end 4.25 4.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 73550157-4327-4235-aa86-7561054a0537))
  (fp_arc (start -4.25 1.45) (mid -4.2366 1.347333) (end -4.197297 1.251544)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9ca7ced1-3398-4f00-9955-0c9c35ab2cd3))
  (fp_arc (start -4.2 -3.2) (mid -4.126777 -3.376777) (end -3.95 -3.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 35f8a424-47a8-4260-9a91-2a7c9878ea3e))
  (fp_arc (start -3.85 4.75) (mid -4.132843 4.632843) (end -4.25 4.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d48f5a09-06e3-4ab3-ac07-823f9129ee9c))
  (fp_arc (start -1.65 -4.35) (mid -1.532843 -4.632843) (end -1.25 -4.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d78f8a8a-7a5c-451d-94c2-00baa129d2d8))
  (fp_arc (start 1.25 -4.75) (mid 1.532843 -4.632843) (end 1.65 -4.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 43d3894e-e7ba-4542-89fe-4223c9b35d85))
  (fp_arc (start 3.95 -3.45) (mid 4.126777 -3.376777) (end 4.2 -3.2)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0045cd8b-f1c8-4e57-b932-c195c57d10c2))
  (fp_arc (start 4.197297 1.251544) (mid 4.2366 1.347333) (end 4.25 1.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp cfcfc4cb-aba8-4688-b88c-048f03356a1f))
  (fp_arc (start 4.25 4.35) (mid 4.132843 4.632843) (end 3.85 4.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d2266c1e-0a87-4a85-be4d-2da651a6d784))
  (fp_line (start -3.95 -3.2) (end -3.95 4.4)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 29480652-8c66-4051-bc75-36253726ed15))
  (fp_line (start -3.95 -3.2) (end -3.15 -3.2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cb0f4c8c-4cfc-4e5a-a14d-c44cbf9d36e7))
  (fp_line (start -3.95 4.4) (end 3.95 4.4)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 77f30657-60d1-4863-9b19-e6ff4841ae25))
  (fp_line (start -3.15 -3.2) (end -3.15 -1.6)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 31ada00b-594b-4acc-a39c-1a383690dfc3))
  (fp_line (start -3.15 -1.6) (end 3.15 -1.6)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 22d974fc-4754-4720-93ac-4acbd663f17a))
  (fp_line (start -1.5 -1.6) (end -1 -0.892893)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e965b576-8fd5-40f1-a472-a9e728676ce0))
  (fp_line (start -1 -0.892893) (end -0.5 -1.6)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 02787e05-afd9-4f8e-a3e2-537236432591))
  (fp_line (start 3.15 -3.2) (end 3.95 -3.2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3c17327f-7cf9-4260-b82b-c2e41320449e))
  (fp_line (start 3.15 -1.6) (end 3.15 -3.2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ef41dc58-712b-4fbc-85f6-2ba5d5858004))
  (fp_line (start 3.95 -3.2) (end 3.95 4.4)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ce6e58d1-fdf8-45a5-b20e-13ee7ef1a546))
  (pad "1" smd roundrect (at -1 -2.85) (size 1 3.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 251a8f8d-dec3-410c-b133-6599a6d960e8))
  (pad "2" smd roundrect (at 1 -2.85) (size 1 3.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b3b18ea0-2264-408e-b8a0-c58b01b20ff7))
  (pad "MP" smd roundrect (at -3.35 2.9) (size 1.5 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.166667) (tstamp 7c4c4e4f-d58c-481a-acc7-9d0fb32b53e3))
  (pad "MP" smd roundrect (at 3.35 2.9) (size 1.5 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.166667) (tstamp 1959b52f-eb53-47aa-8788-230027a9dcca))
  (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_S2B-PH-SM4-TB_1x02-1MP_P2.00mm_Horizontal.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model ":KICAD7_3DMODEL_DIR:Connector_JST.3dshapes/S2B-PH-SM4-TB.STEP"
    (offset (xyz -7.9 12.6 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
