(footprint "AMASS_XT30PW-M_1x02_P2.50mm_Horizontal" (version 20220621) (generator pcbnew)
  (layer "F.Cu")
  (descr "Connector XT30 Horizontal PCB Male, https://www.tme.eu/en/Document/ce4077e36b79046da520ca73227e15de/XT30PW%20SPEC.pdf")
  (tags "RC Connector XT30")
  (property "Sheetfile" "File: AK80 Controller v1.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Generic connectable mounting pin connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
  (property "ki_keywords" "connector")
  (attr through_hole)
  (fp_text reference "J1" (at 0 1.4) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp bec5c389-556a-4594-b5e8-ad4787d61aad)
  )
  (fp_text value "VIN" (at 0 -16.6) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 5053f5cc-926a-4b11-a2b5-c12051af4902)
  )
  (fp_text user "+" (at 0.7 -13.7) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 29418739-4072-47d0-8afa-2aba273ee912)
  )
  (fp_text user "-" (at -0.7 -13.7) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 57cc60aa-37ff-4da1-9126-2a27e9a4ab9f)
  )
  (fp_text user "${REFERENCE}" (at 0 -10.1) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2953e216-b5ca-46f8-a5ea-170df2e12204)
  )
  (fp_line (start -5.06 -4.21) (end -5.65 -4.21)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 90b1a5fb-268e-4589-b092-85666cef90c1))
  (fp_line (start -5.06 -4.21) (end -5.06 -9.11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4cdbc41a-7a03-4089-afe5-9201bde8722a))
  (fp_line (start -5.06 -1.99) (end -5.65 -1.99)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 541633ad-2ee8-4ab7-ae01-a28fb82d341a))
  (fp_line (start -5.06 0.11) (end -5.06 -1.99)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 83af9ce8-3456-4a3b-8d49-4bf3bb7d034d))
  (fp_line (start 5.06 -9.11) (end -5.06 -9.11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 742ff1c6-2537-448f-bc41-7dd1f2aa3f0b))
  (fp_line (start 5.06 -4.21) (end 5.06 -9.11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f953f0bd-bb0a-4b0e-9bd8-0493dd5b3a02))
  (fp_line (start 5.06 0.11) (end -5.06 0.11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3084a53e-fb59-4703-a953-ec2c4615a667))
  (fp_line (start 5.06 0.11) (end 5.06 -1.99)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 88d7a8ac-b8fb-4a73-b8e6-fbcbb4925eb5))
  (fp_line (start 5.65 -4.21) (end 5.06 -4.21)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5175911c-648f-4504-b9e4-eefdeb49255e))
  (fp_line (start 5.65 -1.99) (end 5.06 -1.99)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3fb826c4-3d72-4ba9-a0c1-65a342fca8d9))
  (fp_arc (start -5.65 -1.99) (mid -6.76 -3.1) (end -5.65 -4.21)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e6037c0a-9a1e-4b37-974f-43f1eaf824eb))
  (fp_arc (start 5.65 -4.21) (mid 6.76 -3.1) (end 5.65 -1.99)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c7a1631d-74eb-491c-967e-f4235c688917))
  (fp_line (start -7 -4.75) (end -7 -1.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3878ed7f-c883-4b8c-97cd-aa3dbb6692b4))
  (fp_line (start -7 -1.5) (end -5.5 -1.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f484fd00-1427-4d0a-b638-f061e86c27cd))
  (fp_line (start -5.5 -9) (end -5.5 -4.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 8bd6169d-9c44-436e-a925-1150f15e200a))
  (fp_line (start -5.5 -4.75) (end -7 -4.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a1f28810-b857-4b5f-a8e1-913767c12298))
  (fp_line (start -5.5 -1.5) (end -5.5 0.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a737d999-431b-42f2-bd79-f78b9f9e2620))
  (fp_line (start -5.5 0.5) (end 5.5 0.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d18179ec-e9cf-4b4e-a5e7-f677d56d760c))
  (fp_line (start -4.25 -13) (end -4.25 -9.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6c6d2d8c-eabd-41da-ad44-69f09c4b7b9f))
  (fp_line (start -4.25 -9.5) (end -5 -9.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ff555d61-c4fe-4c1d-8e60-5f4d6162a7c9))
  (fp_line (start -2.5 -14.75) (end 2.5 -14.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1cd5204a-aa28-45c5-a5c8-12b24be3903d))
  (fp_line (start 4.25 -13) (end 4.25 -9.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 03c1a06d-eb85-47ff-895c-9f4dd5f164f7))
  (fp_line (start 4.25 -9.5) (end 5 -9.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6cf086a9-b8b7-4267-8869-49d6e6c40563))
  (fp_line (start 5.5 -4.75) (end 5.5 -9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 21e4650d-c611-43ae-a8d1-931d8587ae53))
  (fp_line (start 5.5 -1.5) (end 7 -1.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e7335d42-987f-40cb-9a4c-f0236f972c4b))
  (fp_line (start 5.5 0.5) (end 5.5 -1.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 69d33f92-e77a-47b4-b5a1-f16fb7ad52f9))
  (fp_line (start 7 -4.75) (end 5.5 -4.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 5df30c2f-f8c3-4714-b345-863fb888f46b))
  (fp_line (start 7 -1.5) (end 7 -4.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 8a89ca73-07c6-465d-b344-6cc5c228700a))
  (fp_arc (start -5.5 -9) (mid -5.353553 -9.353553) (end -5 -9.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 7fcc7fbd-fbeb-400c-9d7e-0761470f77e5))
  (fp_arc (start -4.25 -13) (mid -3.737437 -14.237437) (end -2.5 -14.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0c7ee5d3-a0b6-489e-8088-4227864d99b6))
  (fp_arc (start 2.5 -14.75) (mid 3.737437 -14.237437) (end 4.25 -13)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a78cc0cf-52f1-4b8e-8a90-613a3d5464dd))
  (fp_arc (start 5 -9.5) (mid 5.353553 -9.353553) (end 5.5 -9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2ac5b06c-2851-4d53-a5f9-cd5bae78fd8b))
  (fp_line (start -4.95 -4.1) (end -5.65 -4.1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 28cbb325-dcb8-4db0-bf4c-e17d7ed387cd))
  (fp_line (start -4.95 -4.1) (end -4.95 -9)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2b636d1c-9b97-4fc9-a1ec-014877563c0f))
  (fp_line (start -4.95 -2.1) (end -5.65 -2.1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7b59c035-43a6-4de5-8a78-06b60198d46b))
  (fp_line (start -4.95 0) (end -4.95 -2.1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 09aca410-1166-44a2-969a-474083e2ec4c))
  (fp_line (start 4.95 -9) (end -4.95 -9)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d55ef1ab-7ca6-480e-8413-86ebaa85c1c9))
  (fp_line (start 4.95 -4.1) (end 4.95 -9)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3a921fe4-8e8b-4371-860b-82ebd8445d88))
  (fp_line (start 4.95 0) (end -4.95 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 532615dc-12b9-4426-8040-d7fca77ed8b0))
  (fp_line (start 4.95 0) (end 4.95 -2.1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fd0d2d39-6c71-4241-81bf-5241e4c946e6))
  (fp_line (start 5.65 -4.1) (end 4.95 -4.1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b3cf3460-bc19-40be-9f7a-def56718059e))
  (fp_line (start 5.65 -2.1) (end 4.95 -2.1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ccba3c1e-a0a7-43e7-95c2-5ff4144bd478))
  (fp_arc (start -5.65 -2.1) (mid -6.65 -3.1) (end -5.65 -4.1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7c370942-a096-448a-94fd-ba00d9cf0016))
  (fp_arc (start 5.65 -4.1) (mid 6.65 -3.1) (end 5.65 -2.1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 194460aa-ccff-4e66-831b-eb99f081066a))
  (pad "1" thru_hole circle (at -2.5 -13 180) (size 2.5 2.5) (drill 1.9) (layers *.Cu *.Mask) (tstamp 4ae371e8-60ff-4b74-b65e-55d96516dc21))
  (pad "1" connect roundrect (at -2.5 -13 180) (size 3.5 3.5) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25) (tstamp f00800e9-d036-4f84-9a87-43bc89383be7))
  (pad "2" thru_hole circle (at 2.5 -13 180) (size 2.5 2.5) (drill 1.9) (layers *.Cu *.Mask) (tstamp 4cad8d57-1612-4ae2-abe0-26f201784346))
  (pad "2" connect circle (at 2.5 -13 180) (size 3.5 3.5) (layers "B.Cu" "B.Mask") (tstamp 9fbb6afe-5771-4515-84ea-558d5155e51d))
  (pad "MP" thru_hole circle (at -5.5 -3.1 180) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask) (tstamp 83120044-d28a-4f58-bb41-92b2b7b295f1))
  (pad "MP" connect circle (at -5.5 -3.1 180) (size 2.1 2.1) (layers "B.Cu" "B.Mask") (tstamp 21f4f164-c367-42ea-b283-66028ef2b064))
  (pad "MP" thru_hole circle (at 5.5 -3.1 180) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask) (tstamp 0bbeef76-437a-476b-a6f2-739909e764a4))
  (pad "MP" connect circle (at 5.5 -3.1 180) (size 2.1 2.1) (layers "B.Cu" "B.Mask") (tstamp 40fe85ac-3810-4c37-9391-b5b80c81ad3d))
  (model "${KICAD7_3DMODEL_DIR}/Connector_AMASS.3dshapes/XT30PW-M.stp"
    (offset (xyz 0 9 2.55))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
