(module "Panasonic_EVP-BB" (layer F.Cu) (tedit 5E01CA15)
  (attr smd)
  (fp_text reference "REF**" (at 0 -1.5 unlocked) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text value "Panasonic_EVP-BB" (at 0 1.6 unlocked) (layer F.Fab)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.Fab) (width 0.12))
  (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.Fab) (width 0.12))
  (fp_line (start 1.3 0.8) (end -1.3 0.8) (layer F.Fab) (width 0.12))
  (fp_line (start -1.3 0.8) (end -1.3 -0.8) (layer F.Fab) (width 0.12))
  (fp_line (start -1.3 -0.8) (end -0.9 -0.9) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.9 -0.9) (end 0.9 -0.9) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.9 -0.9) (end 1.3 -0.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.3 0.8) (end -0.9 0.9) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.9 0.9) (end 0.9 0.9) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.9 0.9) (end 1.3 0.8) (layer F.SilkS) (width 0.15))
  (fp_circle (center 0 0) (end 0.35 0) (layer F.Fab) (width 0.15))
  (fp_line (start -1.7 -0.8) (end -0.9 -1.1) (layer F.CrtYd) (width 0.12))
  (fp_line (start -0.9 -1.1) (end 0.9 -1.1) (layer F.CrtYd) (width 0.12))
  (fp_line (start 0.9 -1.1) (end 1.7 -0.8) (layer F.CrtYd) (width 0.12))
  (fp_line (start 1.7 -0.8) (end 1.7 0.8) (layer F.CrtYd) (width 0.12))
  (fp_line (start 1.7 0.8) (end 0.9 1.1) (layer F.CrtYd) (width 0.12))
  (fp_line (start 0.9 1.1) (end -0.9 1.1) (layer F.CrtYd) (width 0.12))
  (fp_line (start -0.9 1.1) (end -1.7 0.8) (layer F.CrtYd) (width 0.12))
  (fp_line (start -1.7 0.8) (end -1.7 -0.8) (layer F.CrtYd) (width 0.12))
  (pad "1" smd roundrect (at -1.325 -0.375) (size 0.55 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.111))
  (pad "1" smd roundrect (at -1.325 0.375) (size 0.55 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.111))
  (pad "2" smd roundrect (at 1.325 -0.375) (size 0.55 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.111))
  (pad "2" smd roundrect (at 1.325 0.375) (size 0.55 0.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.111))
  (model "${KICAD7_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/EVPBB0AAB000.step"
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
