(module JST_GH_BM05B-GHS (layer F.Cu) (tedit 57519B01)
  (descr "JST GH series connector, BM05B-GHS-TBT, top entry type")
  (tags "connector jst GH SMT top vertical entry 1.25mm pitch")
  (attr smd)
  (fp_text reference P2 (at -4.25 -2) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value UART (at 0 -3.25) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_line (start -3.15 2.975) (end 3.15 2.975) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.15 2.975) (end 3.15 2.475) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.15 2.475) (end -3.15 2.475) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.15 2.475) (end -3.15 2.975) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.85 -0.225) (end -4.85 -1.325) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.85 -1.325) (end -3.2 -1.325) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.2 -1.325) (end -3.2 -0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.2 -0.825) (end -4.35 -0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.35 -0.825) (end -4.35 -0.225) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.35 -0.225) (end -4.85 -0.225) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.85 -0.225) (end 4.85 -1.325) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.85 -1.325) (end 3.2 -1.325) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.2 -1.325) (end 3.2 -0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.2 -0.825) (end 4.35 -0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.35 -0.825) (end 4.35 -0.225) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.35 -0.225) (end 4.85 -0.225) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.75 0.325) (end -2.75 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.75 0.825) (end -2.25 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.25 0.825) (end -2.25 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.25 0.325) (end -2.75 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.5 0.325) (end -1.5 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.5 0.825) (end -1 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start -1 0.825) (end -1 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start -1 0.325) (end -1.5 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.25 0.325) (end -0.25 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.25 0.825) (end 0.25 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.25 0.825) (end 0.25 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.25 0.325) (end -0.25 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start 1 0.325) (end 1 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start 1 0.825) (end 1.5 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.5 0.825) (end 1.5 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.5 0.325) (end 1 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.25 0.325) (end 2.25 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.25 0.825) (end 2.75 0.825) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.75 0.825) (end 2.75 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.75 0.325) (end 2.25 0.325) (layer F.SilkS) (width 0.15))
  (fp_line (start -5.25 -3.05) (end -5.25 3.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.25 3.6) (end 5.25 3.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5.25 3.6) (end 5.25 -3.05) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5.25 -3.05) (end -5.25 -3.05) (layer F.CrtYd) (width 0.05))
  (pad 1 smd roundrect (at -2.5 -1.675) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (pad 2 smd roundrect (at -1.25 -1.675) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (pad 3 smd roundrect (at 0 -1.675) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (pad 4 smd roundrect (at 1.25 -1.675) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (pad 5 smd roundrect (at 2.5 -1.675) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (pad 6 smd roundrect (at 4.25 1.675) (size 1 2.8) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (pad 6 smd roundrect (at -4.25 1.675) (size 1 2.8) (layers F.Cu F.Paste F.Mask)(roundrect_rratio 0.25))
  (model 3D/SH/JST_GH_BM05B-GHS.wrl
    (at (xyz -0.187 -0.095 0.01))
    (scale (xyz 0.3937 0.3937 0.3937))
    (rotate (xyz 90 180 0))
  )
)
