(module JP-3 (layer F.Cu) (tedit 59EE1E55)
  (solder_mask_margin 0.1)
  (fp_text reference JP1 (at 0 -1) (layer F.Fab)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text value PWRSRC (at 0 0.7) (layer F.Fab) hide
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (pad 3 connect rect (at 0.45 0) (size 0.25 1) (layers F.Cu))
  (pad 2 connect rect (at 0 0) (size 0.25 1) (layers F.Cu))
  (pad 1 connect rect (at -0.45 0) (size 0.25 1) (layers F.Cu))
  (pad 4 connect rect (at 0 0) (size 0.95 0.8) (layers F.Mask))
  (pad 5 smd roundrect (at -0.25 0) (size 0.8 1.2) (layers F.Paste)(roundrect_rratio 0.15))
)
