(footprint "Texas_RGE0024C_EP2.1x2.1mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Texas  QFN, 24 Pin (http://www.ti.com/lit/ds/symlink/pca9548a.pdf#page=37), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "Texas QFN NoLead")
  (property "LCSC" "C555456")
  (property "MFG" "TI")
  (property "MPN" "TCA9548ARGER")
  (property "Sheetfile" "QuadCameraCarrier.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Low voltage 8-channel I2C switch with reset, QFN-24")
  (property "ki_keywords" "Low voltage 8-channel I2C switch with reset")
  (attr smd)
  (fp_text reference "U10" (at 0 -3.32) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 79a0b164-b961-4a27-afb2-5299ab0fe067)
  )
  (fp_text value "TCA9548ARGER" (at 0 3.32) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b9557e11-5b1e-4ebf-8268-351d25cd0d93)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f3a74720-42dd-49a1-87b9-62baa3f9349c)
  )
  (fp_line (start -2.11 2.11) (end -2.11 1.635)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7a230948-0bbd-4656-94a8-8e6ca9768713))
  (fp_line (start -1.635 -2.11) (end -2.11 -2.11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 94c63a9b-c7af-487e-a63c-f286dfc55d72))
  (fp_line (start -1.635 2.11) (end -2.11 2.11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 86d9a6b0-1239-4e17-8c64-d58f92d79b0c))
  (fp_line (start 1.635 -2.11) (end 2.11 -2.11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9b869f7b-dfd5-4cd8-aea5-8787ef59bd42))
  (fp_line (start 1.635 2.11) (end 2.11 2.11)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c8c5631b-4aa7-4da3-9938-be98663db61b))
  (fp_line (start 2.11 -2.11) (end 2.11 -1.635)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f0d3765e-cb4c-4127-905b-a271d6a03845))
  (fp_line (start 2.11 2.11) (end 2.11 1.635)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9859d7d0-52fb-4bee-855e-710d8fc88f5e))
  (fp_line (start -2.45 -1.3) (end -2.45 1.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2e454f57-b36b-4cb5-9604-24659d70aa78))
  (fp_line (start -2.25 -2) (end -2.249847 -1.523624)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e9479b0a-476d-4dd8-9157-b276db7c44ed))
  (fp_line (start -2.25 2) (end -2.249847 1.523624)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 29783207-f449-43a1-b5ae-8be17a19e391))
  (fp_line (start -2 -2.25) (end -1.523624 -2.249847)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a405e5de-109a-4d5f-806b-64cbc50752de))
  (fp_line (start -2 2.25) (end -1.523624 2.249847)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f0e66b9f-820a-434e-ad54-c95ffd5dcaae))
  (fp_line (start -1.3 2.45) (end 1.3 2.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b5f81bbe-eae1-4930-b97f-0d2521f8f73d))
  (fp_line (start 1.3 -2.45) (end -1.3 -2.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 80df3c83-ef30-4c80-9f12-6a447d27fac3))
  (fp_line (start 2 -2.25) (end 1.523624 -2.249847)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9ebad39d-333d-4e38-a56d-53d887136083))
  (fp_line (start 2 2.25) (end 1.523624 2.249847)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 37698de8-c7a9-47d8-afe0-7c30022a819d))
  (fp_line (start 2.25 -2) (end 2.249847 -1.523624)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 8ffb9985-a657-467a-86f9-d250ea8e96a0))
  (fp_line (start 2.25 2) (end 2.249847 1.523624)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 62f0dda1-9f30-4ada-915e-05f953010248))
  (fp_line (start 2.45 -1.3) (end 2.45 1.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4c19a62f-f159-420f-91b3-57165646839d))
  (fp_arc (start -2.45 -1.3) (mid -2.392654 -1.450058) (end -2.249847 -1.523624)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 7e661595-2af1-45f0-84b6-9d735423364b))
  (fp_arc (start -2.25 -2) (mid -2.176777 -2.176777) (end -2 -2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 61c6a5ff-65d0-4454-97eb-82fba82a548e))
  (fp_arc (start -2.249847 1.523624) (mid -2.392653 1.450057) (end -2.45 1.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ad5e36d5-3126-4f5f-a3a7-1873d99a8a4a))
  (fp_arc (start -2 2.25) (mid -2.176777 2.176777) (end -2.25 2)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 03b85754-c94a-4a06-aeb3-c0fc20e57e68))
  (fp_arc (start -1.523624 -2.249847) (mid -1.450057 -2.392653) (end -1.3 -2.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4bd8d9e3-f8dd-4bb5-aca0-04b15f62a7d2))
  (fp_arc (start -1.3 2.45) (mid -1.450058 2.392654) (end -1.523624 2.249847)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e6ca2e07-bc70-46cc-ba25-4b277c1ad3ca))
  (fp_arc (start 1.3 -2.45) (mid 1.450057 -2.392654) (end 1.523624 -2.249847)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6101392c-cc9f-443d-b2d0-91014d5576e4))
  (fp_arc (start 1.523624 2.249847) (mid 1.450057 2.392654) (end 1.3 2.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 18eaec4e-0baa-4704-b653-5c9bd95b8e07))
  (fp_arc (start 2 -2.25) (mid 2.176777 -2.176777) (end 2.25 -2)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 77521587-6ab9-46e6-a3dd-7ed683ed133a))
  (fp_arc (start 2.249847 -1.523624) (mid 2.392654 -1.450057) (end 2.45 -1.3)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 78cd3d9c-64f3-4c94-a34a-4221eda4a68a))
  (fp_arc (start 2.25 2) (mid 2.176777 2.176777) (end 2 2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 753a4998-961c-4325-8b41-783c2e4c7719))
  (fp_arc (start 2.45 1.3) (mid 2.392654 1.450057) (end 2.249847 1.523624)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a32719b7-2bea-4c5a-b824-2c0247e4584c))
  (fp_line (start -2 -1) (end -1 -2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5a349c2e-736a-4ebf-9b74-ed72762769f1))
  (fp_line (start -2 2) (end -2 -1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7256a4e5-d31d-4782-9bb8-c0fc5859a55b))
  (fp_line (start -1 -2) (end 2 -2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 41966b62-691d-406a-8155-cfbe12852a84))
  (fp_line (start 2 -2) (end 2 2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ed6468d3-20d2-4724-8e36-be7cfd8dfd59))
  (fp_line (start 2 2) (end -2 2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp db539d57-f6a5-456c-9fa6-6b6b030e9792))
  (pad "" smd oval (at -1.9 -1.25) (size 0.6 0.2) (layers "F.Paste") (tstamp db856df8-2038-407a-b785-895e8c6f39f3))
  (pad "" smd oval (at -1.9 -0.75) (size 0.6 0.2) (layers "F.Paste") (tstamp 97c15407-fb8c-474c-a874-0ea2764e8431))
  (pad "" smd oval (at -1.9 -0.25) (size 0.6 0.2) (layers "F.Paste") (tstamp fe5f5b04-a4bd-4f56-8095-48a6bc0abb04))
  (pad "" smd oval (at -1.9 0.25) (size 0.6 0.2) (layers "F.Paste") (tstamp dd1f0d45-a779-4809-9536-736668c3f6b3))
  (pad "" smd oval (at -1.9 0.75) (size 0.6 0.2) (layers "F.Paste") (tstamp 3cf8bd0f-3b10-4b95-ab07-39849477148c))
  (pad "" smd oval (at -1.9 1.25) (size 0.6 0.2) (layers "F.Paste") (tstamp a7c2e633-6445-49ca-8c46-3d011821add8))
  (pad "" smd roundrect (at -0.525 -0.525) (size 0.85 0.85) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp b6d755ec-d5e9-48ed-aa98-5907dcc76ae9))
  (pad "" smd roundrect (at -0.525 0.525) (size 0.85 0.85) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp 66d7f4df-75eb-4420-8a7c-05810369bbc4))
  (pad "" smd roundrect (at 0.525 -0.525) (size 0.85 0.85) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp 4d0ae54d-6956-4b24-a5c5-f9c1c689b082))
  (pad "" smd roundrect (at 0.525 0.525) (size 0.85 0.85) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp f369c873-8224-4f5d-a7f8-b47bb3b46323))
  (pad "1" smd roundrect (at -1.9 -1.25) (size 0.8 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp 67b4b148-6380-4b20-93e0-ffb2a3275d21))
  (pad "2" smd roundrect (at -1.9 -0.75) (size 0.8 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp c786c447-9033-4d78-b4e1-3394324f97e2))
  (pad "3" smd roundrect (at -1.9 -0.25) (size 0.8 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp 3f2cec57-a696-4eea-b8a8-1569a60767b1))
  (pad "4" smd roundrect (at -1.9 0.25) (size 0.8 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp 194ef247-f644-45ea-a8db-bfdf3f2c5662))
  (pad "5" smd roundrect (at -1.9 0.75) (size 0.8 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp 178e8ab1-403a-4e19-aa8a-8950fb0ea839))
  (pad "6" smd roundrect (at -1.9 1.25) (size 0.8 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp cbe53dac-a754-4a35-981e-c5ffbdfa7412))
  (pad "7" smd roundrect (at -1.25 1.9 90) (size 0.8 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp 1b7a4aea-feff-4de8-9b34-0da5754229e2))
  (pad "8" smd roundrect (at -0.75 1.9 90) (size 0.8 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp 3a1402a2-484d-4bd4-a5d0-029676264cb3))
  (pad "9" smd roundrect (at -0.25 1.9 90) (size 0.8 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp 8653e90c-53b5-49c0-a93d-f74261fb2477))
  (pad "10" smd roundrect (at 0.25 1.9 90) (size 0.8 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp bec6446d-605f-41df-8e03-4d3f34f182d9))
  (pad "11" smd roundrect (at 0.75 1.9 90) (size 0.8 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp eeae0691-fc2e-4f97-8021-9a8f638e4088))
  (pad "12" smd roundrect (at 1.25 1.9 90) (size 0.8 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp 2d352b1b-48d8-42bc-bd69-1f699c077217))
  (pad "13" smd roundrect (at 1.9 1.25 180) (size 0.8 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp 858090fc-e093-4ab0-a704-79c8c633f0c8))
  (pad "14" smd roundrect (at 1.9 0.75 180) (size 0.8 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp 357595ee-e12b-4abe-90ac-03bf558b77ae))
  (pad "15" smd roundrect (at 1.9 0.25 180) (size 0.8 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp 2457f0fe-de94-42c5-9f56-5bcfad7a3007))
  (pad "16" smd roundrect (at 1.9 -0.25 180) (size 0.8 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp db2f0f83-f40d-4fee-9e65-2f65d0ec941d))
  (pad "17" smd roundrect (at 1.9 -0.75 180) (size 0.8 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp 66161ba9-5ce4-4c1e-8dc8-f4f5102571f9))
  (pad "18" smd roundrect (at 1.9 -1.25 180) (size 0.8 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp 603542c4-e50f-4f39-86b6-40caca933636))
  (pad "19" smd roundrect (at 1.25 -1.9 270) (size 0.8 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp 736811c2-b953-4f51-9484-8b5d102575af))
  (pad "20" smd roundrect (at 0.75 -1.9 270) (size 0.8 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp 4f3ebe05-9f21-4c46-93c0-d0c3d77c3e9d))
  (pad "21" smd roundrect (at 0.25 -1.9 270) (size 0.8 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp 5a1ed3ea-4e13-4cbf-822a-d925c27f8e50))
  (pad "22" smd roundrect (at -0.25 -1.9 270) (size 0.8 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp 57d5aefb-09be-4538-8ae9-f6f4eef7448c))
  (pad "23" smd roundrect (at -0.75 -1.9 270) (size 0.8 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp 95d437c0-a483-498a-b185-4fa34a0304fb))
  (pad "24" smd roundrect (at -1.25 -1.9 270) (size 0.8 0.25) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.33)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp adcb1d45-36fa-4032-a92a-37f28fe1bd33))
  (pad "25" smd rect (at 0 0) (size 2.1 2.1) (layers "F.Cu" "F.Mask") (tstamp ad9eb6af-ae92-4e0f-8ecb-88ea8ad8b8fd))
  (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_RGE0024C_EP2.1x2.1mm.wrl" hide
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model ":KICAD7_3DMODEL_DIR:Package_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
