(footprint "Ebyte E220-900M30S" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -19.95 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1bba86a6-5f61-4794-8cbc-b273a37006da)
  )
  (fp_text value "Ebyte E220-900M30S" (at 0.1 -6.1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d229479b-a2e0-4f12-b822-67aa9daca334)
  )
  (fp_text user "${REFERENCE}" (at 0.1 -4.6 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 97c24fe4-6543-4e71-8e97-4c942f1b330e)
  )
  (fp_arc (start -12.225 -19.4) (mid -12.203033 -19.453033) (end -12.15 -19.475)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 941af88a-bc61-4466-86eb-ec1493446925))
  (fp_arc (start -12.15 19.475) (mid -12.203033 19.453033) (end -12.225 19.4)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 41164346-ff78-4596-82a1-dd971747486e))
  (fp_arc (start 12.15 -19.475) (mid 12.203033 -19.453033) (end 12.225 -19.4)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp f14fca5f-57b4-459c-afe4-d508e633ff35))
  (fp_arc (start 12.225 19.4) (mid 12.203033 19.453033) (end 12.15 19.475)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 7d5e5dec-288c-4598-a96d-d17d4eccee05))
  (fp_poly
    (pts
      (xy 12.75 13.8)
      (xy 13 13.6)
      (xy 13 14)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 7c5a413e-53ee-4ad5-ad8f-24b0f541d18e))
  (fp_poly
    (pts
      (xy -12.15 17.9)
      (xy -12.15 19.4)
      (xy -10.65 19.4)
      (xy -10.65 19.55)
      (xy -12.15 19.55)
      (xy -12.3 19.4)
      (xy -12.3 17.9)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 0f207bb3-033c-46ad-b73e-1b10e3f73346))
  (fp_poly
    (pts
      (xy -10.65 -19.4)
      (xy -12.15 -19.4)
      (xy -12.15 -17.9)
      (xy -12.3 -17.9)
      (xy -12.3 -19.4)
      (xy -12.15 -19.55)
      (xy -10.65 -19.55)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 30900a0a-baaa-47c0-b412-08eeb215ebea))
  (fp_poly
    (pts
      (xy 10.65 19.4)
      (xy 12.15 19.4)
      (xy 12.15 17.9)
      (xy 12.3 17.9)
      (xy 12.3 19.4)
      (xy 12.15 19.55)
      (xy 10.65 19.55)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 7d95412b-8403-490d-b1e8-12989aab98e5))
  (fp_poly
    (pts
      (xy 12.15 -17.9)
      (xy 12.15 -19.4)
      (xy 10.65 -19.4)
      (xy 10.65 -19.55)
      (xy 12.15 -19.55)
      (xy 12.3 -19.4)
      (xy 12.3 -17.9)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp a38e1cd8-6680-4e4d-b2cb-901f666735e5))
  (fp_line (start -12.75 13.95) (end -12.75 -16.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b2af6512-0bd2-4baf-8882-84e0afc24f45))
  (fp_line (start -12.5 -19.25) (end -12.504505 -17.304955)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b6dfbb20-56f2-4c95-bf88-3f3e9ec079e3))
  (fp_line (start -12.5 19.25) (end -12.504505 14.504955)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 25e8eced-72ad-468a-a23a-5e1746227b1a))
  (fp_line (start -12 -19.75) (end 12 -19.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 974389ec-2d52-4449-ad5c-e137bb8a0a41))
  (fp_line (start 12 19.75) (end -12 19.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b3ade02e-d7fd-4d95-898a-160097c27c29))
  (fp_line (start 12.5 -19.25) (end 12.504505 -17.304955)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 68cb2279-d1be-4a98-ad1e-25ab129e9566))
  (fp_line (start 12.5 19.25) (end 12.504505 14.504955)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 9489c268-cf9a-4036-8c35-b0c7bbec6a85))
  (fp_line (start 12.75 13.95) (end 12.75 -16.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 43cbc65d-77de-443d-906b-8a8cbb0f2993))
  (fp_arc (start -12.75 -16.75) (mid -12.685886 -17.053415) (end -12.504505 -17.304955)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 5d894232-ebb6-4a71-8b52-205a61778990))
  (fp_arc (start -12.504505 14.504955) (mid -12.685886 14.253415) (end -12.75 13.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0094542b-c943-4be2-9b4f-036d1fa4c754))
  (fp_arc (start -12.5 -19.25) (mid -12.353553 -19.603553) (end -12 -19.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 8e29823a-8f46-4e06-9f2d-2d0d29c14ea4))
  (fp_arc (start -12 19.75) (mid -12.353553 19.603553) (end -12.5 19.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c091615f-cca2-4cb0-b91c-e658d19dd662))
  (fp_arc (start 12 -19.75) (mid 12.353553 -19.603553) (end 12.5 -19.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e6ad09dd-228c-4d4f-8fbf-b773a0b025c3))
  (fp_arc (start 12.5 19.25) (mid 12.353553 19.603553) (end 12 19.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp fbd05a53-b78e-4ff5-9bd3-e943efdee4a4))
  (fp_arc (start 12.504505 -17.304955) (mid 12.685886 -17.053415) (end 12.75 -16.75)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 875bf267-6971-42b5-8af4-0184594113d0))
  (fp_arc (start 12.75 13.95) (mid 12.685886 14.253415) (end 12.504505 14.504955)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c0d13dff-130f-490e-93a6-2e8702517f5b))
  (fp_rect (start -12 -19.25) (end 12 19.25)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 424841cf-7b3d-46d2-b1a8-ff27f2212a06))
  (pad "1" smd roundrect (at 11.5 13.82) (size 2.2 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.4)
    (chamfer_ratio 0.07) (chamfer top_left bottom_left) (tstamp 0613222f-bcff-4fac-a949-f71247c3f3f5))
  (pad "2" smd roundrect (at 11.5 11.28) (size 2.2 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.4)
    (chamfer_ratio 0.07) (chamfer top_left bottom_left) (tstamp 40f6fd38-c31d-4070-95b3-58316f589a9b))
  (pad "3" smd roundrect (at 11.5 8.74) (size 2.2 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.4)
    (chamfer_ratio 0.07) (chamfer top_left bottom_left) (tstamp a38ec597-cdce-43a9-a602-a4011d4e17f5))
  (pad "4" smd roundrect (at 11.5 1.14) (size 2.2 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.4)
    (chamfer_ratio 0.07) (chamfer top_left bottom_left) (tstamp 8cbc21a2-dcc3-4987-9e20-c20c9e1b5ce9))
  (pad "5" smd roundrect (at 11.5 -1.4) (size 2.2 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.4)
    (chamfer_ratio 0.07) (chamfer top_left bottom_left) (tstamp 31d0c94a-4cf3-471a-808e-48cd75408afa))
  (pad "6" smd roundrect (at 11.5 -3.94) (size 2.2 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.4)
    (chamfer_ratio 0.07) (chamfer top_left bottom_left) (tstamp 71e5b3d2-5a3a-4319-8145-01daa73bb298))
  (pad "7" smd roundrect (at 11.5 -6.48) (size 2.2 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.4)
    (chamfer_ratio 0.07) (chamfer top_left bottom_left) (tstamp dc5d2ba3-f7c3-4767-9c8e-c60cf7c1b18c))
  (pad "8" smd roundrect (at 11.5 -9.02) (size 2.2 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.4)
    (chamfer_ratio 0.07) (chamfer top_left bottom_left) (tstamp c2685043-97a1-44bb-9e86-e552e6810bbb))
  (pad "9" smd roundrect (at 11.5 -11.56) (size 2.2 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.4)
    (chamfer_ratio 0.07) (chamfer top_left bottom_left) (tstamp 55cc72f4-9a30-477b-9efd-a67990f8b06b))
  (pad "10" smd roundrect (at 11.5 -14.1) (size 2.2 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.4)
    (chamfer_ratio 0.07) (chamfer top_left bottom_left) (tstamp 0d0f1fd8-1663-499d-b383-6bfd39074c37))
  (pad "11" smd roundrect (at 11.5 -16.64) (size 2.2 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.4)
    (chamfer_ratio 0.07) (chamfer top_left bottom_left) (tstamp 8b41a9d0-ffb7-40fb-8b29-0b7de3fbb291))
  (pad "12" smd roundrect (at -11.5 -16.64 180) (size 2.2 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.4)
    (chamfer_ratio 0.07) (chamfer top_left bottom_left) (tstamp a82f8024-7987-49c0-b4a1-0f95c8efc611))
  (pad "13" smd roundrect (at -11.5 -14.1 180) (size 2.2 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.4)
    (chamfer_ratio 0.07) (chamfer top_left bottom_left) (tstamp 627a31f7-1a2f-41c4-ad6f-2c5d9eac33bf))
  (pad "14" smd roundrect (at -11.5 -11.56 180) (size 2.2 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.4)
    (chamfer_ratio 0.07) (chamfer top_left bottom_left) (tstamp ebe2c3e1-4448-4348-934a-b18b7d009e66))
  (pad "15" smd roundrect (at -11.5 -9.02 180) (size 2.2 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.4)
    (chamfer_ratio 0.07) (chamfer top_left bottom_left) (tstamp 06869ee7-018a-415f-8e1d-04513d7e1709))
  (pad "16" smd roundrect (at -11.5 -6.48 180) (size 2.2 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.4)
    (chamfer_ratio 0.07) (chamfer top_left bottom_left) (tstamp 522c45b9-7e9d-465f-822e-5eba44ecf31e))
  (pad "17" smd roundrect (at -11.5 -3.94 180) (size 2.2 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.4)
    (chamfer_ratio 0.07) (chamfer top_left bottom_left) (tstamp 2aba4c55-6e47-4829-aac0-59aac6cbf537))
  (pad "18" smd roundrect (at -11.5 -1.4 180) (size 2.2 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.4)
    (chamfer_ratio 0.07) (chamfer top_left bottom_left) (tstamp 0d6eb6d9-d6ce-46b2-b46f-49e500ebf88b))
  (pad "19" smd roundrect (at -11.5 1.14 180) (size 2.2 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.4)
    (chamfer_ratio 0.07) (chamfer top_left bottom_left) (tstamp 1fdc2937-b266-4121-adee-ad817d21bf38))
  (pad "20" smd roundrect (at -11.5 8.74 180) (size 2.2 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.4)
    (chamfer_ratio 0.07) (chamfer top_left bottom_left) (tstamp 88d8b9ad-8b31-4038-b113-c4bdc007c61d))
  (pad "21" smd roundrect (at -11.5 11.28 180) (size 2.2 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.4)
    (chamfer_ratio 0.07) (chamfer top_left bottom_left) (tstamp f86ec252-20d3-4fb8-a2f3-e2fd8dbb4b05))
  (pad "22" smd roundrect (at -11.5 13.82 180) (size 2.2 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.4)
    (chamfer_ratio 0.07) (chamfer top_left bottom_left) (tstamp 23634e01-49d1-4d2a-996c-8b941b7c2512))
  (model ":KICAD7_3DMODEL_DIR:RF_Module.3dshapes/Ebyte E220-900M30S.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
