(footprint "D_SMC" (version 20220621) (generator pcbnew)
  (layer "F.Cu")
  (descr "Diode SMC (DO-214AB)")
  (tags "Diode SMC (DO-214AB)")
  (property "Dielectric" "")
  (property "Footprint_Density" "")
  (property "Footprint_Library" "")
  (property "JLCPCB Part" "")
  (property "LCSC" "C310158")
  (property "MFG" "Brightking")
  (property "MPN" "SMDJ78CA/TR7")
  (property "MPN_ALT1" "")
  (property "Mouser" "")
  (property "Note" "")
  (property "Package" "")
  (property "Sheetfile" "File: AK80 Controller v1.kicad_sch")
  (property "Sheetname" "")
  (property "Spice_Model" "")
  (property "Spice_Netlist_Enabled" "")
  (property "Spice_Primitive" "")
  (property "Tolerance" "")
  (property "USD_per_1" "")
  (property "USD_per_1000" "")
  (property "Voltage" "")
  (attr smd)
  (fp_text reference "D10" (at 0 -4.1) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a53bff99-e8e9-4e92-ad16-96bbd9a288ff)
  )
  (fp_text value "78V 23.8A" (at 0 4.2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 90ed91c6-0451-4341-b61e-80de3c2abcef)
  )
  (fp_text user "${REFERENCE}" (at 0 -1.9) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e433612f-b733-4b37-8307-d46ba4b8d85a)
  )
  (fp_line (start -4.8 -3.25) (end 3.6 -3.25)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp faaf1fab-49da-476c-8f0a-39f783b3effe))
  (fp_line (start -4.8 3.25) (end -4.8 -3.25)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e9f06f24-8745-44e7-82bb-31861cd1a414))
  (fp_line (start -4.8 3.25) (end 3.6 3.25)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 557fdc8b-b5b3-4a24-a5cc-0347d6fb5177))
  (fp_line (start -4.8 1.4) (end -4.8 -1.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e4356a38-9584-4ded-9ff5-6c696a6e9051))
  (fp_line (start -4.4 -1.8) (end -3.8 -1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c44f3a99-ab92-4a62-b434-80a48789f41b))
  (fp_line (start -3.8 -1.8) (end -3.8 -3.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b4b73bc8-75c2-4d24-b94b-34cbbc778935))
  (fp_line (start -3.8 1.8) (end -4.4 1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 461774f0-e2f7-47bd-9c68-0df938454c00))
  (fp_line (start -3.8 3.1) (end -3.8 1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 8ae88bbf-9175-40b9-9614-73a2f57ba3d5))
  (fp_line (start -3.55 -3.35) (end 3.55 -3.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 5c5673ed-0868-40fe-a0fd-81ea86af9f73))
  (fp_line (start 3.55 3.35) (end -3.55 3.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d6d57ee4-2957-4f30-8f82-ff3a27663d53))
  (fp_line (start 3.8 -3.1) (end 3.8 -1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 774662fc-2d1e-4f61-8cc7-db6c365d9530))
  (fp_line (start 3.8 -1.8) (end 4.4 -1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 7f60b342-d5a1-4b98-b1e1-a46fa1f1da03))
  (fp_line (start 3.8 1.8) (end 3.8 3.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 04d731ff-ad9a-4e88-8bef-951436bd3a3b))
  (fp_line (start 4.4 1.8) (end 3.8 1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp bdab74d8-2537-4f0a-a30b-c3a5b59c8564))
  (fp_line (start 4.8 -1.4) (end 4.8 1.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 49902a97-f566-4a4b-844b-a91acd82530e))
  (fp_arc (start -4.8 -1.4) (mid -4.682843 -1.682843) (end -4.4 -1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 38669586-fb01-4962-9aad-d6e99b429229))
  (fp_arc (start -4.4 1.8) (mid -4.682843 1.682843) (end -4.8 1.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a2a25dca-4814-4aa8-bc0b-f2ab94970362))
  (fp_arc (start -3.8 -3.1) (mid -3.726777 -3.276777) (end -3.55 -3.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f77ecc20-2721-49ab-b437-b6c219b1fe9f))
  (fp_arc (start -3.55 3.35) (mid -3.726777 3.276777) (end -3.8 3.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp be3f6972-5a66-4a6c-b63d-e282d6c74cc9))
  (fp_arc (start 3.55 -3.35) (mid 3.726777 -3.276777) (end 3.8 -3.1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3a4d459f-669b-4866-beac-d7c795d5ff06))
  (fp_arc (start 3.8 3.1) (mid 3.726777 3.276777) (end 3.55 3.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1c6c5540-5c06-478a-bef7-11c726b81c82))
  (fp_arc (start 4.4 -1.8) (mid 4.682843 -1.682843) (end 4.8 -1.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp fe929f71-009a-4ff6-b277-df0d12b0ee38))
  (fp_arc (start 4.8 1.4) (mid 4.682843 1.682843) (end 4.4 1.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 843560ee-7b9d-4d0c-8621-902204f38196))
  (fp_line (start -3.55 3.1) (end -3.55 -3.1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9a220e62-62f3-402b-b800-dcc5a8b076d3))
  (fp_line (start -0.64944 -0.79908) (end -0.64944 0.80112)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp de16a4c0-ea02-41b0-b329-c4a3be51b851))
  (fp_line (start -0.64944 0.00102) (end -1.55114 0.00102)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ce987405-8d36-4a2b-a3d6-78c2dc8a4162))
  (fp_line (start -0.64944 0.00102) (end 0.50118 -0.79908)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8832fb62-1b93-465d-9fd2-ae77df51fca4))
  (fp_line (start -0.64944 0.00102) (end 0.50118 0.75032)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 46d38ad9-19ca-4715-93e6-6af440090e0a))
  (fp_line (start 0.50118 0.00102) (end 1.4994 0.00102)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f9b2dd3c-18c6-4a86-b3d7-2b777e110bae))
  (fp_line (start 0.50118 0.75032) (end 0.50118 -0.79908)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dd52c9eb-4608-4b20-bdef-0c503fd6c199))
  (fp_line (start 3.55 -3.1) (end -3.55 -3.1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c711b12a-b46a-4229-9747-24f2a02f9427))
  (fp_line (start 3.55 -3.1) (end 3.55 3.1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1e38d329-1fa4-4cf2-bfd9-8c4da41951c5))
  (fp_line (start 3.55 3.1) (end -3.55 3.1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d570da61-a436-41e4-8615-a1f49dc47767))
  (pad "1" smd roundrect (at -3.4 0 90) (size 3.3 2.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1) (tstamp 14a4dfc6-8717-4c80-a123-21e357e19e76))
  (pad "2" smd roundrect (at 3.4 0 90) (size 3.3 2.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1) (tstamp 6af51126-72cf-4e09-bbba-734a897224d4))
  (model "${KICAD7_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMC.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
