(module Program_Pogo_6P_1.25mm (layer F.Cu) (tedit 56AA7495)
  (solder_mask_margin 0.001)
  (attr virtual)
  (fp_text reference P1 (at -1.8 0 90) (layer Cmts.User)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text value CONN-5 (at 1.7 0 90) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text user 1 (at 0 -4.325) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (pad 1 thru_hole rect (at 0 -3.125) (size 2 1.05) (drill 0.74) (layers *.Cu *.Mask))
  (pad 2 connect oval (at 0 -1.875) (size 2 1.05) (layers F.Cu F.Mask))
  (pad 3 connect oval (at 0 -0.625) (size 2 1.05) (layers F.Cu F.Mask))
  (pad 4 connect oval (at 0 0.625) (size 2 1.05) (layers F.Cu F.Mask))
  (pad 5 connect oval (at 0 1.875) (size 2 1.05) (layers F.Cu F.Mask))
  (pad 6 thru_hole oval (at 0 3.125) (size 2 1.05) (drill 0.74) (layers *.Cu *.Mask))
)
