(footprint "2P_TH_1.5x2.5_P2" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -1.45 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 00d6e831-3729-4c35-a504-df7c0368c32c)
  )
  (fp_text value "2P_TH_1.5x2.5_P2" (at 0 2.55 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 38f8e0dd-6e47-42a6-b591-f0d36fd918bf)
  )
  (fp_text user "${REFERENCE}" (at 0 -1.45 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 8625d9b7-44ce-4619-af98-ec77972663a0)
  )
  (fp_line (start -2 -0.55) (end -2 1.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 49b11f22-04ef-4d2a-9475-3d20be524737))
  (fp_line (start -1.55 -1) (end 1.4 -1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 7526a839-a5ef-4748-bab5-41bf864fed1e))
  (fp_line (start 1.4 2) (end -1.55 2)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6d156db2-e49e-4fa6-81dc-baa524f9f8f2))
  (fp_line (start 2 -0.4) (end 2 1.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0dafc7d6-4116-4e6d-bd72-1cbe5ea42a7b))
  (fp_arc (start -2 -0.55) (mid -1.868198 -0.868198) (end -1.55 -1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c31ac4fa-b5eb-4f54-a5d5-f7cc35f1a1bc))
  (fp_arc (start -1.55 2) (mid -1.868198 1.868198) (end -2 1.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c39daf46-2400-473e-b431-f45aa165f33d))
  (fp_arc (start 1.4 -1) (mid 1.824264 -0.824264) (end 2 -0.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1469c31f-7871-4bba-81df-3c0098f84acc))
  (fp_arc (start 2 1.4) (mid 1.824264 1.824264) (end 1.4 2)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 52d19e02-a812-4d64-86d4-772f70b27e58))
  (pad "1" thru_hole circle (at -1 0) (size 1.1 1.1) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp a5fc1198-00f9-4520-9024-b0779f871d3c))
  (pad "1" smd roundrect (at -1 0.5) (size 1.5 2.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1333333333) (tstamp 796533eb-2e62-4c31-8a04-e6dda60f9a1f))
  (pad "2" thru_hole circle (at 1 0) (size 1.1 1.1) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp 6bb5ae67-3dee-4edd-a97a-d7c3655d8cc7))
  (pad "2" smd roundrect (at 1 0.5) (size 1.5 2.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2666666667) (tstamp c61ccb5d-dc51-4bd5-a086-d7603a6b9420))
)
