(footprint "DF40HC(3.5)-100DS-0.4V(51)" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Sheetfile" "RK3588_Camcorder_Carrier.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "DF40HC-3D0-100DS-0D4V-51")
  (property "ki_keywords" "connector")
  (attr smd)
  (fp_text reference "J2" (at -12.3 0 90 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp af1beda2-be18-48dc-89ae-5e930e8ec4d8)
  )
  (fp_text value "DF40HC(3.5)-100DS-0.4V(51)" (at 0 0.65 unlocked) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
    (tstamp d38ab1bf-d60d-412f-b3c9-2923fae1e2bc)
  )
  (fp_text user "${REFERENCE}" (at 0 -0.75 unlocked) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.125)))
    (tstamp 5cdc824a-44ec-4759-bac1-08460dc953e4)
  )
  (fp_arc (start -11.475 -1.575) (mid -11.453033 -1.628033) (end -11.4 -1.65)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 0716a0a9-5e46-433a-99d5-a0a5e32009f8))
  (fp_arc (start -11.4 1.65) (mid -11.453033 1.628033) (end -11.475 1.575)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp ac2fe3be-beb8-4166-85e2-c95434213bc8))
  (fp_arc (start 11.4 -1.65) (mid 11.453033 -1.628033) (end 11.475 -1.575)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 551b329c-d39f-470e-bfd1-60cd7153f949))
  (fp_arc (start 11.475 1.575) (mid 11.453033 1.628033) (end 11.4 1.65)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 48a2b3de-a618-44e4-a9c2-e9e8a98c13bd))
  (fp_poly
    (pts
      (xy -9.65 -2.25)
      (xy -9.95 -2.25)
      (xy -9.8 -2)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 0712f05d-42e8-4506-ac6a-0b4c1470ca9e))
  (fp_poly
    (pts
      (xy -10.3 1.575)
      (xy -11.4 1.575)
      (xy -11.4 -1.575)
      (xy -10.3 -1.575)
      (xy -10.3 -1.725)
      (xy -11.4 -1.725)
      (xy -11.55 -1.575)
      (xy -11.55 1.575)
      (xy -11.4 1.725)
      (xy -10.3 1.725)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 9c289848-d20a-49b3-b996-17fc0dc99410))
  (fp_poly
    (pts
      (xy 10.3 -1.575)
      (xy 11.4 -1.575)
      (xy 11.4 1.575)
      (xy 10.3 1.575)
      (xy 10.3 1.725)
      (xy 11.4 1.725)
      (xy 11.55 1.575)
      (xy 11.55 -1.575)
      (xy 11.4 -1.725)
      (xy 10.3 -1.725)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 0136ad08-4d62-4d14-9603-206829534802))
  (fp_rect (start -9.9 -0.46) (end -9.7 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 69f9cc2c-f0d5-4fe5-b14a-77be7f30d1e1))
  (fp_rect (start -9.9 1.19) (end -9.7 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 2e413f12-5fc9-42d0-beab-bd98880ca473))
  (fp_rect (start -9.5 -0.46) (end -9.3 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 75965088-2f67-48e9-aef4-c1e6e59aaa54))
  (fp_rect (start -9.5 1.19) (end -9.3 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 38cadac4-8144-4069-a2f4-2ba4eaf54732))
  (fp_rect (start -9.1 -0.46) (end -8.9 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 3cceabf8-e230-4ef9-9b32-a4d277cb7c6c))
  (fp_rect (start -9.1 1.19) (end -8.9 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp b3d56424-5f84-4b5b-9290-82c127baf912))
  (fp_rect (start -8.7 -0.46) (end -8.5 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 3f535bd8-9ac2-4fda-8790-f4ace5c552c3))
  (fp_rect (start -8.7 1.19) (end -8.5 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 2d1e3100-6b00-4bc8-b1b2-6e6c2c3de115))
  (fp_rect (start -8.3 -0.46) (end -8.1 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp c900b302-4b72-4904-bffe-6971e1d26e17))
  (fp_rect (start -8.3 1.19) (end -8.1 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 033ee30f-3551-49de-91af-4a8fc1bebbd4))
  (fp_rect (start -7.9 -0.46) (end -7.7 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 2dc94a12-b798-4802-873e-dd3d42ba1f33))
  (fp_rect (start -7.9 1.19) (end -7.7 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp e7ac9252-6c58-465f-90d4-ff12137787a7))
  (fp_rect (start -7.5 -0.46) (end -7.3 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 5671cb0b-7d3d-4a48-855a-65a14df58501))
  (fp_rect (start -7.5 1.19) (end -7.3 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp a908b4cc-ba33-4d6d-bb3f-adb0f813f624))
  (fp_rect (start -7.1 -0.46) (end -6.9 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp a39a9585-cb15-4a91-9382-66981bf189e5))
  (fp_rect (start -7.1 1.19) (end -6.9 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 76df6856-ef6c-4b09-ae2e-93c2306c35aa))
  (fp_rect (start -6.7 -0.46) (end -6.5 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 71249a3a-461e-4b9b-99a1-725ceb8cba28))
  (fp_rect (start -6.7 1.19) (end -6.5 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 7295f3bf-729f-4ac4-8be8-832a1c51d4e3))
  (fp_rect (start -6.3 -0.46) (end -6.1 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 4b987af6-58d8-4070-8c42-2355ff6db52e))
  (fp_rect (start -6.3 1.19) (end -6.1 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 9d4c37c0-d4bd-4536-a253-b7ccb9a6e058))
  (fp_rect (start -5.9 -0.46) (end -5.7 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 6c4052e7-e370-48ff-815a-e7e769258416))
  (fp_rect (start -5.9 1.19) (end -5.7 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 423b0bed-2254-43c6-9ef2-7e20d6353281))
  (fp_rect (start -5.5 -0.46) (end -5.3 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 79ff36a3-700d-47dc-b4e0-eafd37bcae6d))
  (fp_rect (start -5.5 1.19) (end -5.3 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 53817c0c-3511-4dbf-9659-1f0960afb54a))
  (fp_rect (start -5.1 -0.46) (end -4.9 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 3f5cd0a6-f2c9-4648-925b-5b0a391584ce))
  (fp_rect (start -5.1 1.19) (end -4.9 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 78d4b63d-102f-4846-bb9f-ff9cfb7668ef))
  (fp_rect (start -4.7 -0.46) (end -4.5 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 22249848-cf34-44c2-a9ae-001504e4a5b4))
  (fp_rect (start -4.7 1.19) (end -4.5 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp b43aac09-7a41-4b37-af7e-27aa17a528d0))
  (fp_rect (start -4.3 -0.46) (end -4.1 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 0d6eaec7-ea04-4d62-bbf0-cb7734a8b92e))
  (fp_rect (start -4.3 1.19) (end -4.1 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 8facd7f3-9ef4-4456-ba8b-b52b5e992679))
  (fp_rect (start -3.9 -0.46) (end -3.7 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 84d77277-eb99-4b12-b746-34df8b2c0d03))
  (fp_rect (start -3.9 1.19) (end -3.7 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp e81e26af-5985-428c-ab6c-f4e36438fb93))
  (fp_rect (start -3.5 -0.46) (end -3.3 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 56146a5b-dc91-4d56-9844-30d55906d206))
  (fp_rect (start -3.5 1.19) (end -3.3 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 3c5c1662-5538-4dcd-9457-27d918f5b138))
  (fp_rect (start -3.1 -0.46) (end -2.9 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 818368ad-e978-4506-97a3-5eff13c8af35))
  (fp_rect (start -3.1 1.19) (end -2.9 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 147e785d-efa2-4bb6-a881-3d75b09e22b0))
  (fp_rect (start -2.7 -0.46) (end -2.5 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 638ad781-4033-4b76-b550-f7830cd55417))
  (fp_rect (start -2.7 1.19) (end -2.5 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp cce4bd51-6bf7-4c3a-8e25-253a562fd062))
  (fp_rect (start -2.3 -0.46) (end -2.1 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 90b57161-d5d2-41b4-b2b2-193cb6a29765))
  (fp_rect (start -2.3 1.19) (end -2.1 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 59c675fc-6556-4779-8e53-8a01b5db0347))
  (fp_rect (start -1.9 -0.46) (end -1.7 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 83fd318c-6e22-4fac-87f3-e61d9bd6ea5f))
  (fp_rect (start -1.9 1.19) (end -1.7 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 83c6fc26-11b2-4621-ba2f-65bb21d0bac3))
  (fp_rect (start -1.5 -0.46) (end -1.3 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp ba7e55ac-6e84-47d3-be07-d046174000d6))
  (fp_rect (start -1.5 1.19) (end -1.3 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 85a506ad-eba6-476b-a694-bb45553c9142))
  (fp_rect (start -1.1 -0.46) (end -0.9 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 663cd8a7-fc91-4392-ac92-db606c84e5be))
  (fp_rect (start -1.1 1.19) (end -0.9 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 062b4af8-6834-4225-bdd5-c564b40ae7fa))
  (fp_rect (start -0.7 -0.46) (end -0.5 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 25b57c2f-725b-42a1-be8d-362e192e1c9b))
  (fp_rect (start -0.7 1.19) (end -0.5 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 679769bb-4b01-4adc-95be-d00a2b8a191f))
  (fp_rect (start -0.3 -0.46) (end -0.1 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 8be0e096-c83d-4619-b83a-b9f1f95e45b0))
  (fp_rect (start -0.3 1.19) (end -0.1 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 52895244-7d80-4f3e-8826-d84a7461bb6e))
  (fp_rect (start 0.1 -0.46) (end 0.3 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp cd7ec84a-71f2-45ba-bb68-8eea6637f470))
  (fp_rect (start 0.1 1.19) (end 0.3 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 51ee6e66-034d-4c4b-bedc-c6c885666bd6))
  (fp_rect (start 0.5 -0.46) (end 0.7 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 8111c203-3d2b-466f-b2e6-1b32cf89e897))
  (fp_rect (start 0.5 1.19) (end 0.7 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp aa9403df-f29c-4224-b7e7-cded7137685e))
  (fp_rect (start 0.9 -0.46) (end 1.1 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 8143dabb-b560-43f3-a78c-81cf673a368d))
  (fp_rect (start 0.9 1.19) (end 1.1 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp e052ce5f-e09a-46a1-a566-0136955fc2c4))
  (fp_rect (start 1.3 -0.46) (end 1.5 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 15229a29-dbca-4dc1-a6e4-caaa45dae26f))
  (fp_rect (start 1.3 1.19) (end 1.5 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 175fa2c9-f568-4579-9f8b-37b8f697081c))
  (fp_rect (start 1.7 -0.46) (end 1.9 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 5febdbcd-ad0a-445c-88e1-929cf1ef2950))
  (fp_rect (start 1.7 1.19) (end 1.9 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp daaab9f6-f318-4cd5-a505-f74405e19d2b))
  (fp_rect (start 2.1 -0.46) (end 2.3 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 660e24d4-7b9e-4b44-9877-7150aa9ad3db))
  (fp_rect (start 2.1 1.19) (end 2.3 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 6c94bf0a-c00a-4c60-aa1f-6f464326035c))
  (fp_rect (start 2.5 -0.46) (end 2.7 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 69dc2ed6-1bc5-4404-ace7-0d396fc483b7))
  (fp_rect (start 2.5 1.19) (end 2.7 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 5c6eecee-ac58-46e7-ad91-ad9e824f2233))
  (fp_rect (start 2.9 -0.46) (end 3.1 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp b679fbe8-c7e1-4e15-9cc3-1d64e490050e))
  (fp_rect (start 2.9 1.19) (end 3.1 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 8795934e-7f77-4dd6-9727-a2a16b1542bc))
  (fp_rect (start 3.3 -0.46) (end 3.5 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 60f8f1f0-b6da-474d-b147-9d099de7a0ce))
  (fp_rect (start 3.3 1.19) (end 3.5 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp f477adb1-75df-49e8-b943-bf432f54720d))
  (fp_rect (start 3.7 -0.46) (end 3.9 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 38a73603-e30c-4610-894e-744f7b521a3f))
  (fp_rect (start 3.7 1.19) (end 3.9 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 006765d2-3019-4753-afbb-0061a0e4baef))
  (fp_rect (start 4.1 -0.46) (end 4.3 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 4a38d28c-795f-4645-a510-b8f2839020f7))
  (fp_rect (start 4.1 1.19) (end 4.3 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp d544d390-c6dc-4100-8d27-6abefbf5d941))
  (fp_rect (start 4.5 -0.46) (end 4.7 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp f0dabef3-8639-496c-a26d-82df418372f2))
  (fp_rect (start 4.5 1.19) (end 4.7 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 357b2d08-58f8-4f56-b29b-d664a4aa69da))
  (fp_rect (start 4.9 -0.46) (end 5.1 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 0912f00d-3a1c-4b19-a3cf-2afd9cd90a10))
  (fp_rect (start 4.9 1.19) (end 5.1 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 51e3b40a-0446-4e21-8e8d-8fbe6076a509))
  (fp_rect (start 5.3 -0.46) (end 5.5 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 22ac1a98-6e1e-4a4b-af41-60bdb7deef7b))
  (fp_rect (start 5.3 1.19) (end 5.5 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp aa77d242-74eb-429a-adea-11eb684f76a8))
  (fp_rect (start 5.7 -0.46) (end 5.9 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 88c29881-9c00-49df-9117-80f62d69ec80))
  (fp_rect (start 5.7 1.19) (end 5.9 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 3c50d1aa-8475-4972-b83f-40347ba3e587))
  (fp_rect (start 6.1 -0.46) (end 6.3 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 7f3f4b35-42bc-4846-93a1-ec1258bfda29))
  (fp_rect (start 6.1 1.19) (end 6.3 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp c6ca6d66-68bd-4288-b612-bb854f7c8f97))
  (fp_rect (start 6.5 -0.46) (end 6.7 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 5ea08d5d-2e5a-4b72-8372-6d8291d28767))
  (fp_rect (start 6.5 1.19) (end 6.7 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp ef7e62e2-bb94-447c-9bba-095d298ad396))
  (fp_rect (start 6.9 -0.46) (end 7.1 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 894cf45b-26b7-4a65-baa1-161c3915d970))
  (fp_rect (start 6.9 1.19) (end 7.1 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 5c52994e-717e-479e-a655-1ce1dc5b7c1b))
  (fp_rect (start 7.3 -0.46) (end 7.5 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 8881c477-554c-4743-8daa-077a639cc43b))
  (fp_rect (start 7.3 1.19) (end 7.5 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 02a2fd3e-f23b-452d-b9bb-9b0323dfbd29))
  (fp_rect (start 7.7 -0.46) (end 7.9 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 3deb3260-f680-48c9-9b9d-e447229ae36e))
  (fp_rect (start 7.7 1.19) (end 7.9 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 641f5f80-b0fc-4882-b52f-7d4b3133a216))
  (fp_rect (start 8.1 -0.46) (end 8.3 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp f820fbed-f1ec-453a-94dc-0ddfc9445b74))
  (fp_rect (start 8.1 1.19) (end 8.3 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp a2f3f32d-e6ab-4471-a29c-15daad9936df))
  (fp_rect (start 8.5 -0.46) (end 8.7 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp be52582b-bdab-429c-b1ff-5f8668e09fc6))
  (fp_rect (start 8.5 1.19) (end 8.7 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 6e79b93b-aa07-4381-a71d-d4a7c05e0aa2))
  (fp_rect (start 8.9 -0.46) (end 9.1 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 546ed8cc-850e-4ef7-8d6f-e5ab497540fe))
  (fp_rect (start 8.9 1.19) (end 9.1 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp f75bab2e-aff5-479d-9120-681c008b6cf5))
  (fp_rect (start 9.3 -0.46) (end 9.5 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 57b001a6-92c9-4b05-9b5c-14fc1b535761))
  (fp_rect (start 9.3 1.19) (end 9.5 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp b7b49506-5226-4e3e-8dab-fbaa319cb2a7))
  (fp_rect (start 9.7 -0.46) (end 9.9 -1.19)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 45324df0-2ee1-4373-8242-8d79419ac16e))
  (fp_rect (start 9.7 1.19) (end 9.9 0.46)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 4fcd09e2-723f-4a80-8f75-1af48f74f4c5))
  (fp_line (start -11.55 -1.45) (end -11.55 1.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d18e33c1-b15d-40c0-9244-4db37d540374))
  (fp_line (start -11.3 -1.7) (end -10.05 -1.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4bd28724-dabd-47de-922f-eb65519c6c7b))
  (fp_line (start -11.3 1.7) (end -10.05 1.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 61da2211-fb94-4c7d-b30d-2622a6b63420))
  (fp_line (start -10.05 -1.7) (end -10.05 -1.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 8ee34f5b-a747-4df8-83b9-978daef5bca0))
  (fp_line (start -10.05 1.7) (end -10.05 1.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 150b623a-6010-4c83-b4d9-dcf27f49b2c4))
  (fp_line (start -9.9 2.05) (end 9.9 2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 7ba59d56-e116-47d9-a18a-a1fda0758f7f))
  (fp_line (start 9.9 -2.05) (end -9.9 -2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c57c253e-176b-4d6e-a27a-f27671a913a8))
  (fp_line (start 10.05 -1.7) (end 10.05 -1.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0559f624-437a-4fa0-9db6-b80d7cc0614c))
  (fp_line (start 10.05 1.7) (end 10.05 1.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 862d04c9-5f3a-4a5b-9a1c-080459721590))
  (fp_line (start 11.3 -1.7) (end 10.05 -1.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp cd5062fa-531a-4e63-94d1-f38ab0cdef5a))
  (fp_line (start 11.3 1.7) (end 10.05 1.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d0ad9fea-5ee5-49b4-bcd7-356bc01a2ce2))
  (fp_line (start 11.55 1.45) (end 11.55 -1.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 431ef1da-8a6b-40c1-b5a5-c0681b1c742e))
  (fp_arc (start -11.55 -1.45) (mid -11.476777 -1.626777) (end -11.3 -1.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 604ffa8f-3b4e-444b-812d-501c750da07b))
  (fp_arc (start -11.3 1.7) (mid -11.476777 1.626777) (end -11.55 1.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c64ea258-c376-431c-9ddc-7d116efbc79a))
  (fp_arc (start -10.05 -1.9) (mid -10.006066 -2.006066) (end -9.9 -2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f8cd53a9-a397-4ee2-aba6-32df848e6d45))
  (fp_arc (start -9.9 2.05) (mid -10.006066 2.006066) (end -10.05 1.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4536eaa6-bb29-46a2-b5c8-bc3580716f15))
  (fp_arc (start 9.9 -2.05) (mid 10.006066 -2.006066) (end 10.05 -1.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 25ab2524-5ffa-4cca-9913-3334f9c065c2))
  (fp_arc (start 10.05 1.9) (mid 10.006066 2.006066) (end 9.9 2.05)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 80ca3b48-73b9-48e0-9a1f-9b300003a5bb))
  (fp_arc (start 11.3 -1.7) (mid 11.476777 -1.626777) (end 11.55 -1.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6d8ebb89-17c2-432e-a03b-835e84e98bf9))
  (fp_arc (start 11.55 1.45) (mid 11.476777 1.626777) (end 11.3 1.7)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c4ff8556-6442-4117-abb5-d425c7438d7c))
  (fp_rect (start -11.3 1.47) (end 11.3 -1.47)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 830b1299-f9dc-48bb-9500-57b2575e8296))
  (pad "" smd oval (at -9.8 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 15cecd09-d8b4-462f-9436-80de53eeb325))
  (pad "" smd oval (at -9.8 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 822403d8-2ac8-4830-9b59-f9cb74965072))
  (pad "" smd oval (at -9.4 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp f83f18f1-f430-46b3-a446-246dc120e1b7))
  (pad "" smd oval (at -9.4 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 3761f46f-f1be-4286-a564-15d00269dd10))
  (pad "" smd oval (at -9 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 93a944ce-bf47-47a9-9c8c-2de1f1a323f7))
  (pad "" smd oval (at -9 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 01116b88-fa8e-449e-bd24-26a814f8e867))
  (pad "" smd oval (at -8.6 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp b5229df5-4c62-48b0-a7c3-c5d35705e4b9))
  (pad "" smd oval (at -8.6 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp d4a041da-755f-4af9-b17b-ca4dac6917b9))
  (pad "" smd oval (at -8.2 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 71ecf003-19db-49ca-a59b-2e8c866abeb2))
  (pad "" smd oval (at -8.2 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp d243c630-efeb-44df-9068-16b0fa38f521))
  (pad "" smd oval (at -7.8 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp e612e3c6-06af-4047-bbb2-101b29c96e3f))
  (pad "" smd oval (at -7.8 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 63b7e6ef-dcee-466d-b9b6-220326b73c35))
  (pad "" smd oval (at -7.4 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 8cce5f93-28f2-4859-a3b1-d13dcf980260))
  (pad "" smd oval (at -7.4 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp b92200b7-441f-4ad6-ba86-a889c25a8231))
  (pad "" smd oval (at -7 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 1bb9e302-0baa-4e0d-9692-8cfb24bff89d))
  (pad "" smd oval (at -7 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 127e119c-5df1-4cb5-8eb1-6109563bd996))
  (pad "" smd oval (at -6.6 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp ad8206b9-de71-4bbc-bb3a-4def3875e751))
  (pad "" smd oval (at -6.6 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 39840e6c-fbe4-483c-8d04-4919958db5fa))
  (pad "" smd oval (at -6.2 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 031a060e-25bf-4063-aa98-47e4cc829b00))
  (pad "" smd oval (at -6.2 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp f0338875-f7a3-4a34-9434-9960f26c34d2))
  (pad "" smd oval (at -5.8 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 7baedcad-f17e-40f9-b48b-dc4b2da651e3))
  (pad "" smd oval (at -5.8 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 263d1f34-930a-48f5-9da8-99df4dd3285d))
  (pad "" smd oval (at -5.4 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 7ea30fb4-62e1-41a9-8428-dc91850f03d7))
  (pad "" smd oval (at -5.4 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp d20378fd-9f70-46aa-93d1-e0a36fd81456))
  (pad "" smd oval (at -5 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp e4b88658-fc8b-476c-9794-fb7fdd8f52b3))
  (pad "" smd oval (at -5 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 1e446c14-4d76-4e3e-8d94-e8d829c4e4e9))
  (pad "" smd oval (at -4.6 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 51d57b2f-f65c-422e-86e8-591479de60f9))
  (pad "" smd oval (at -4.6 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp a287b4c4-ea06-4c3f-8261-ed8d6646d220))
  (pad "" smd oval (at -4.2 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp bc6bb4b6-9b2c-45d7-8138-0b88deb3a9f2))
  (pad "" smd oval (at -4.2 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 676a54cd-566f-43a4-9fa3-741ef89407f8))
  (pad "" smd oval (at -3.8 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp cd1ffcc2-a4e4-4f5a-a770-9e8373420003))
  (pad "" smd oval (at -3.8 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp f7efff05-0505-483e-9637-f8e8854659c5))
  (pad "" smd oval (at -3.4 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 0b8d47fa-a420-4969-8367-ca2d4a26bea5))
  (pad "" smd oval (at -3.4 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp f53de902-54bb-4730-a5de-958b8146bb36))
  (pad "" smd oval (at -3 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 90aa94d7-8c59-4c32-bb8a-6aee3d484c0c))
  (pad "" smd oval (at -3 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 90c3bf7e-0508-4e5e-910a-03db9ad77424))
  (pad "" smd oval (at -2.6 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 3597d4ec-ba8a-4a15-9c13-a6f2bd2e1b2a))
  (pad "" smd oval (at -2.6 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 501787de-45a4-492f-9ddd-0a07b16041dd))
  (pad "" smd oval (at -2.2 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp eded50bd-b078-403f-8e3b-5c0a3dbcb621))
  (pad "" smd oval (at -2.2 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 4c642cbc-e056-4a61-9934-0003f0431c10))
  (pad "" smd oval (at -1.8 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 664ad2af-4134-46fa-92d7-0be3eb57bb6f))
  (pad "" smd oval (at -1.8 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp b3cb3da0-5baf-4366-99b4-8c27ba1d877a))
  (pad "" smd oval (at -1.4 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 3d4feec3-c246-4fec-9133-374705b7fa9f))
  (pad "" smd oval (at -1.4 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp a2b15aaf-e732-4053-a1dd-81800fce02a4))
  (pad "" smd oval (at -1 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 97abc32f-6cf3-4e9c-9066-49edf1d1647b))
  (pad "" smd oval (at -1 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 1c9d0076-d260-4cd8-ba07-0259a6fdf4ac))
  (pad "" smd oval (at -0.6 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp af279820-2dcc-403a-971d-2af57cee2510))
  (pad "" smd oval (at -0.6 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp b6c43910-1e0c-452f-afb6-f4b0ea4cfbe5))
  (pad "" smd oval (at -0.2 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 07104296-203b-47a2-9ca5-9f0c41dc3a1e))
  (pad "" smd oval (at -0.2 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp aa2bd532-86ce-46af-8189-036e18a3912a))
  (pad "" smd oval (at 0.2 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 103b5719-5b4e-4476-a0e7-cdd19157bb1c))
  (pad "" smd oval (at 0.2 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 195066e1-69c3-4d6c-b2db-968942e7f190))
  (pad "" smd oval (at 0.6 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp d131cad6-f149-4897-8e2f-87a1459fcadd))
  (pad "" smd oval (at 0.6 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 57a235a8-fb40-4281-a22e-2b181f80748a))
  (pad "" smd oval (at 1 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 95ebc2bc-6050-4aa3-928a-e7093468231a))
  (pad "" smd oval (at 1 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 3e144604-61f8-419c-a164-e68b5cff984a))
  (pad "" smd oval (at 1.4 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 5c646749-93fd-4c77-8f8a-42eb4cc10b52))
  (pad "" smd oval (at 1.4 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp c5428c7a-d11d-4ed6-9dec-ec0aac32fab6))
  (pad "" smd oval (at 1.8 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 9f6906d8-cce1-48ad-b4ef-c7ebb6327316))
  (pad "" smd oval (at 1.8 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp f032c5ae-1ea9-4a04-92c8-2846b26fa0d4))
  (pad "" smd oval (at 2.2 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 1bbf744f-54b9-4c1f-bb47-99e84005e891))
  (pad "" smd oval (at 2.2 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp a2213bbf-ccf3-40d8-aaca-b6d36428c390))
  (pad "" smd oval (at 2.6 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 604604d0-a5fd-4940-9c2a-e668c6aedd72))
  (pad "" smd oval (at 2.6 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp b7ccebd1-339e-4711-9960-cab708c2e948))
  (pad "" smd oval (at 3 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 87fb2fed-b9a0-4d5e-825e-09332180d13d))
  (pad "" smd oval (at 3 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp a61f97e6-fae2-43a0-be26-ee131b0656a1))
  (pad "" smd oval (at 3.4 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 6cc2db20-3213-488a-941f-b727d98704db))
  (pad "" smd oval (at 3.4 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 427ab915-0839-4b4d-b821-75e6197628f9))
  (pad "" smd oval (at 3.8 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp d8511fb6-f46d-4b91-8453-d14a1e0998ea))
  (pad "" smd oval (at 3.8 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 7d5ebd8d-977f-4d70-990a-615749fb4bf0))
  (pad "" smd oval (at 4.2 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 27dee819-0d0a-47fd-b0f6-9552f533b008))
  (pad "" smd oval (at 4.2 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 95291639-9b2b-423d-ae77-bad6fa05c906))
  (pad "" smd oval (at 4.6 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp b54a0834-7a54-4116-bbf9-af99d94c7ae6))
  (pad "" smd oval (at 4.6 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp cf91a248-1830-44b8-9b10-7a595a52058d))
  (pad "" smd oval (at 5 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 3df76fde-363c-495e-8f42-615aca30c381))
  (pad "" smd oval (at 5 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 5d43f324-ced3-4c67-85d3-80c1579c9f6a))
  (pad "" smd oval (at 5.4 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp eb6c0d9d-0dcb-48bc-a59c-3172adfcedd0))
  (pad "" smd oval (at 5.4 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 02bc0890-5411-4850-a19f-f21f569fec50))
  (pad "" smd oval (at 5.8 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 5223ef97-9ad1-4713-85d8-c21f05d66994))
  (pad "" smd oval (at 5.8 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp fc34e273-20c0-453a-8d06-777932e6a94f))
  (pad "" smd oval (at 6.2 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 7332eff3-a98d-4ee8-a37c-af0898652804))
  (pad "" smd oval (at 6.2 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 0ed443e9-d1c1-4287-b4f5-364433c6da0e))
  (pad "" smd oval (at 6.6 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 0994e4c8-6691-4570-8d3c-933fdbb52654))
  (pad "" smd oval (at 6.6 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp ca6b1913-d3cb-4bdb-9376-38445dcb25f9))
  (pad "" smd oval (at 7 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 552c9aef-7453-4a81-9ce2-7c40e7094241))
  (pad "" smd oval (at 7 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp fe9a9c83-3210-47bf-97e7-83a98dc1b66f))
  (pad "" smd oval (at 7.4 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 4bba7589-6022-4ff0-8e4d-f911c447720e))
  (pad "" smd oval (at 7.4 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp e2ddde77-1fb4-4d0c-ae57-2d24927e97fd))
  (pad "" smd oval (at 7.8 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp cded0447-0b5d-4f7e-9523-ca5668547d61))
  (pad "" smd oval (at 7.8 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 41363a4f-33d4-450f-a058-cd21c30b49a1))
  (pad "" smd oval (at 8.2 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp cdc6a09f-99dd-405e-a634-635de683a71e))
  (pad "" smd oval (at 8.2 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp ecab4e24-1928-4f96-a36a-930e9067ae74))
  (pad "" smd oval (at 8.6 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 349255e4-60a6-4752-93e4-654f6d318d15))
  (pad "" smd oval (at 8.6 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 5925acc6-d253-421b-bf9a-688fbf3ef380))
  (pad "" smd oval (at 9 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 9398a684-fa41-4257-87cf-299c21d3ba6a))
  (pad "" smd oval (at 9 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp b150e502-2317-4139-8587-eb2b090a0146))
  (pad "" smd oval (at 9.4 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 6b7d1f0b-ff97-46f4-9660-e232b7ba46aa))
  (pad "" smd oval (at 9.4 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp a1be3406-4abd-473d-8fc1-85607bad14f4))
  (pad "" smd oval (at 9.8 -1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 96ba312c-c325-4a55-9cb9-03172a511af1))
  (pad "" smd oval (at 9.8 1.6) (size 0.2 0.5) (layers "F.Paste")
    (thermal_bridge_angle 45) (tstamp 7959be5b-e502-4806-9e86-095dc19c3063))
  (pad "1" smd roundrect (at -9.8 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp d995bd87-ca49-4bed-88b5-3f2ede05298f))
  (pad "2" smd roundrect (at -9.8 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 03ede6ce-93d0-47bc-af16-9a42b53a45aa))
  (pad "3" smd roundrect (at -9.4 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 8729b20b-80e2-46de-934a-06554f6ddfe5))
  (pad "4" smd roundrect (at -9.4 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp dec342b9-7438-42bc-8300-7f698b097826))
  (pad "5" smd roundrect (at -9 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 35149eb6-b75c-4e63-880c-2ad448d71f2c))
  (pad "6" smd roundrect (at -9 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 39ef965c-b0a0-465c-bfef-96b581987ce3))
  (pad "7" smd roundrect (at -8.6 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp bd1eab29-4f43-4ae8-83eb-00929f92002a))
  (pad "8" smd roundrect (at -8.6 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 4c945f0d-6a50-4070-a413-201ca7468d0e))
  (pad "9" smd roundrect (at -8.2 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 956af7f5-bf2b-4d9b-82f7-c84f5fa7c3dd))
  (pad "10" smd roundrect (at -8.2 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 127705fb-c25d-4a2f-a6c1-f5cd34cf423d))
  (pad "11" smd roundrect (at -7.8 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp bc2fe6af-417d-450b-98e0-e7a2c79879f1))
  (pad "12" smd roundrect (at -7.8 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 7e993314-a00b-4823-af42-360408c34925))
  (pad "13" smd roundrect (at -7.4 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 9b0ce802-63a7-4d3f-a327-1c8f5c4b3edc))
  (pad "14" smd roundrect (at -7.4 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 6bd94fff-1205-4788-ae16-2e41a9bcbdba))
  (pad "15" smd roundrect (at -7 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 23b00d32-f284-4bcd-aa2f-bc2ff2ef8a74))
  (pad "16" smd roundrect (at -7 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp d2bdbec7-08df-458d-b02c-926876e96c89))
  (pad "17" smd roundrect (at -6.6 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp d3e3ff19-e5a6-4186-9ff3-35c887de8806))
  (pad "18" smd roundrect (at -6.6 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 6ec8010f-2e91-4a40-8906-4f2442b521ca))
  (pad "19" smd roundrect (at -6.2 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp f1ae2b94-dcee-4120-a9e0-d4d1fdbce079))
  (pad "20" smd roundrect (at -6.2 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp e1027029-5727-4c8b-9b52-5612e74e8d49))
  (pad "21" smd roundrect (at -5.8 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 4d70e7bc-1462-4a26-a1fa-8395cefded9b))
  (pad "22" smd roundrect (at -5.8 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 4a8d0210-72e2-4cd5-b285-0520b94c80d9))
  (pad "23" smd roundrect (at -5.4 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 70b45d9c-be17-46f3-817b-dbea4da246dd))
  (pad "24" smd roundrect (at -5.4 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 67c6a6f3-b149-4fdf-ab43-a6ff8f7a69ec))
  (pad "25" smd roundrect (at -5 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp f421d5d3-d736-4a40-975e-1b8c49b7564d))
  (pad "26" smd roundrect (at -5 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp d1c351bd-24f9-434f-b22f-81d0cf36226f))
  (pad "27" smd roundrect (at -4.6 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 64d6fa8d-29f4-4b55-980b-b9d11603254d))
  (pad "28" smd roundrect (at -4.6 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 789d82d1-fff0-4b89-96d4-f05fffbee855))
  (pad "29" smd roundrect (at -4.2 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp ecd0dd2a-450d-469b-9f8c-9ea742ae2f10))
  (pad "30" smd roundrect (at -4.2 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 5d6a5d73-5f1c-448f-86b6-09772d0980f2))
  (pad "31" smd roundrect (at -3.8 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp f47cf855-e5f2-4b1e-8f34-7fce28490304))
  (pad "32" smd roundrect (at -3.8 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp f3f2121d-68e8-46ed-8694-ab77c827cbfc))
  (pad "33" smd roundrect (at -3.4 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp b2a13d4a-32ab-44a4-be7d-84aee5ff187d))
  (pad "34" smd roundrect (at -3.4 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 9751f9fe-54e3-49c6-9f0f-3646e9ece9c8))
  (pad "35" smd roundrect (at -3 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp c7b832af-152c-432d-b96f-058bd2b3222d))
  (pad "36" smd roundrect (at -3 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp caa7b6fa-9987-4389-87d9-e7cfad3fe609))
  (pad "37" smd roundrect (at -2.6 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp f0314fb2-497a-4f4f-838e-ef546f043449))
  (pad "38" smd roundrect (at -2.6 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp ea86beb4-37f1-45a7-8a4d-159a739b7fea))
  (pad "39" smd roundrect (at -2.2 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 220a1878-e732-41d4-8938-bf1171615db4))
  (pad "40" smd roundrect (at -2.2 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 18792f42-3016-4eb6-8056-b66dcc5496ec))
  (pad "41" smd roundrect (at -1.8 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp a725e79c-b716-482b-a372-5da7d6d4a89c))
  (pad "42" smd roundrect (at -1.8 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 1e1b517e-12bf-463f-9e43-6cd8c2195725))
  (pad "43" smd roundrect (at -1.4 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp a22279df-cc6b-4691-ae7f-8e2b9cf85ef7))
  (pad "44" smd roundrect (at -1.4 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp c2d96480-53fd-4c11-a873-29e9753ac8b0))
  (pad "45" smd roundrect (at -1 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 7a6e85ca-1656-4d4a-83e9-4d90e8fe52b4))
  (pad "46" smd roundrect (at -1 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 0698aa48-bab9-44c8-a7ca-63234e85021e))
  (pad "47" smd roundrect (at -0.6 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 5ceca8d5-e407-4718-abdc-620aac168f6b))
  (pad "48" smd roundrect (at -0.6 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 28a6526f-e89c-408f-8216-3f520ed088c1))
  (pad "49" smd roundrect (at -0.2 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 23967bed-ba84-412c-9161-b56f427e6aea))
  (pad "50" smd roundrect (at -0.2 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 4209ffb5-8071-4431-ac13-b86a81b72cb7))
  (pad "51" smd roundrect (at 0.2 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 4e828c8a-4e56-4702-b82b-daa56552c088))
  (pad "52" smd roundrect (at 0.2 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp d63543e8-a9be-438c-8218-3431337774de))
  (pad "53" smd roundrect (at 0.6 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp a684a84a-308f-42fc-9c88-36e8dd397f9e))
  (pad "54" smd roundrect (at 0.6 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 54623a15-dcd8-4a22-b8ee-6749ba5fb6e4))
  (pad "55" smd roundrect (at 1 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 26c225d8-6b49-4e23-b2be-40f0a3d7731c))
  (pad "56" smd roundrect (at 1 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp e217a020-b802-4494-afec-63472f6928f9))
  (pad "57" smd roundrect (at 1.4 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 808d31f9-aeba-4abe-9db1-f2bb0889c8a4))
  (pad "58" smd roundrect (at 1.4 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 8ed300d5-f901-4c4a-873c-035c0f94649a))
  (pad "59" smd roundrect (at 1.8 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp ac76b790-993b-40a0-89df-5757f5010eda))
  (pad "60" smd roundrect (at 1.8 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp bb0e5877-a1bf-4cc4-a7fe-92a789b5191d))
  (pad "61" smd roundrect (at 2.2 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 90a19483-b0fa-490f-a950-ca650213b292))
  (pad "62" smd roundrect (at 2.2 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp d7d87506-ee71-4d24-aa76-fa4cd55986bf))
  (pad "63" smd roundrect (at 2.6 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp b037dd81-7c2c-4273-b11d-8c19004922ab))
  (pad "64" smd roundrect (at 2.6 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 9b46c1e4-f130-478c-99fd-d46e70d25f95))
  (pad "65" smd roundrect (at 3 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp a33a5fc8-ba6e-4df5-838c-b8f9f4a95da3))
  (pad "66" smd roundrect (at 3 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp a63fa4b9-1d31-47f8-8756-8869e4b9b148))
  (pad "67" smd roundrect (at 3.4 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 59730f87-7eb7-4162-9380-7c9e560f0646))
  (pad "68" smd roundrect (at 3.4 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp ba980392-db65-4acb-928a-30def130bfb1))
  (pad "69" smd roundrect (at 3.8 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 4bf9a52e-de5a-452a-8aa1-a1319c148eb1))
  (pad "70" smd roundrect (at 3.8 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 0f70ea0e-85f9-40c6-9f2d-2e6e1c608d2a))
  (pad "71" smd roundrect (at 4.2 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp e63abd1c-6c14-496c-91e5-5680872742e7))
  (pad "72" smd roundrect (at 4.2 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 6ff01ef4-362b-47a6-b346-3d226abd7875))
  (pad "73" smd roundrect (at 4.6 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 514dd88a-f0d5-4ec4-a939-f38290e6b786))
  (pad "74" smd roundrect (at 4.6 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 75987563-f830-45de-b0f1-f17a8cc6ce51))
  (pad "75" smd roundrect (at 5 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp d8e6abea-408e-4127-a715-ae6b3de7e869))
  (pad "76" smd roundrect (at 5 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 9efc975b-6f8d-4252-a598-de99413d52eb))
  (pad "77" smd roundrect (at 5.4 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 05ffc55f-9a1d-4cab-84cf-703af5246a02))
  (pad "78" smd roundrect (at 5.4 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 00f44735-89f3-4b30-8301-07a20e96a3f8))
  (pad "79" smd roundrect (at 5.8 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 856ed626-e393-4438-8b7e-3fc9f12a3410))
  (pad "80" smd roundrect (at 5.8 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp beee46d0-6b1b-4e56-99fe-9007cfc14278))
  (pad "81" smd roundrect (at 6.2 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 71572b6d-c613-4dbf-8cad-178e56af8ecb))
  (pad "82" smd roundrect (at 6.2 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 6e4ec428-c99d-4815-af4c-40dbdf2c3fd7))
  (pad "83" smd roundrect (at 6.6 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp e803532e-86fb-451c-934a-4736558b139b))
  (pad "84" smd roundrect (at 6.6 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 71d05f32-47e8-4455-9b5a-7fbd3b726655))
  (pad "85" smd roundrect (at 7 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp ba02e6f4-018d-4a57-b618-1fa6cac47213))
  (pad "86" smd roundrect (at 7 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 3612fbc5-78fe-43bc-b1c0-7ec7ac8c5246))
  (pad "87" smd roundrect (at 7.4 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 0230620e-f684-4dd1-ba78-e46b9ba9d235))
  (pad "88" smd roundrect (at 7.4 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 31c7b26f-d228-4bc9-872f-114d60615322))
  (pad "89" smd roundrect (at 7.8 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 90f9713f-e877-47f3-a2cf-019fd1cf5dfe))
  (pad "90" smd roundrect (at 7.8 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 6bdba350-3314-4388-aa4c-2fd4a6cab642))
  (pad "91" smd roundrect (at 8.2 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp fb5e645c-b97c-4f57-a47e-4f0a568ae568))
  (pad "92" smd roundrect (at 8.2 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp c0256446-08fc-4008-8cd3-c09fefe30a2d))
  (pad "93" smd roundrect (at 8.6 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 23b0a9bb-39a9-456f-9a64-8c72e26954e7))
  (pad "94" smd roundrect (at 8.6 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp a06bf0b3-68b5-479b-81a3-68361dc361dd))
  (pad "95" smd roundrect (at 9 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 35a2d749-9fdd-4feb-a1e0-b73bb75dce12))
  (pad "96" smd roundrect (at 9 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 506bf457-adcc-4cbf-bf7f-24222b028735))
  (pad "97" smd roundrect (at 9.4 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 57957487-6e62-4752-88db-1d3acf62f9a5))
  (pad "98" smd roundrect (at 9.4 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 1e1c5fac-6927-444b-9125-eeed9a937729))
  (pad "99" smd roundrect (at 9.8 -1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 08e2d0f6-3862-4617-b40e-f71ae27a1a70))
  (pad "100" smd roundrect (at 9.8 1.54) (size 0.2 0.7) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp 6100ecf9-f826-432c-8af0-f61d52523758))
  (model ":KICAD6_3DMODEL_DIR:Connector_Hirose.3dshapes/DF40HC(3.5)-100DS-0.4V.stp"
    (offset (xyz -0.12 0 1.5))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 90))
  )
)
