(footprint "ToolingHole_JLCPCB_1.152mm" (version 20210722) (generator pcbnew) (layer "F.Cu")
  (tedit 610BD8B4)
  (property "Sheetfile" "StepperDriverModuleCarrier.kicad_sch")
  (property "Sheetname" "")
  (attr exclude_from_pos_files)
  (fp_text reference "FD1" (at 0 0 unlocked) (layer "F.SilkS") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 7833f8ac-cd1e-42f9-9f58-5810110f75de)
  )
  (fp_text value "FIDUCIAL_MARKER" (at 0 0 unlocked) (layer "F.Fab") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e2f6e29b-7e68-43f0-bc2c-2da66b15489d)
  )
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d48d919f-cee2-4aa6-a849-5ae8e1a2b749)
  )
  (pad "" np_thru_hole circle (at 0 0) (size 1.3 1.3) (drill 1.152) (layers *.Mask)
    (solder_mask_margin 0.1) (clearance 0.1) (zone_connect 0) (thermal_gap 0.248) (tstamp 58de9570-a4ba-4d8e-b243-0935a2a8173c))
)
