(module Socket-1_2mm (layer F.Cu) (tedit 584B4306)
  (solder_mask_margin -0.01)
  (fp_text reference J1 (at 0 -1.75) (layer Cmts.User)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value VAL** (at 0 1.75) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_line (start -1 -1) (end 1 -1) (layer F.SilkS) (width 0.125))
  (fp_line (start 1 -1) (end 1 1) (layer F.SilkS) (width 0.125))
  (fp_line (start 1 1) (end -1 1) (layer F.SilkS) (width 0.125))
  (fp_line (start -1 1) (end -1 -1) (layer F.SilkS) (width 0.125))
  (pad 1 thru_hole roundrect (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)(roundrect_rratio 0.25))
  (model Pin_header_socket_1x1_2mm.step
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 90))
  )
)
