(module "USB_C_Plug_XKB_U261-24XN-4BS60" (layer "F.Cu") (tedit 5FA52BA6)
  (attr smd)
  (fp_text reference "REF**" (at 6.45 1.05 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c6c0b4f4-4f2a-48ba-8366-87f5aebd8960)
  )
  (fp_text value "USB-C_Plug_XKB_Connectivity_U261-24XN-4BS60" (at 0 -1.2 unlocked) (layer "F.Fab")
    (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp ad33d667-62a0-4b38-9480-d6c82dc435d4)
  )
  (fp_text user "${REF}" (at 0 -2.35 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a5ed6aef-50d7-4b0c-893b-1d3d40631a1f)
  )
  (fp_line (start 2.75 -0.9) (end 3.05 -0.6) (layer "Dwgs.User") (width 0.1) (tstamp 022643f5-f2df-4588-b9ce-937736fb60ad))
  (fp_line (start -2.75 -0.9) (end 2.75 -0.9) (layer "Dwgs.User") (width 0.1) (tstamp 5ba6dbfa-62d6-4626-b462-3ec0739beea3))
  (fp_line (start 3.05 -0.6) (end 3.05 0) (layer "Dwgs.User") (width 0.1) (tstamp ad99b15d-5109-49c9-b5f4-5209d979ae4d))
  (fp_line (start 3.05 0) (end 3.95 0) (layer "Dwgs.User") (width 0.1) (tstamp b4f6f4b9-ed5a-409f-9bba-125010a5edf6))
  (fp_line (start -2.75 -0.9) (end -3.05 -0.6) (layer "Dwgs.User") (width 0.1) (tstamp bde10155-fb84-4e54-9462-6324e8c26a5a))
  (fp_line (start -3.05 -0.6) (end 3.05 -0.6) (layer "Dwgs.User") (width 0.1) (tstamp ccc675ba-b15e-4707-8030-d02aa06fe7f4))
  (fp_line (start -3.05 0) (end -3.95 0) (layer "Dwgs.User") (width 0.1) (tstamp e2ccd790-77d4-41b3-8966-c18034c4c823))
  (fp_line (start -3.05 -0.6) (end -3.05 0) (layer "Dwgs.User") (width 0.1) (tstamp e8b98976-3cc1-4fe2-b9db-3e58e597fc46))
  (pad "A1" smd roundrect (at -2.75 1.05) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp d8b41f02-bf22-482a-baa8-ca044ad6c99e))
  (pad "A2" smd roundrect (at -2.25 1.05) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 8d0bf527-13cd-448f-b236-fa7b7853236c))
  (pad "A3" smd roundrect (at -1.75 1.05) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 3390c2eb-8755-4c28-b143-bf60714aa98c))
  (pad "A4" smd roundrect (at -1.25 1.05) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 5b69bb25-09be-449d-90c0-8a59d5eb9955))
  (pad "A5" smd roundrect (at -0.75 1.05) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp e4c1fc0f-e837-465b-87b6-87959b4ecad8))
  (pad "A6" smd roundrect (at -0.25 1.05) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 934d582b-d7c7-472d-b0b0-acc8d161d972))
  (pad "A7" smd roundrect (at 0.25 1.05) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 6330fa65-bb5b-4403-ae39-682162090e5d))
  (pad "A8" smd roundrect (at 0.75 1.05) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp ab50fb43-82c2-4b21-a865-be66fd67ae5b))
  (pad "A9" smd roundrect (at 1.25 1.05) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 4a96344a-d622-4406-96e9-37816008c80a))
  (pad "A10" smd roundrect (at 1.75 1.05) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp fa2d0dd5-715f-441c-bc86-bc02991cabb8))
  (pad "A11" smd roundrect (at 2.25 1.05) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 9fa58d91-d792-40c7-91ff-eaa936388691))
  (pad "A12" smd roundrect (at 2.75 1.05) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.167) (tstamp 6660c231-b85d-4a8d-bf0b-4fbfd5b73160))
  (pad "B1" smd roundrect (at 2.75 1.05) (size 0.3 1.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.167) (tstamp 9bcea551-165c-4f6a-b8c5-71c15c01de85))
  (pad "B2" smd roundrect (at 2.25 1.05) (size 0.3 1.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.167) (tstamp cec9f36d-aed4-43db-9fa7-14f21021f664))
  (pad "B3" smd roundrect (at 1.75 1.05) (size 0.3 1.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.167) (tstamp 6ea622bb-0520-4ebf-b8ab-ad9b1e0c5c85))
  (pad "B4" smd roundrect (at 1.25 1.05) (size 0.3 1.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.167) (tstamp da33cf62-ef27-446b-8902-ba903fe6cbac))
  (pad "B5" smd roundrect (at 0.75 1.05) (size 0.3 1.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.167) (tstamp e80e7868-9ff4-4ce6-89a0-a24e6da41d75))
  (pad "B6" smd roundrect (at 0.25 1.05) (size 0.3 1.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.167) (tstamp 6f05c5b8-daaa-4796-b46d-77dce197ae20))
  (pad "B7" smd roundrect (at -0.25 1.05) (size 0.3 1.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.167) (tstamp 871fc785-e4fc-4b6f-b44d-eef5f8069d95))
  (pad "B8" smd roundrect (at -0.75 1.05) (size 0.3 1.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.167) (tstamp cb4d5beb-4baf-4175-9397-b440cc3b4e2b))
  (pad "B9" smd roundrect (at -1.25 1.05) (size 0.3 1.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.167) (tstamp 3342ad4d-590f-41ec-9d09-1144d2cbf58b))
  (pad "B10" smd roundrect (at -1.75 1.05) (size 0.3 1.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.167) (tstamp 82913bbb-eef1-456b-9d01-fa118be5be7f))
  (pad "B11" smd roundrect (at -2.25 1.05) (size 0.3 1.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.167) (tstamp 67968015-49c6-410e-b8c8-f3804f9962ee))
  (pad "B12" smd roundrect (at -2.75 1.05) (size 0.3 1.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.167) (tstamp 9b73b487-e13f-4ee9-8003-64e8e9fce68d))
  (pad "S1" smd roundrect (at -3.6 1.1) (size 0.7 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.143) (tstamp 45157c81-a5c2-4253-b1d1-358b6172abda))
  (pad "S1" smd roundrect (at 3.6 1.1) (size 0.7 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.143) (tstamp cec11061-e9a3-409c-9220-98428be11815))
  (model "${KICAD7_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Plug_XKB_Connectivity_U261-24XN-4BS60.step"
    (offset (xyz 0 0 -0.4))
    (scale (xyz 1 1 1))
    (rotate (xyz 90 0 0))
  )
)
