(footprint "Reomax_R1245"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "F7"
		(at 0 -3 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "605ee9b3-c51c-443e-a6df-e4c95c5258ec")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "80A"
		(at 0 3 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "449ba569-e679-41e8-be8f-9fc99a417a6e")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Fuse:Reomax_R1245"
		(at 0 -14 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "727b7129-fb89-41d2-9492-d325ab25a1f5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 -14 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c443b2a6-7365-42c9-9cbe-6fc06568c37c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 -14 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "93f9589b-8078-4d09-8059-9d59bff1bccf")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "Reomax"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "efc9704c-b5cf-4942-b061-7d3079727657")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "R1245.80"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b9716bb0-e595-4de8-a99a-05d98867ceed")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" "C2762492"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b381eda7-077e-464b-8d57-2fa06ce558d3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Sim.Enable" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b4afc4e0-a191-4527-9099-ab2025f5e4df")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -7.3 2.1)
		(end -7.3 -2.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "4ff63196-a624-4263-abd6-540cd32ee6e7")
	)
	(fp_line
		(start -6 3.4)
		(end 6 3.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "cbd8f5fd-7fa5-443b-b94c-301d6fc0f019")
	)
	(fp_line
		(start 6 -3.4)
		(end -6 -3.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "8baeac63-dafe-410b-9b5b-0d3e16316432")
	)
	(fp_line
		(start 7.3 -2.1)
		(end 7.3 2.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "e8bad75f-6f28-4773-a31e-c5197a938a64")
	)
	(fp_arc
		(start -7.3 -2.1)
		(mid -6.919239 -3.019239)
		(end -6 -3.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "abd6ee2d-e36f-4853-9cd7-fca7792d3fd6")
	)
	(fp_arc
		(start -6 3.4)
		(mid -6.919239 3.019239)
		(end -7.3 2.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "276dacc3-48dc-4c65-ba39-a94aba4448e8")
	)
	(fp_arc
		(start 6 -3.4)
		(mid 6.919239 -3.019239)
		(end 7.3 -2.1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9aa44409-d717-41fa-9b79-bcff6d7503b3")
	)
	(fp_arc
		(start 7.3 2.1)
		(mid 6.919239 3.019239)
		(end 6 3.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "8e4d0581-b4ca-42f0-909f-3747f1ba1773")
	)
	(fp_line
		(start -3.42 2.25)
		(end -3.42 -2.25)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "426f80ae-83c5-4e3d-9335-88c86007d94d")
	)
	(fp_line
		(start 3.42 -2.25)
		(end 3.42 2.25)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "78d67299-25ac-4dc9-9683-a4c51254b604")
	)
	(fp_poly
		(pts
			(xy -6.225 -2.25) (xy -6.225 2.25) (xy 6.225 2.25) (xy 6.225 -2.25)
		)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "0620adf4-0721-49b2-a6ed-97c7754f41e7")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -3 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "bfb777c9-ee32-49f6-b2c3-fbff10ede8a1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -5 0)
		(size 4.28 6.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(thermal_bridge_angle 45)
		(uuid "fcdbda72-872d-40af-a323-41e53a419da2")
	)
	(pad "2" smd roundrect
		(at 5 0)
		(size 4.28 6.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(chamfer_ratio 0.1)
		(chamfer top_left bottom_left)
		(thermal_bridge_angle 45)
		(uuid "44058e40-c136-4081-afa4-7bb4105dd476")
	)
	(model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/FUSE-SMD_L12.5-W4.5.step"
		(offset
			(xyz 0 0 2)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)