(module Tayo_Yuden_NR40xx (layer F.Cu) (tedit 5BDDB435)
  (solder_mask_margin 0.075)
  (solder_paste_margin -0.05)
  (attr smd)
  (fp_text reference L1 (at 0 -2.75) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text value NRG4026T150M (at 0 2.9) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_line (start 1.9 2.4) (end 2.4 2.4) (layer F.SilkS) (width 0.127))
  (fp_line (start 2.4 2.4) (end 2.4 1.8) (layer F.SilkS) (width 0.127))
  (fp_line (start -2.4 2.4) (end -1.9 2.4) (layer F.SilkS) (width 0.127))
  (fp_line (start -2.4 2.4) (end -2.4 1.8) (layer F.SilkS) (width 0.127))
  (fp_line (start 1.9 -2.4) (end 2.4 -2.4) (layer F.SilkS) (width 0.127))
  (fp_line (start 2.4 -2.4) (end 2.4 -1.8) (layer F.SilkS) (width 0.127))
  (fp_line (start -2.4 -2.4) (end -1.9 -2.4) (layer F.SilkS) (width 0.127))
  (fp_line (start -2.4 -2.4) (end -2.4 -1.8) (layer F.SilkS) (width 0.127))
  (fp_line (start 2.5 -2.5) (end 2.5 2.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.5 2.5) (end -2.5 2.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.5 2.5) (end -2.5 -2.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.5 -2.5) (end 2.5 -2.5) (layer F.CrtYd) (width 0.05))
  (pad 1 smd rect (at -1.4 0) (size 1.2 3.7) (layers F.Cu F.Paste F.Mask)
    (zone_connect 2))
  (pad 2 smd rect (at 1.4 0) (size 1.2 3.7) (layers F.Cu F.Paste F.Mask)
    (zone_connect 2))
  (model ${KICAD7_3DMODEL_DIR}/Inductor_SMD.3dshapes/Inductor_SMD_3.0x3.0x1.5.wrl
    (at (xyz 0 0 0))
    (scale (xyz 13.333333 13.333333 13.333333))
    (rotate (xyz 270 0 90))
  )
)
