(module Terminal_Block_6P_5mm_Wurth_691137710006 (layer F.Cu) (tedit 59492915)
  (solder_mask_margin -0.02)
  (fp_text reference J1 (at -15.6 -4 90) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.15)))
  )
  (fp_text value DRIVER (at 0 -8.15) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.15)))
  )
  (fp_line (start -15 -7.5) (end -15 0) (layer F.SilkS) (width 0.15))
  (fp_line (start -15 0) (end 10 0) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 0) (end 0 -7.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 15 -7.5) (end -15 -7.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -12.15 -4.5) (end -12.15 -3.5) (layer F.Fab) (width 0.01))
  (fp_line (start -12.15 -3.5) (end -12.85 -3.5) (layer F.Fab) (width 0.01))
  (fp_line (start -12.85 -3.5) (end -12.85 -4.5) (layer F.Fab) (width 0.01))
  (fp_line (start -12.85 -4.5) (end -12.15 -4.5) (layer F.Fab) (width 0.01))
  (fp_line (start -10 0) (end -10 0) (layer F.Fab) (width 0.15))
  (fp_line (start 15.5 -8) (end 15.5 0.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 15.5 0.5) (end -15.5 0.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -15.5 0.5) (end -15.5 -8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -15.5 -8) (end 15.5 -8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -10 -7.5) (end -10 0) (layer F.SilkS) (width 0.15))
  (fp_line (start -5 -7.5) (end -5 0) (layer F.SilkS) (width 0.15))
  (fp_line (start 15 -7) (end -15 -7) (layer F.SilkS) (width 0.15))
  (fp_line (start -15 -7.1) (end 15 -7.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 -7.1) (end 0 -7.2) (layer F.SilkS) (width 0.15))
  (fp_line (start 15 -7.2) (end -15 -7.2) (layer F.SilkS) (width 0.15))
  (fp_line (start -15 -7.2) (end -15 -7.3) (layer F.SilkS) (width 0.15))
  (fp_line (start -15 -7.3) (end 15 -7.3) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 -7.3) (end 0 -7.4) (layer F.SilkS) (width 0.15))
  (fp_line (start 15 -7.4) (end -15 -7.4) (layer F.SilkS) (width 0.15))
  (fp_line (start 5 -7.5) (end 5 0) (layer F.SilkS) (width 0.15))
  (fp_line (start 10 -7.5) (end 10 0) (layer F.SilkS) (width 0.15))
  (fp_line (start 10 0) (end 15 0) (layer F.SilkS) (width 0.15))
  (fp_line (start 15 0) (end 15 -7.5) (layer F.SilkS) (width 0.15))
  (pad 1 thru_hole circle (at -12.5 -4) (size 1.7 1.7) (drill 1.3) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -7.5 -4) (size 1.7 1.7) (drill 1.3) (layers *.Cu *.Mask))
  (pad 1 connect circle (at -12.5 -4) (size 2.8 2.8) (layers B.Cu B.Mask))
  (pad 2 connect circle (at -7.5 -4) (size 2.8 2.8) (layers B.Cu B.Mask))
  (pad 3 connect circle (at -2.5 -4) (size 2.8 2.8) (layers B.Cu B.Mask))
  (pad 3 thru_hole circle (at -2.5 -4) (size 1.7 1.7) (drill 1.3) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 2.5 -4) (size 1.7 1.7) (drill 1.3) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 7.5 -4) (size 1.7 1.7) (drill 1.3) (layers *.Cu *.Mask))
  (pad 4 connect circle (at 2.5 -4) (size 2.8 2.8) (layers B.Cu B.Mask))
  (pad 5 connect circle (at 7.5 -4) (size 2.8 2.8) (layers B.Cu B.Mask))
  (pad 6 connect circle (at 12.5 -4) (size 2.8 2.8) (layers B.Cu B.Mask))
  (pad 6 thru_hole circle (at 12.5 -4) (size 1.7 1.7) (drill 1.3) (layers *.Cu *.Mask))
  (model ${KICAD7_3DMODEL_DIR}/TerminalBlock_Wurth.3dshapes/Wurth_691137710006.stp
    (at (xyz -0.5905511811023623 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 90))
  )
)
