(module USB_C_Plug_Molex_105444 (layer F.Cu) (tedit 5BDD53A1)
  (descr "Universal Serial Bus (USB) Shielded I/O Plug, Type C, Right Angle, Surface Mount, http://www.molex.com/pdm_docs/sd/1054440001_sd.pdf")
  (tags "USB Type-C Plug Edge Mount")
  (attr smd)
  (fp_text reference P1 (at 0 2.04) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value USB_C_Plug (at 0 -1.96) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 2.04) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.1)))
  )
  (fp_line (start -4.3 1.96) (end -4.3 -1.46) (layer F.CrtYd) (width 0.05))
  (fp_text user "PCB Edge" (at 0.25 -0.5) (layer Dwgs.User)
    (effects (font (size 0.5 0.5) (thickness 0.08)))
  )
  (fp_line (start 3.35 0) (end 4.3 0) (layer F.Fab) (width 0.1))
  (fp_line (start 3.05 -0.66) (end 3.05 -0.3) (layer F.Fab) (width 0.1))
  (fp_arc (start 2.75 -0.66) (end 2.75 -0.96) (angle 90) (layer F.Fab) (width 0.1))
  (fp_line (start -2.75 -0.96) (end 2.75 -0.96) (layer F.Fab) (width 0.1))
  (fp_arc (start -2.75 -0.66) (end -3.05 -0.66) (angle 90) (layer F.Fab) (width 0.1))
  (fp_arc (start 3.35 -0.3) (end 3.35 0) (angle 90) (layer F.Fab) (width 0.1))
  (fp_line (start -3.05 -0.66) (end -3.05 -0.3) (layer F.Fab) (width 0.1))
  (fp_arc (start -3.35 -0.3) (end -3.05 -0.3) (angle 90) (layer F.Fab) (width 0.1))
  (fp_line (start -3.35 0) (end -4.3 0) (layer F.Fab) (width 0.1))
  (fp_line (start 4.3 1.96) (end 4.3 -1.46) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.3 -1.46) (end -4.3 -1.46) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.3 1.96) (end -4.3 1.96) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.85 0.9) (end 2.85 0.9) (layer F.Fab) (width 0.12))
  (fp_line (start -3.65 1.05) (end -3.2 1.05) (layer F.Fab) (width 0.12))
  (fp_line (start -4.1 -11) (end 4.1 -11) (layer F.Fab) (width 0.15))
  (fp_line (start -4.1 -11) (end -4.1 -4.45) (layer F.Fab) (width 0.15))
  (fp_line (start -4.1 -4.45) (end 4.1 -4.45) (layer F.Fab) (width 0.15))
  (fp_line (start 4.1 -11) (end 4.1 -4.45) (layer F.Fab) (width 0.15))
  (pad A1 smd roundrect (at -2.75 0.04) (size 0.34 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad A2 smd roundrect (at -2.25 0.04) (size 0.34 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad A3 smd roundrect (at -1.75 0.04) (size 0.34 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad A4 smd roundrect (at -1.25 0.04) (size 0.34 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad A5 smd roundrect (at -0.75 0.04) (size 0.34 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad A6 smd roundrect (at -0.25 0.04) (size 0.34 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad A7 smd roundrect (at 0.25 0.04) (size 0.34 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad A8 smd roundrect (at 0.75 0.04) (size 0.34 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad A9 smd roundrect (at 1.25 0.04) (size 0.34 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad A10 smd roundrect (at 1.75 0.04) (size 0.34 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad A11 smd roundrect (at 2.25 0.04) (size 0.34 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad A12 smd roundrect (at 2.75 0.04) (size 0.34 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad S1 smd roundrect (at -3.42 0.88) (size 0.7 1.15) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad S1 smd roundrect (at 3.42 0.88) (size 0.7 1.15) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  (pad B1 smd roundrect (at 2.75 0.04) (size 0.34 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  (pad B2 smd roundrect (at 2.25 0.04) (size 0.34 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  (pad B3 smd roundrect (at 1.75 0.04) (size 0.34 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  (pad B4 smd roundrect (at 1.25 0.04) (size 0.34 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  (pad B5 smd roundrect (at 0.75 0.04) (size 0.34 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  (pad B8 smd roundrect (at -0.75 0.04) (size 0.34 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  (pad B9 smd roundrect (at -1.25 0.04) (size 0.34 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  (pad B10 smd roundrect (at -1.75 0.04) (size 0.34 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  (pad B11 smd roundrect (at -2.25 0.04) (size 0.34 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  (pad B12 smd roundrect (at -2.75 0.04) (size 0.34 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  (model ${KICAD7_3DMODEL_DIR}/Connector_USB.3dshapes/Molex_105444.step
    (offset (xyz 0 3.3 -0.381))
    (scale (xyz 1 1 1))
    (rotate (xyz 90 0 0))
  )
)
