(footprint "Strain Gauge lands" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at -0.03 -22.69 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 876ab372-41d4-40cb-bbb2-d859637a6a41)
  )
  (fp_text value "Strain Gauge lands" (at -0.03 -21.19 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c81ef797-2ed0-4a61-9e64-6c57355ebc2b)
  )
  (fp_text user "${REFERENCE}" (at -0.03 -19.69 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 45f8772a-050d-4c97-9001-e4c022a5dde6)
  )
  (fp_circle (center 0 0) (end 6 0)
    (stroke (width 0.12) (type default)) (fill none) (layer "Dwgs.User") (tstamp a477146e-27ee-4bd2-aa56-13688dbf24ed))
  (pad "1" smd circle (at 1.5 -4.5) (size 2 2) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp e5dd346e-fcca-4b1d-8a0b-7a1e63b63d18))
  (pad "2" smd circle (at 1.5 -2.25) (size 2 2) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp f2192fd5-eb50-45a6-ad6f-4c8b2c9d9257))
)
