(module "DSUB-5+2_Male_straddle_mounted" (layer F.Cu) (tedit 5D9F6615)
  (fp_text reference "REF**" (at 4.25 0 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "DSUB-5+2_Male_straddle_mounted" (at -4 0 90) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.05)))
  )
  (fp_line (start 0 -15) (end 0 15) (layer Dwgs.User) (width 0.05))
  (pad "A1" thru_hole oval (at 4.75 -6.85) (size 15.7 6.3) (drill oval 15.1 5.6) (layers *.Cu *.Mask))
  (pad "A2" thru_hole oval (at 4.75 6.85) (size 15.7 6.3) (drill oval 15.1 5.6) (layers *.Cu *.Mask))
  (pad "1" connect roundrect (at 1.5 -1.384) (size 3.6 1.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2))
  (pad "2" connect roundrect (at 1.5 1.384) (size 3.6 1.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2))
  (pad "3" connect roundrect (at 1.5 -2.6) (size 3.6 1.5) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.2))
  (pad "4" connect roundrect (at 1.5 0) (size 3.6 1.5) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.2))
  (pad "5" connect roundrect (at 1.5 2.6) (size 3.6 1.5) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.2))
  (model "${KICAD7_3DMODEL_DIR}/Connector_Dsub.3dshapes/NorComp_680M7W2103L401.step"
    (offset (xyz -6.15 0 -0.65))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 90))
  )
)
