(module Maxim_MAX4372x_UCSP_1x1.5mm_BGA (layer F.Cu) (tedit 5489DB6E)
  (solder_mask_margin -0.04)
  (solder_paste_margin -0.06)
  (attr smd)
  (fp_text reference U1 (at 0 -1.2) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text value VAL** (at 0 1.2) (layer Cmts.User)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_circle (center -1.2 -0.65) (end -1.2 -0.7) (layer F.SilkS) (width 0.127))
  (fp_line (start 0.95 0.4) (end 0.95 0.7) (layer F.SilkS) (width 0.127))
  (fp_line (start 0.95 0.7) (end 0.65 0.7) (layer F.SilkS) (width 0.127))
  (fp_line (start 0.95 -0.4) (end 0.95 -0.7) (layer F.SilkS) (width 0.127))
  (fp_line (start 0.95 -0.7) (end 0.65 -0.7) (layer F.SilkS) (width 0.127))
  (fp_line (start -0.95 -0.4) (end -0.95 -0.7) (layer F.SilkS) (width 0.127))
  (fp_line (start -0.95 -0.7) (end -0.65 -0.7) (layer F.SilkS) (width 0.127))
  (fp_line (start -0.95 0.7) (end -0.65 0.7) (layer F.SilkS) (width 0.127))
  (fp_line (start -0.95 0.7) (end -0.95 0.4) (layer F.SilkS) (width 0.127))
  (fp_line (start -1 -0.75) (end -1 0.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1 0.75) (end 1 0.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1 0.75) (end 1 -0.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1 -0.75) (end 1 -0.75) (layer F.CrtYd) (width 0.05))
  (pad A1 smd circle (at -0.5 -0.25) (size 0.35 0.35) (layers F.Cu F.Paste F.Mask))
  (pad A2 smd circle (at 0 -0.25) (size 0.35 0.35) (layers F.Cu F.Paste F.Mask))
  (pad A3 smd circle (at 0.5 -0.25) (size 0.35 0.35) (layers F.Cu F.Paste F.Mask))
  (pad B1 smd circle (at -0.5 0.25) (size 0.35 0.35) (layers F.Cu F.Paste F.Mask))
  (pad B3 smd circle (at 0.5 0.25) (size 0.35 0.35) (layers F.Cu F.Paste F.Mask))
)
