(footprint "IX61G-A-10P" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Field2" "")
  (property "Sheetfile" "Ethernet.kicad_sch")
  (property "Sheetname" "Ethernet")
  (property "ki_description" "Generic connectable mounting pin connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)")
  (property "ki_keywords" "connector")
  (attr smd)
  (fp_text reference "J25" (at -4.3 -0.15 90 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 1c226b39-f915-4112-af22-b4cf32fd4ad2)
  )
  (fp_text value "Eth" (at 0 -6.7 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp 9bf4c2d1-5381-4e40-9874-b3b47e85d129)
  )
  (fp_text user "Recommended pitch" (at 0 10.5 unlocked) (layer "Dwgs.User")
      (effects (font (size 0.25 0.25) (thickness 0.0625)) (justify bottom))
    (tstamp 40698187-b2ec-490c-b847-c19c35e5eee5)
  )
  (fp_text user "${REFERENCE}" (at 0 -7.15 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp 19abb0fa-00ae-4428-9bf7-6018e0e38b21)
  )
  (fp_text user "Connector panel face" (at 0 2.05 unlocked) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.1)) (justify bottom))
    (tstamp e7344312-fe49-498c-8445-0baeb35c44b8)
  )
  (fp_line (start -5.05 -4.5) (end -5.05 -9.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e30cbfea-432a-4a41-86ba-1adf2f649a01))
  (fp_line (start -4.9 -9.65) (end -3.7 -9.65)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 20fa0e1c-1d44-44eb-a57d-b3b994a9beef))
  (fp_line (start -3.75 -4.35) (end -4.9 -4.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 724254c1-36e8-4b2b-96eb-185d58a6812f))
  (fp_line (start -3.75 0) (end -3.75 -4.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 657bceb4-4443-4852-9636-5958c2cf15fe))
  (fp_line (start -3.7 -9.65) (end -3.7 -10.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1effec37-62b6-4a53-8bf1-34b06d710a51))
  (fp_line (start -3.5 -11) (end -1.25 -11)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a00e72d5-5c1e-4de7-a79e-764b623c6a2a))
  (fp_line (start -1.05 -10.8) (end -1.05 -10.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 851ff286-5f5c-45a7-840f-6cf00a1a6cd6))
  (fp_line (start -1.05 -10.4) (end 1.05 -10.4)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1e216b40-09d1-4d1c-a91e-6235123b34e0))
  (fp_line (start 1.05 -10.4) (end 1.05 -10.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 29b152a4-8578-4a07-b78d-b9129039dc2a))
  (fp_line (start 1.25 -11) (end 3.5 -11)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e0663fd1-a06b-431a-89e3-726e84b884c1))
  (fp_line (start 3.7 -10.8) (end 3.7 -9.65)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 35cec8ed-6878-41e2-94ae-9022b8e93465))
  (fp_line (start 3.7 -9.65) (end 4.9 -9.65)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 094071fc-ddf9-4e9e-87d9-663afcac7818))
  (fp_line (start 3.75 -4.35) (end 3.75 0)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a55f0720-193b-4881-a8d0-fdb802c1fef3))
  (fp_line (start 3.75 0) (end -3.75 0)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0193a6b8-e7fb-4b25-a076-ac6a5560d197))
  (fp_line (start 4.9 -4.35) (end 3.75 -4.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 402f4624-6190-43a4-a7b9-72ae6bd42110))
  (fp_line (start 5.05 -9.5) (end 5.05 -4.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3ab41ad0-1318-444a-9999-4411bdfacc07))
  (fp_arc (start -5.05 -9.5) (mid -5.006066 -9.606066) (end -4.9 -9.65)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 60b9872b-eaed-470e-8352-db4247dae068))
  (fp_arc (start -4.9 -4.35) (mid -5.006066 -4.393934) (end -5.05 -4.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 31c7935f-529d-4e5d-92f0-7fc34342364c))
  (fp_arc (start -3.7 -10.8) (mid -3.641421 -10.941421) (end -3.5 -11)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6bc73ab5-c1d6-446a-b478-b7dfafae62f3))
  (fp_arc (start -1.25 -11) (mid -1.108579 -10.941421) (end -1.05 -10.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 85b19458-d631-45fc-9365-7caefc7b9c27))
  (fp_arc (start 1.05 -10.8) (mid 1.108579 -10.941421) (end 1.25 -11)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6c17ee32-5dbb-4c46-b979-a7553ce09a54))
  (fp_arc (start 3.5 -11) (mid 3.641421 -10.941421) (end 3.7 -10.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e37e2df3-b2c7-4282-9df4-924a8cc56a50))
  (fp_arc (start 4.9 -9.65) (mid 5.006066 -9.606066) (end 5.05 -9.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 184cef7b-f5ca-4f46-af81-4268889a7ee6))
  (fp_arc (start 5.05 -4.5) (mid 5.006066 -4.393934) (end 4.9 -4.35)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d242dbb0-71ed-4edc-83d3-dbba8f396802))
  (fp_line (start -3.2 2.25) (end -3.2 0)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 2aeb88ea-1731-4c92-b766-ba28e7eb7bd3))
  (fp_line (start -3.2 2.25) (end 3.2 2.25)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp c6b1ff54-e8b5-4ad5-9d4e-5349abb65032))
  (fp_line (start 3.2 2.25) (end 3.2 0)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp cf044808-33ab-4d62-b931-4c8240da7ad9))
  (pad "" smd roundrect (at -3.9 -7.5) (size 2.5 2.7) (layers "F.Paste") (roundrect_rratio 0.1) (tstamp fd083eff-11f8-44b5-8d67-760b62784d79))
  (pad "" smd roundrect (at -2.6 -1.75) (size 2.5 2.7) (layers "F.Paste") (roundrect_rratio 0.1) (tstamp 81b0ead9-63dc-42e1-b854-bca55705a9f7))
  (pad "" smd roundrect (at 0 -9) (size 2 3) (layers "F.Paste") (roundrect_rratio 0.125) (tstamp e3794ef2-b845-4be2-842b-47645fba6e91))
  (pad "" np_thru_hole oval (at 0 -1.25) (size 1.3 2) (drill oval 1.2 1.9) (layers "F&B.Cu" "*.Mask") (tstamp 73713e6a-401b-4362-b676-51863f0bcad9))
  (pad "" smd roundrect (at 2.6 -1.75) (size 2.5 2.7) (layers "F.Paste") (roundrect_rratio 0.1) (tstamp 801aac19-fe8d-4627-ab46-7c43f66b62e7))
  (pad "" smd roundrect (at 3.9 -7.5) (size 2.5 2.7) (layers "F.Paste") (roundrect_rratio 0.1) (tstamp 8347135c-0ac7-498d-a011-d3d7435f6ac7))
  (pad "1" smd roundrect (at -3.375 -10.15) (size 0.3 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1666666667) (tstamp 03cf3b80-bd36-46bd-8b66-784820a22cbc))
  (pad "2" smd roundrect (at -2.875 -10.15) (size 0.3 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1666666667) (tstamp 85044925-04af-4520-9426-9580bb1ed24a))
  (pad "3" smd roundrect (at -2.375 -10.15) (size 0.3 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1666666667) (tstamp 555e65a1-15f7-490b-9d9d-7cc1caa12fd8))
  (pad "4" smd roundrect (at -1.875 -10.15) (size 0.3 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1666666667) (tstamp 897ba1da-c8f0-4133-9b4e-94bfff9dadf3))
  (pad "5" smd roundrect (at -1.375 -10.15) (size 0.3 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1666666667) (tstamp d4d5e186-0e66-40bf-a1d7-c132290962af))
  (pad "6" smd roundrect (at 1.375 -10.15) (size 0.3 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1666666667) (tstamp a3873da5-4fee-4e4e-b81a-6260f299b39e))
  (pad "7" smd roundrect (at 1.875 -10.15) (size 0.3 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1666666667) (tstamp 4ec290a7-484b-46cb-821a-88150f6867fc))
  (pad "8" smd roundrect (at 2.375 -10.15) (size 0.3 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1666666667) (tstamp a483d057-7bbd-4cb7-8cd2-9fc8a510cb8c))
  (pad "9" smd roundrect (at 2.875 -10.15) (size 0.3 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1666666667) (tstamp 4bc88d99-e99d-4826-96da-61e47a41143b))
  (pad "10" smd roundrect (at 3.375 -10.15) (size 0.3 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1666666667) (tstamp 0858145d-8a5a-4512-8163-0320cda2b9de))
  (pad "MP" thru_hole roundrect (at -4.2 -7.5) (size 1.4 2.7) (drill oval 0.8 2.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 8ef242ef-4e3c-4e6a-b4cd-5800ab5c2788))
  (pad "MP" thru_hole roundrect (at -2.9 -1.75) (size 1.4 2.7) (drill oval 0.8 2.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 60e346e6-6ec5-4935-89b1-45d1f02ddb99))
  (pad "MP" thru_hole roundrect (at 0 -9.25) (size 2 2) (drill 1.4) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.125)
    (thermal_bridge_angle 45) (tstamp e0bffbf8-d1b7-423c-8d8e-a049ff91ea69))
  (pad "MP" thru_hole roundrect (at 2.9 -1.75) (size 1.4 2.7) (drill oval 0.8 2.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp b4258d29-cc4c-42a2-82f8-2bdc0d36f576))
  (pad "MP" thru_hole roundrect (at 4.2 -7.5) (size 1.4 2.7) (drill oval 0.8 2.1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1785714286)
    (thermal_bridge_angle 45) (tstamp 98990453-757e-4f18-b082-8ffe744386ac))
  (zone (net 0) (net_name "") (layer "F.Cu") (tstamp 1d5f5dac-9490-4984-80d5-b57ece2530ca) (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy -3.6 0)
        (xy -3.6 -4.499999)
        (xy -4.9 -4.499999)
        (xy -4.9 -9.499999)
        (xy 4.899999 -9.5)
        (xy 4.899999 -4.5)
        (xy 3.599999 -4.5)
        (xy 3.6 0)
      )
    )
  )
  (model "${KICAD7_3DMODEL_DIR}/Connector_Hirose.3dshapes/IX61G-A-10P.stp"
    (offset (xyz 203.25 -0.6 3.2))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
)
