(footprint "UQFN-8 1.4x1.2 P0.4mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -1.4 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 92f96e78-32da-4078-9380-e0693fdbd43c)
  )
  (fp_text value "UQFN-8 1.4x1.2 P0.4mm" (at 0 1.35 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.15)))
    (tstamp 8fe8a8bb-6716-4b51-a45b-fd2327605be4)
  )
  (fp_text user "${REFERENCE}" (at -0.05 1.05 unlocked) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp c5ba263e-172d-47c5-a331-01c8d66211ad)
  )
  (fp_arc (start -0.875 -0.7) (mid -0.853033 -0.753033) (end -0.8 -0.775)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 03ffb7c1-dfff-4dd6-a4a7-85b7c616f051))
  (fp_arc (start -0.8 0.775) (mid -0.853033 0.753033) (end -0.875 0.7)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 33ab86cd-a419-46f4-8e44-e209ba8a492e))
  (fp_arc (start 0.8 -0.775) (mid 0.853033 -0.753033) (end 0.875 -0.7)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 5217cae5-af62-4c02-ac42-178b2e740007))
  (fp_arc (start 0.875 0.7) (mid 0.853033 0.753033) (end 0.8 0.775)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp e6e74700-301d-4c8c-857b-1e94a2c90eef))
  (fp_poly
    (pts
      (xy -0.9 0)
      (xy -1.1 -0.15)
      (xy -1.1 0.15)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp b97bf09c-f295-4083-b766-ab4fa43a63b8))
  (fp_poly
    (pts
      (xy -0.6 -0.7)
      (xy -0.8 -0.7)
      (xy -0.8 -0.2)
      (xy -0.95 -0.2)
      (xy -0.95 -0.7)
      (xy -0.8 -0.85)
      (xy -0.6 -0.85)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 0bb8b20c-e649-4c73-9bcc-454f5c82bcd4))
  (fp_poly
    (pts
      (xy -0.6 0.7)
      (xy -0.8 0.7)
      (xy -0.8 0.2)
      (xy -0.95 0.2)
      (xy -0.95 0.7)
      (xy -0.8 0.85)
      (xy -0.6 0.85)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp ac201592-8fe4-409b-8a6b-6fba0671cda6))
  (fp_poly
    (pts
      (xy 0.6 -0.7)
      (xy 0.8 -0.7)
      (xy 0.8 -0.2)
      (xy 0.95 -0.2)
      (xy 0.95 -0.7)
      (xy 0.8 -0.85)
      (xy 0.6 -0.85)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp c7f6aab7-d98c-48f3-a27b-c2b01424d9f2))
  (fp_poly
    (pts
      (xy 0.6 0.7)
      (xy 0.8 0.7)
      (xy 0.8 0.2)
      (xy 0.95 0.2)
      (xy 0.95 0.7)
      (xy 0.8 0.85)
      (xy 0.6 0.85)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp e0067e1c-57d4-42b8-adf0-3e90347963b1))
  (fp_line (start -0.95 -0.6) (end -0.95 0.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 861e2de7-d85a-4f0f-bedc-9423bfdb3caa))
  (fp_line (start -0.7 0.85) (end 0.7 0.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 39a4bf0c-bbc5-4945-81eb-48e1c59eee05))
  (fp_line (start 0.7 -0.85) (end -0.7 -0.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e1701ce5-122d-4751-b8b6-aaecaea236ea))
  (fp_line (start 0.95 0.6) (end 0.95 -0.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 45c03292-d6be-462f-8d35-7663c499a55e))
  (fp_arc (start -0.95 -0.6) (mid -0.876777 -0.776777) (end -0.7 -0.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp cd4336d3-4a14-4d5c-be9e-0c23a2489e10))
  (fp_arc (start -0.7 0.85) (mid -0.876777 0.776777) (end -0.95 0.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2acf683f-afc0-415a-8136-6d650cecc6d6))
  (fp_arc (start 0.7 -0.85) (mid 0.876777 -0.776777) (end 0.95 -0.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0c478289-2d83-4c58-891e-45933c505b94))
  (fp_arc (start 0.95 0.6) (mid 0.876777 0.776777) (end 0.7 0.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 4300c116-f59f-47d5-b3ca-df8893f597cb))
  (fp_rect (start -0.7 -0.6) (end 0.7 0.6)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 793d0ea5-a26c-4baf-8b82-afad695664d7))
  (pad "1" smd roundrect (at -0.525 0 90) (size 0.25 0.55) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.05) (chamfer bottom_left bottom_right)
    (thermal_bridge_angle 45) (tstamp 961bd9a7-bac7-4431-8b54-3bbec0ed9b72))
  (pad "2" smd roundrect (at -0.4 0.475 180) (size 0.25 0.45) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.05) (chamfer bottom_left bottom_right)
    (thermal_bridge_angle 45) (tstamp cfd463c8-b896-4ab0-a3b9-089e18a7f388))
  (pad "3" smd roundrect (at 0 0.475 180) (size 0.25 0.45) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.05) (chamfer bottom_left bottom_right)
    (thermal_bridge_angle 45) (tstamp 824478bd-7aae-4506-93d9-e05c6c799429))
  (pad "4" smd roundrect (at 0.4 0.475 180) (size 0.25 0.45) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.05) (chamfer bottom_left bottom_right)
    (thermal_bridge_angle 45) (tstamp bf26dc2d-81f8-4e59-b63e-24ba1ba94b6c))
  (pad "5" smd roundrect (at 0.575 0 270) (size 0.25 0.45) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.05) (chamfer bottom_left bottom_right)
    (thermal_bridge_angle 45) (tstamp 430f1235-728c-496e-92dc-bde28204a021))
  (pad "6" smd roundrect (at 0.4 -0.475) (size 0.25 0.45) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.05) (chamfer bottom_left bottom_right)
    (thermal_bridge_angle 45) (tstamp 0ea9eb4f-1e1a-4c40-a761-676fa0c8f4c7))
  (pad "7" smd roundrect (at 0 -0.475) (size 0.25 0.45) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.05) (chamfer bottom_left bottom_right)
    (thermal_bridge_angle 45) (tstamp 9bb0ecde-57bc-4137-b8e6-0c4fac2cce77))
  (pad "8" smd roundrect (at -0.4 -0.475) (size 0.25 0.45) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
    (chamfer_ratio 0.05) (chamfer bottom_left bottom_right)
    (thermal_bridge_angle 45) (tstamp c0ff2dc3-fd0a-463b-9da2-6141d11758c6))
)
