(module "7P_2x0.7_1_pitch_DS" (layer F.Cu) (tedit 5DFB89C7)
  (fp_text reference "J1" (at 0 -1.75 unlocked) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "Conn_01x07" (at 0 -1.75 unlocked) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.05)))
  )
  (pad "6" thru_hole circle (at 2 0.5) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask))
  (pad "5" thru_hole circle (at 1 0.5) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask))
  (pad "4" thru_hole circle (at 0 0.5) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask))
  (pad "3" thru_hole circle (at -1 0.5) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask))
  (pad "2" thru_hole circle (at -2 0.5) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask))
  (pad "6" thru_hole circle (at 2 -0.5) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask))
  (pad "5" thru_hole circle (at 1 -0.5) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask))
  (pad "4" thru_hole circle (at 0 -0.5) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask))
  (pad "3" thru_hole circle (at -1 -0.5) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask))
  (pad "2" thru_hole circle (at -2 -0.5) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask))
  (pad "1" thru_hole circle (at -3 0.5) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask))
  (pad "1" thru_hole circle (at -3 -0.5) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask))
  (pad "6" thru_hole roundrect (at 2 0) (size 0.7 2) (drill 0.3) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
  (pad "5" thru_hole roundrect (at 1 0) (size 0.7 2) (drill 0.3) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
  (pad "4" thru_hole roundrect (at 0 0) (size 0.7 2) (drill 0.3) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
  (pad "3" thru_hole roundrect (at -1 0) (size 0.7 2) (drill 0.3) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
  (pad "2" thru_hole roundrect (at -2 0) (size 0.7 2) (drill 0.3) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
  (pad "1" thru_hole roundrect (at -3 0) (size 0.7 2) (drill 0.3) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
  (pad "7" thru_hole roundrect (at 3 0) (size 0.7 2) (drill 0.3) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
  (pad "7" thru_hole circle (at 3 -0.5) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask))
  (pad "7" thru_hole circle (at 3 0.5) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask))
)
