(module JP-4_2mm (layer F.Cu) (tedit 54896C07)
  (fp_text reference JP-4_2mm (at 0 -1.75) (layer Cmts.User)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text value VAL** (at 0 1.75) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_line (start 2 1) (end 4 1) (layer F.SilkS) (width 0.127))
  (fp_line (start 2 -1) (end 4 -1) (layer F.SilkS) (width 0.127))
  (fp_line (start 2 1) (end -2 1) (layer F.SilkS) (width 0.127))
  (fp_line (start -2 -1) (end 2 -1) (layer F.SilkS) (width 0.127))
  (fp_line (start 4 -1) (end 4 1) (layer F.SilkS) (width 0.127))
  (fp_line (start -4 -1) (end -2 -1) (layer F.SilkS) (width 0.127))
  (fp_line (start -2 -1) (end -2 1) (layer F.SilkS) (width 0.127))
  (fp_line (start -2 1) (end -4 1) (layer F.SilkS) (width 0.127))
  (fp_line (start -4 1) (end -4 -1) (layer F.SilkS) (width 0.127))
  (fp_line (start 4.5 -1.5) (end -4.5 -1.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.5 -1.5) (end 4.5 2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.5 2) (end -4.5 2) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.5 2) (end -4.5 -1.5) (layer F.CrtYd) (width 0.05))
  (pad 1 thru_hole rect (at -3 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -1 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 1 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
  (pad 2 connect oval (at -1 0.125) (size 1.5 1.75) (layers B.Cu B.Mask))
  (pad 1 connect rect (at -3 0.125) (size 1.5 1.75) (layers B.Cu B.Mask))
  (pad 3 connect oval (at 1 0.125) (size 1.5 1.75) (layers B.Cu B.Mask))
  (pad 4 thru_hole circle (at 3 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
  (pad 4 connect oval (at 3 0.125) (size 1.5 1.75) (layers B.Cu B.Mask))
)
