(footprint "AS0B82x-S55B-7H" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (solder_paste_margin -0.1)
  (attr smd)
  (fp_text reference "REF**" (at 0.7 -17.3 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b51155d8-1baa-46de-8587-be502d2b2483)
  )
  (fp_text value "AS0B82x-S55B-7H" (at 0.7 -15.8 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp bd35bca7-ddfd-45c9-b732-9456e739fa51)
  )
  (fp_text user "${REFERENCE}" (at 0.7 -14.3 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp cda60b8e-f775-4876-b829-946399ba448d)
  )
  (fp_rect (start -42.3 -4.2) (end 42.3 4.7)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.Fab") (tstamp 14d27689-3463-4471-9956-dca1a506118e))
  (pad "" smd roundrect (at -44 -0.72) (size 3 5.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 1bcfdbce-62bb-41bf-af32-0bc74b44d956))
  (pad "" np_thru_hole circle (at -41 0) (size 1.3 1.3) (drill 1.1) (layers "F&B.Cu" "*.Mask") (tstamp f0df5fef-c274-41fa-86aa-66580b3bc3e7))
  (pad "" smd roundrect (at -39.55 3.2) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp bbdaaf35-6149-403d-b82f-db0fa493c8d4))
  (pad "" smd roundrect (at -39.55 4.3) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp 5529392f-4c5c-424d-b747-0b768dbba860))
  (pad "" smd roundrect (at -39.3 -4.05) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp 6b9b51f3-8a1a-4682-84c3-b47f9f1643ed))
  (pad "" smd roundrect (at -39.3 -2.95) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp 7a48ee3d-929d-4d85-a3b6-444fb538466d))
  (pad "" smd roundrect (at -38.35 3.2) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp 01355562-8155-47b6-be1f-4ebab06f60e1))
  (pad "" smd roundrect (at -38.35 4.3) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp 83e0e3ba-53ff-4d04-b551-f1306569a159))
  (pad "" smd roundrect (at -38.1 -4.05) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp 65ec8272-10d6-4d6b-b7fa-de6110c831dd))
  (pad "" smd roundrect (at -38.1 -2.95) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp fb39faba-9dbf-4df1-90f1-e0aaf54578d4))
  (pad "" smd roundrect (at -37.15 3.2) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp 78424a83-83e3-4907-a613-eebfebd4de49))
  (pad "" smd roundrect (at -37.15 4.3) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp 675c1bf4-7669-4d4d-8be9-0565affa92e2))
  (pad "" smd roundrect (at -36.9 -4.05) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp 63368a06-f609-4801-99bb-9825a5cc67a4))
  (pad "" smd roundrect (at -36.9 -2.95) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp 726bf5c2-1640-492b-97f7-7c58e84bb775))
  (pad "" smd roundrect (at -35.95 3.2) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp 3dcf7974-6f3a-463a-b285-f48661cfdca3))
  (pad "" smd roundrect (at -35.95 4.3) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp 7ebdf03a-2de0-4817-8ea2-7d13f18f56de))
  (pad "" smd roundrect (at -35.7 -4.05) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp 38b18aef-7e1a-41ae-965c-4e16f71a4193))
  (pad "" smd roundrect (at -35.7 -2.95) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp 014fc532-3f14-4c73-b225-d90f9a8c6f32))
  (pad "" smd roundrect (at -34.55 3.2) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp e8d12c5f-463c-44d1-823f-6f416be30212))
  (pad "" smd roundrect (at -34.55 4.3) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp b790ad46-c4e9-4c37-8030-6565503e2d25))
  (pad "" smd roundrect (at -34.3 -4.05) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp ae0dc0de-c877-41ab-ba0d-d8c86eb6b60c))
  (pad "" smd roundrect (at -34.3 -2.95) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp 86a22bd8-d268-4f17-a736-b8a4cceba5b9))
  (pad "" smd roundrect (at -33.35 3.2) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp 286ad67d-da30-45dc-87a0-5efe39192580))
  (pad "" smd roundrect (at -33.35 4.3) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp 64223e3d-a0ff-4376-8909-c96f7cf1e652))
  (pad "" smd roundrect (at -33.1 -4.05) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp 74660bb0-26fa-442d-ba8f-69580fe928bc))
  (pad "" smd roundrect (at -33.1 -2.95) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp 290d77a4-4678-435b-8721-7443aab72607))
  (pad "" smd roundrect (at -32.15 3.2) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp 0960064a-2c2a-490e-a2e9-aa51abec1999))
  (pad "" smd roundrect (at -32.15 4.3) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp f5110ae0-d014-4221-abe6-5af6f8d7056f))
  (pad "" smd roundrect (at -31.9 -4.05) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp e51b1e82-9e03-435c-b884-d7ddf13030e5))
  (pad "" smd roundrect (at -31.9 -2.95) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp 7e448c99-be4a-4d91-9ae0-4b412acc608c))
  (pad "" smd roundrect (at -30.95 3.2) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp e3dd8741-569c-4cd7-b869-757426350a0a))
  (pad "" smd roundrect (at -30.95 4.3) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp 099ea7a9-d2e1-4152-bfa3-2fa8a1cf9e03))
  (pad "" smd roundrect (at -30.7 -4.05) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp 69aa18d6-a345-479f-aa9d-8b139a306138))
  (pad "" smd roundrect (at -30.7 -2.95) (size 1 0.8) (layers "F.Paste") (roundrect_rratio 0.1875) (tstamp fdfc1d3c-f812-436c-95c1-8e2b43b3978e))
  (pad "" smd roundrect (at -29.6 3.75) (size 1 1.4) (layers "F.Paste") (roundrect_rratio 0.1428571429) (tstamp 92e4c4a4-241e-4463-b0f8-d35e2276c309))
  (pad "" smd roundrect (at -29 3.75) (size 2.4 2) (layers "F.Mask") (roundrect_rratio 0.02631578947) (tstamp 3eb0c0cb-c1e8-4d7b-90d0-4ff2f3434070))
  (pad "" smd roundrect (at -28.4 3.75) (size 1 1.4) (layers "F.Paste") (roundrect_rratio 0.1428571429) (tstamp f49d1f18-9590-451b-93f7-59681c202eda))
  (pad "" smd roundrect (at -26.75 3.75) (size 1.7 1.4) (layers "F.Paste") (roundrect_rratio 0.1428571429) (tstamp ac5b5f5c-e967-4c13-bfa6-061078f4c9fe))
  (pad "" smd roundrect (at -26.75 3.75) (size 1.9 2) (layers "F.Mask") (roundrect_rratio 0.02631578947) (tstamp 2ecfc53a-0c8a-4a59-b515-e2dd48ee8c85))
  (pad "" np_thru_hole circle (at 41 0) (size 1.8 1.8) (drill 1.6) (layers "F&B.Cu" "*.Mask") (tstamp b8852abd-0f5b-4601-b258-d20d185bafee))
  (pad "" smd roundrect (at 44 -0.72) (size 3 5.15) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp aaab5282-608a-4885-8962-104219e455f6))
  (pad "1" smd roundrect (at -30 3.75) (size 0.4 2) (layers "F.Cu") (roundrect_rratio 0.125) (tstamp 56f93803-cf2f-4a32-a8aa-e172fcf2dbff))
  (pad "2" smd roundrect (at -29.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp cfe45b64-3584-40d7-b601-246dc4a81585))
  (pad "3" smd roundrect (at -29.5 3.75) (size 0.4 2) (layers "F.Cu") (roundrect_rratio 0.125) (tstamp b3969f68-4f36-45ca-be12-e3601c068a26))
  (pad "4" smd roundrect (at -29.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp d9b2edd4-107a-441c-882d-a2776c5cf4b7))
  (pad "5" smd roundrect (at -29 3.75) (size 0.4 2) (layers "F.Cu") (roundrect_rratio 0.125) (tstamp 88a94deb-14c7-4fe7-8054-2c9aa35a6f99))
  (pad "6" smd roundrect (at -28.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 2f03c596-4bd5-4ff7-8f0d-a32c76d05d81))
  (pad "7" smd roundrect (at -28.5 3.75) (size 0.4 2) (layers "F.Cu") (roundrect_rratio 0.125) (tstamp 869b12d0-9f94-48dd-bedc-d81ea3d66c20))
  (pad "8" smd roundrect (at -28.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 3bf3d6ed-d424-40d8-930e-396d072e5769))
  (pad "9" smd roundrect (at -28 3.75) (size 0.4 2) (layers "F.Cu") (roundrect_rratio 0.125) (tstamp 4e68744f-1002-4044-a55b-e0499ee2fce8))
  (pad "10" smd roundrect (at -27.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 532cf37d-91ec-40d6-a586-38798efa9611))
  (pad "11" smd roundrect (at -27.5 3.75) (size 0.4 2) (layers "F.Cu") (roundrect_rratio 0.125) (tstamp 798fff47-03f5-48bd-8b33-5f555f92c83e))
  (pad "12" smd roundrect (at -27.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 908b9c3b-02a1-471b-996a-705d9c76dabc))
  (pad "13" smd roundrect (at -27 3.75) (size 0.4 2) (layers "F.Cu") (roundrect_rratio 0.125) (tstamp ec2df221-643c-4e32-a469-73de6e97e5b6))
  (pad "14" smd roundrect (at -26.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp e54ef82e-b462-49f6-87d5-bb02dcd99860))
  (pad "15" smd roundrect (at -26.5 3.75) (size 0.4 2) (layers "F.Cu") (roundrect_rratio 0.125) (tstamp 9515be71-e4be-4584-8c8d-d37f47582e51))
  (pad "16" smd roundrect (at -26.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 09c2498c-1f43-46e7-aa28-6399a6641aac))
  (pad "17" smd roundrect (at -26 3.75) (size 0.4 2) (layers "F.Cu") (roundrect_rratio 0.125) (tstamp 5f93bbfe-df0a-447e-90c6-aacc15e2f295))
  (pad "18" smd roundrect (at -25.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 0b94cb27-3479-4b7a-9808-ef325c0244e8))
  (pad "19" smd roundrect (at -25.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp adc0462c-14af-46d5-b74e-c3b438a1fb72))
  (pad "20" smd roundrect (at -25.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp fa5a2752-f107-41e0-bb7b-c70131ca7dbc))
  (pad "21" smd roundrect (at -25 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp deb1bb28-2802-44a6-bdcb-e4d8cf83f949))
  (pad "22" smd roundrect (at -24.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp be265028-355c-4689-bd2a-b05b27146561))
  (pad "23" smd roundrect (at -24.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 6533b736-284b-4c76-b63b-feae07c89283))
  (pad "24" smd roundrect (at -24.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 07533a59-f85f-4bf2-8a7b-98948a5d54d7))
  (pad "25" smd roundrect (at -24 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 8015f850-e8b1-44f1-aaee-9d6acc4bf45c))
  (pad "26" smd roundrect (at -23.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp a14fce1e-11b3-4766-b9ff-a5ffc743a901))
  (pad "27" smd roundrect (at -23.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp d36380fa-7148-49a8-bc72-7aa166c64e77))
  (pad "28" smd roundrect (at -23.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp c4b852b4-f6f4-4452-a6a0-08a0b498808e))
  (pad "29" smd roundrect (at -23 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 49805f7d-7767-4ae1-9ea1-1494c7131222))
  (pad "30" smd roundrect (at -22.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 0561b931-f692-482d-bfc7-647d0d9b9758))
  (pad "31" smd roundrect (at -22.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp bb4eafe8-be3c-42b3-af1f-0b6ebc506061))
  (pad "32" smd roundrect (at -22.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp cab61def-c72b-4921-ae59-eae3a0fb81d2))
  (pad "33" smd roundrect (at -22 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 95fc70c2-8f4b-4681-8779-f0fac53159d8))
  (pad "34" smd roundrect (at -21.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 7e326766-7a88-424f-bf98-74c322332353))
  (pad "35" smd roundrect (at -21.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 8d3e42eb-1e37-4e3d-bb9a-78ebbeacc6c1))
  (pad "36" smd roundrect (at -21.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp b723aa5b-ab32-47f2-bf6a-712978b14679))
  (pad "37" smd roundrect (at -21 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 7684d5ae-a875-4c97-8be7-7e88629ddaf9))
  (pad "38" smd roundrect (at -20.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp ab9d4d7a-055c-4b4e-bebb-c2c3326eb47d))
  (pad "39" smd roundrect (at -20.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 7cbc167a-87ef-488c-8285-b6f9662f099f))
  (pad "40" smd roundrect (at -20.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp bc06730a-dc75-443c-8c43-46d4987f9d20))
  (pad "41" smd roundrect (at -20 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 3b896229-77e9-4b38-a678-2a96a0fd51b1))
  (pad "42" smd roundrect (at -19.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 52937dc8-7e14-460e-ba6d-55e1dd6cea1d))
  (pad "43" smd roundrect (at -19.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 6ea25078-8c1f-4734-9d33-f043a861d001))
  (pad "44" smd roundrect (at -19.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 0d5e95ec-4abd-46f2-9209-61ce757f8846))
  (pad "45" smd roundrect (at -19 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 6ab43fc9-0d1e-496d-99bc-2761e6228d69))
  (pad "46" smd roundrect (at -18.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 1f143689-30b2-4c58-90cf-28c4618515cc))
  (pad "47" smd roundrect (at -18.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 4eddd803-5b55-4385-a693-8c6f682079f9))
  (pad "48" smd roundrect (at -18.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp adeaf18b-9910-4a12-b76c-e7ca6c89512b))
  (pad "49" smd roundrect (at -18 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp ff04e317-a0f1-4a88-89e8-070349c20f4c))
  (pad "50" smd roundrect (at -17.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 3247d6b9-6a33-4829-9a55-199cbba77b28))
  (pad "51" smd roundrect (at -17.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 8c16d0db-d8f5-4e96-b466-9df6703a1982))
  (pad "52" smd roundrect (at -17.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 4b17abb7-cf81-4a94-b6e6-d50e78db2ca3))
  (pad "53" smd roundrect (at -17 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp e1a2ea79-3b93-4533-b9b1-3899a3b2016c))
  (pad "54" smd roundrect (at -16.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 044c3279-7c53-4603-aacd-9f3df887c94c))
  (pad "55" smd roundrect (at -16.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp a9340d67-8bae-4ba2-a241-9078ba2ecef5))
  (pad "56" smd roundrect (at -16.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp aee00d2c-1974-4110-9b03-85eb50089894))
  (pad "57" smd roundrect (at -16 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 81c830df-92dc-434f-abe9-9c1d866dcfac))
  (pad "58" smd roundrect (at -15.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 0a5b4c20-7fb8-4dd7-a0a2-5f7b50412113))
  (pad "59" smd roundrect (at -15.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 6edef66d-126b-4e3c-8011-f2bae7fc235d))
  (pad "60" smd roundrect (at -15.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp ec1ad926-031c-4014-b97d-61699ed073fc))
  (pad "61" smd roundrect (at -15 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 2dca0ad4-3abf-4e9c-a16b-719b5aaacaa7))
  (pad "62" smd roundrect (at -14.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 31c55383-bcab-4576-9653-dc08ba8e0b06))
  (pad "63" smd roundrect (at -14.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp df81a7fd-5d40-40d6-99f9-f9ddb8509090))
  (pad "64" smd roundrect (at -14.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 49d4aaab-fb2a-4c91-a16c-894dd885c00e))
  (pad "65" smd roundrect (at -14 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 5eb5dc0f-696d-48a0-b635-5113ae474ec5))
  (pad "66" smd roundrect (at -13.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 0d826515-0aca-4e97-b5f2-ec148ae2ea83))
  (pad "67" smd roundrect (at -13.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 6dd55789-09a8-448f-ae65-a6e584fb0d4a))
  (pad "68" smd roundrect (at -13.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 87ce2d97-c504-4b55-88b7-1892854a14ca))
  (pad "69" smd roundrect (at -13 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 1d3e8c92-bfcb-4749-bcee-45de631ebc7c))
  (pad "70" smd roundrect (at -12.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp d0209ba1-6d3f-4ae7-9113-cfcec6ce3195))
  (pad "71" smd roundrect (at -12.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 11909816-f82b-423c-ba65-385c9c138079))
  (pad "72" smd roundrect (at -12.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp a1ed484b-c2df-442f-b599-899661f9959f))
  (pad "73" smd roundrect (at -12 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp f7c6a268-77cc-4621-8723-b97d08afdacf))
  (pad "74" smd roundrect (at -11.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 7c1e8f7d-d97b-4104-a883-f297969378d3))
  (pad "75" smd roundrect (at -11.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 95e43cd0-da6f-44f3-806d-bf2f3637cc9f))
  (pad "76" smd roundrect (at -11.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 25bbca30-df79-49dc-8de9-3fa32c438314))
  (pad "77" smd roundrect (at -11 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 327ac552-0bf5-4172-810e-9a3950e49711))
  (pad "78" smd roundrect (at -10.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 5a81d19e-c430-483d-8cdf-ea660dded553))
  (pad "79" smd roundrect (at -10.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 86f680fa-2d3a-4c85-9267-17b3a2576f19))
  (pad "80" smd roundrect (at -10.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 4d5e85ef-b4a5-4943-bebb-18c2b1d2cc3f))
  (pad "81" smd roundrect (at -10 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 274f5a43-42fb-46b7-9ecd-d5e78f9dca26))
  (pad "82" smd roundrect (at -9.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 584e759a-4851-458a-b4c0-f090d5f4ca0c))
  (pad "83" smd roundrect (at -9.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 1cca3b9c-da89-49fc-af18-80be654779d4))
  (pad "84" smd roundrect (at -9.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp c8536e38-fd8c-47fc-9676-b94a7470130a))
  (pad "85" smd roundrect (at -9 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp f02ca0bc-f3f5-419e-aa9b-6fa182f66818))
  (pad "86" smd roundrect (at -8.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 9fcb7e6b-4796-42ea-8e16-d2dbc66999e2))
  (pad "87" smd roundrect (at -8.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 66db36bb-d878-4946-bf31-a3373aaede39))
  (pad "88" smd roundrect (at -8.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 07cf7358-268b-4266-8a8d-3d50196f0948))
  (pad "89" smd roundrect (at -8 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp d3541060-bf4f-4957-8644-0d2d8443f17f))
  (pad "90" smd roundrect (at -7.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 29b0fcf7-d018-40a1-a2f0-8938ca2db47a))
  (pad "91" smd roundrect (at -7.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp f26b6640-35d5-4652-96d9-0b7e41f02ff8))
  (pad "92" smd roundrect (at -7.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp d7c89a5f-e26f-4919-bcc3-f1ec170e45e3))
  (pad "93" smd roundrect (at -7 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 64d45944-0ba0-4740-b8ac-f53f42fae6ef))
  (pad "94" smd roundrect (at -6.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 834e21b1-bfae-41c0-b29d-35fe8a88484f))
  (pad "95" smd roundrect (at -6.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp a99a5466-8f98-451a-ae3c-b03f61e15ba1))
  (pad "96" smd roundrect (at -6.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 3e7ffaa0-4809-48a2-9545-e63660e193ab))
  (pad "97" smd roundrect (at -6 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp d7960f60-db53-4932-bdcd-5acbe99c6ab9))
  (pad "98" smd roundrect (at -5.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp d264fb78-5ab7-4a50-b749-7baed53be04b))
  (pad "99" smd roundrect (at -5.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 1b90eab7-2e9b-43de-8878-fafc6556807b))
  (pad "100" smd roundrect (at -5.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp b7239960-e0de-425a-8529-334b6aa17b93))
  (pad "101" smd roundrect (at -5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 6e808af3-a37b-4d3c-accb-d2ed8d7b6f62))
  (pad "102" smd roundrect (at -4.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 737839fd-d914-4651-9326-dc037213ac96))
  (pad "103" smd roundrect (at -4.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp d3fbef7d-12f0-4c8c-893e-48cff37bfa93))
  (pad "104" smd roundrect (at -4.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 8526300c-3aeb-4b63-b9fb-1bc9e3d2e798))
  (pad "105" smd roundrect (at -4 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 3b30a1e2-314a-479c-aedf-76f979d5802a))
  (pad "106" smd roundrect (at -3.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp cc211d81-bd05-4d81-bf8e-4a40a8c89163))
  (pad "107" smd roundrect (at -3.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp c5110aef-d3d4-4db1-ab99-b00d81239305))
  (pad "108" smd roundrect (at -3.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 83b318f9-d3fb-4089-bc72-6ba7a201b8eb))
  (pad "109" smd roundrect (at -3 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp cabee6d1-05e1-4efa-af47-7dba9e86d110))
  (pad "110" smd roundrect (at -2.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 529da192-79b7-4ec6-8bbf-320d3206a74a))
  (pad "111" smd roundrect (at -2.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 4e9ef0ce-eb2d-43ba-8d6c-06b272050408))
  (pad "112" smd roundrect (at -2.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 1d82fdda-d41e-4a17-aac9-77d340387120))
  (pad "113" smd roundrect (at -2 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp dff3274f-0587-464f-816b-a09a0f2adc0e))
  (pad "114" smd roundrect (at -1.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 7682ee81-aadb-4a95-a71f-3919ff79aaff))
  (pad "115" smd roundrect (at -1.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp b585c119-1b5a-4671-9734-9214efd57de3))
  (pad "116" smd roundrect (at -1.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 6b3489e5-4c84-4fc0-8ca2-d2dacf3bf80a))
  (pad "117" smd roundrect (at -1 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 9b9b068b-d2a0-49e0-b069-7e4d32ad391c))
  (pad "118" smd roundrect (at -0.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 44c2c4c5-e8ca-48e1-84a5-523f2c66886e))
  (pad "119" smd roundrect (at -0.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp e6dccbcd-1beb-471d-a0fc-57cffaab4710))
  (pad "120" smd roundrect (at -0.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 269d50d0-d632-4d02-8919-161cc638c138))
  (pad "121" smd roundrect (at 0 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp e00ef24c-9381-4524-a5a0-8f2be611cdaf))
  (pad "122" smd roundrect (at 0.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp aceec963-c562-4454-88f1-b2f67ccce8db))
  (pad "123" smd roundrect (at 0.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 81f463d9-2585-4653-a0d1-d58f3aea1f91))
  (pad "124" smd roundrect (at 0.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 8aa1ab49-1905-4de4-b1c9-276ac98981d7))
  (pad "125" smd roundrect (at 1 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 86c148e6-b862-47a2-9ef4-8771294af875))
  (pad "133" smd roundrect (at 3 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 8c682dcb-54bf-40bc-b0f1-97cd8d9fd426))
  (pad "134" smd roundrect (at 3.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 02e78795-5497-438e-8fa0-59f5d4fbe164))
  (pad "135" smd roundrect (at 3.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 0ce5487d-6811-4c8c-aa7a-7eee68e3197b))
  (pad "136" smd roundrect (at 3.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp a4e4ab8d-ce3f-42d2-b0dd-8104c3c24d4b))
  (pad "137" smd roundrect (at 4 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 6ac180c8-0955-44f2-a6dc-cdb4d7072659))
  (pad "138" smd roundrect (at 4.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp e03f69f0-36bb-4826-af3c-1ea5f3e14b8e))
  (pad "139" smd roundrect (at 4.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 0345f29c-ba5b-45e8-ad35-9ca3768accd3))
  (pad "140" smd roundrect (at 4.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 1391a768-d07e-4340-aec2-683e3d26f1d5))
  (pad "141" smd roundrect (at 5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp ce769f3a-a0f5-4039-b5c7-2417d2dff7e5))
  (pad "142" smd roundrect (at 5.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 889c69a0-57d9-4afb-a6e1-b0795d31eab6))
  (pad "143" smd roundrect (at 5.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 88430252-f10f-4215-abec-61106a81a856))
  (pad "144" smd roundrect (at 5.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 491833f8-4ecd-47e7-89da-5227bc442e5f))
  (pad "145" smd roundrect (at 6 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 5b651ed6-97d6-4904-b2ca-55655b1be879))
  (pad "146" smd roundrect (at 6.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 5530352e-b0b8-4e64-88b8-69eb6ab43c14))
  (pad "147" smd roundrect (at 6.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 9dd49053-8a61-4006-b3ab-65cd05b31633))
  (pad "148" smd roundrect (at 6.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 1b054b91-5521-4d97-9a13-5755f715490e))
  (pad "149" smd roundrect (at 7 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 49e097c9-44be-40b8-83d1-029247d54407))
  (pad "150" smd roundrect (at 7.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 9bcff072-df4a-4588-8a25-0b2f611acadd))
  (pad "151" smd roundrect (at 7.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 847bf3cc-11c2-489b-9bb2-0ccefa2be402))
  (pad "152" smd roundrect (at 7.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 164f2ea1-763b-4190-b874-09053647bd7b))
  (pad "153" smd roundrect (at 8 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 07277a05-9723-4650-b5b2-94843e7e4de5))
  (pad "154" smd roundrect (at 8.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 16c5466e-a5ec-485a-b55e-14322a9bd625))
  (pad "155" smd roundrect (at 8.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 2d442907-8abe-413b-8061-04fdb9cf7dce))
  (pad "156" smd roundrect (at 8.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp fe5a6920-8d53-4343-b28d-71170bc57f67))
  (pad "157" smd roundrect (at 9 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 8e4e4825-47b3-4ca8-8a88-3901606d0963))
  (pad "158" smd roundrect (at 9.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 0c9acae9-84b1-48a8-aefd-69b58867166c))
  (pad "159" smd roundrect (at 9.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp c775c947-9913-4e96-a816-11569cda884c))
  (pad "160" smd roundrect (at 9.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 41391b8b-9bfc-489c-957d-3311e00e93fa))
  (pad "161" smd roundrect (at 10 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 2fb50b87-4776-4a44-b8a0-0ae04ec0a6d1))
  (pad "162" smd roundrect (at 10.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp dc78ff34-cda6-4314-b622-bda31cb455f3))
  (pad "163" smd roundrect (at 10.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 1247a5d0-17cb-4081-b4ad-0701d3073125))
  (pad "164" smd roundrect (at 10.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 8a0f2b4d-a9b9-466f-812a-e0884f5be9fa))
  (pad "165" smd roundrect (at 11 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 8cd58143-4fca-4949-8042-7a645cea8f86))
  (pad "166" smd roundrect (at 11.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 4dd24c1b-db3b-4821-8d4a-6c81941faf22))
  (pad "167" smd roundrect (at 11.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp d1bbb208-bac6-49d1-8f70-765905b3c97b))
  (pad "168" smd roundrect (at 11.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 91f04580-f61a-4d40-8abf-46724b78bf98))
  (pad "169" smd roundrect (at 12 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 3e0869b8-0815-4272-a015-516a29a67ced))
  (pad "170" smd roundrect (at 12.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 81c3bfd7-e768-43f6-b2c2-f12d3c801d5f))
  (pad "171" smd roundrect (at 12.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp b21ec5e8-bd57-4930-aa08-cf348ba796f5))
  (pad "172" smd roundrect (at 12.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 1586abdb-5b32-4c32-8828-e19e57c5879d))
  (pad "173" smd roundrect (at 13 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 9fde8086-3f1e-440b-954c-dbf1b5a75bf3))
  (pad "174" smd roundrect (at 13.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 952c5834-2ae4-456f-b926-76b0e01a19a7))
  (pad "175" smd roundrect (at 13.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 017d9157-9512-4d3f-8f48-f897d0bcacda))
  (pad "176" smd roundrect (at 13.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 180b8850-5998-4454-896c-97bb2789995e))
  (pad "177" smd roundrect (at 14 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 644db7db-a227-45e2-9c23-5308cd63659f))
  (pad "178" smd roundrect (at 14.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 2fc702bd-94bc-481a-a943-7154081d11c9))
  (pad "179" smd roundrect (at 14.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp b21ba674-56fe-4090-89e9-f82e8595eead))
  (pad "180" smd roundrect (at 14.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 9a9ab4ae-15af-4f8a-b5e0-11c76f53b49a))
  (pad "181" smd roundrect (at 15 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp f660773e-3377-4c2d-949f-f3eeb7a7372f))
  (pad "182" smd roundrect (at 15.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 846bdb91-2043-4643-bbf9-7522968d15a6))
  (pad "183" smd roundrect (at 15.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp f6c9d482-2527-42f0-993f-d9caaf8fce39))
  (pad "184" smd roundrect (at 15.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp ddbe7bf7-d801-4264-82f2-24c83864ccf2))
  (pad "185" smd roundrect (at 16 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 01595509-8c41-4a9d-9f32-90e3dd6d0ec6))
  (pad "186" smd roundrect (at 16.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 0f68551d-2065-41d3-81c6-7a415615c11d))
  (pad "187" smd roundrect (at 16.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 7247f39a-8e61-4ee9-90df-82b536b7728b))
  (pad "188" smd roundrect (at 16.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 3351bd34-785a-4b17-ac23-a5b9189d2bfb))
  (pad "189" smd roundrect (at 17 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp c466d828-09ee-4720-92ad-f71dd90de7a6))
  (pad "190" smd roundrect (at 17.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp cfd849c3-edaf-4caf-92cb-8c16e0db8ac5))
  (pad "191" smd roundrect (at 17.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 68f93258-1042-494e-ad4b-52c3fb5ee941))
  (pad "192" smd roundrect (at 17.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 8f1a080e-5f75-4ab6-9fb4-3c3e0ac42dd2))
  (pad "193" smd roundrect (at 18 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 72443bfb-2280-49d5-870d-aba6ac3b7de6))
  (pad "194" smd roundrect (at 18.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 0b6c6691-f19f-467a-943b-13a6873e0b45))
  (pad "195" smd roundrect (at 18.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 4eb92464-d8a3-45db-bbc3-a3ab3f46bc14))
  (pad "196" smd roundrect (at 18.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 8785fb72-ab96-438e-9052-68af3b44113f))
  (pad "197" smd roundrect (at 19 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp e751c57d-6d61-4044-a920-20b2b809064d))
  (pad "198" smd roundrect (at 19.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp ee01d062-cbf4-4622-84cd-2aa087be949f))
  (pad "199" smd roundrect (at 19.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 156cf939-cad3-4951-b221-353c897f14a5))
  (pad "200" smd roundrect (at 19.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 65d553cb-b343-4d05-ab30-b7891c070c02))
  (pad "201" smd roundrect (at 20 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 451b718e-48b3-4e86-ab14-569119428aee))
  (pad "202" smd roundrect (at 20.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp f6f7ab5e-99fe-4558-acae-260520cf4b15))
  (pad "203" smd roundrect (at 20.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp b9cc38d9-46b7-4e5b-b5bf-0689c5e1a773))
  (pad "204" smd roundrect (at 20.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 1c6685ca-b98b-4f5e-897f-faa2c0d25b09))
  (pad "205" smd roundrect (at 21 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 20b5021e-ba2f-4267-8c22-890ae579853c))
  (pad "206" smd roundrect (at 21.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 86af1a7f-0eec-454f-b8d4-2313562c65e2))
  (pad "207" smd roundrect (at 21.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 152fa555-cd06-48e8-8eb1-2b4afe43c830))
  (pad "208" smd roundrect (at 21.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 3b262a2d-4854-4d07-9d72-c7f103c54c01))
  (pad "209" smd roundrect (at 22 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp e9f1398c-278a-498d-a8b4-80e1312f99fb))
  (pad "210" smd roundrect (at 22.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp bd39dd3b-00f4-4b08-990d-6b0df3f81c51))
  (pad "211" smd roundrect (at 22.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 51fc43e6-04cb-4519-85ba-781bc1f35350))
  (pad "212" smd roundrect (at 22.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 5cd2e850-0476-4a33-8c95-8f57d58dc816))
  (pad "213" smd roundrect (at 23 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 448d3597-75c1-4406-b8c1-c4c585f7300a))
  (pad "214" smd roundrect (at 23.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 57072ae1-ceab-495b-8f1d-485879024f8c))
  (pad "215" smd roundrect (at 23.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 718a1f67-2a89-4352-8e9f-70cafc340345))
  (pad "216" smd roundrect (at 23.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 953f4794-5f1f-418a-8d10-7880a1f03b51))
  (pad "217" smd roundrect (at 24 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp cbe13720-a71b-417d-8e46-3bd6e6940dc7))
  (pad "218" smd roundrect (at 24.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp d7af158c-e030-40ae-9e65-dda0da54fa8b))
  (pad "219" smd roundrect (at 24.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp c00627a8-b63c-4497-9edc-dc7eb700b20e))
  (pad "220" smd roundrect (at 24.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp dbcc0ec5-f614-4ad5-9cee-cd1b351ef9c9))
  (pad "221" smd roundrect (at 25 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 4c28408d-9311-4195-869c-eeebc1140179))
  (pad "222" smd roundrect (at 25.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 92dbbef1-df42-45d0-ad1a-61bcc8304413))
  (pad "223" smd roundrect (at 25.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 8e9ff5e1-46a1-4130-a83e-6c58699ccb0e))
  (pad "224" smd roundrect (at 25.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 7e5dec12-bb1b-40ca-83ed-3ccef09e6a9d))
  (pad "225" smd roundrect (at 26 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 3dd7905b-6bae-41c5-8936-603936573aa2))
  (pad "226" smd roundrect (at 26.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 837d6f80-3e86-4882-bd94-8c6817db4adf))
  (pad "227" smd roundrect (at 26.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 7a1bd10e-48a6-4692-a614-b8b2507c798d))
  (pad "228" smd roundrect (at 26.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp c16e934e-4f63-4038-a667-a09a860024e1))
  (pad "229" smd roundrect (at 27 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 28ecd8de-02dc-4b56-9940-9c2a4e558fdf))
  (pad "230" smd roundrect (at 27.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 20f6cade-6772-4b6c-b127-28d4e61eb317))
  (pad "231" smd roundrect (at 27.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp caa8b1bf-698b-4ccf-a18a-5ab7c0e9b89d))
  (pad "232" smd roundrect (at 27.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp ffbb7b99-df0b-4a11-85e5-36c6c3ca419c))
  (pad "233" smd roundrect (at 28 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 24811466-a8ea-4406-b2ea-38bf4bf315c2))
  (pad "234" smd roundrect (at 28.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 36d46a4e-d33f-4017-92ce-e312a3643520))
  (pad "235" smd roundrect (at 28.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp fc34b3cb-285d-4aff-9f5b-4e30bf1ac540))
  (pad "236" smd roundrect (at 28.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp aeecaa82-22b6-42fe-8262-2f152b25731c))
  (pad "237" smd roundrect (at 29 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 09a04934-a0ff-42e4-a39b-a191cc169394))
  (pad "238" smd roundrect (at 29.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp e427a985-302c-4e9d-98cb-9be8dafba665))
  (pad "239" smd roundrect (at 29.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 7b1e4eb2-6947-47a6-acdf-4c04db77da14))
  (pad "240" smd roundrect (at 29.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp c655de0b-1e4a-4c6b-9697-19dbccfbf7a5))
  (pad "241" smd roundrect (at 30 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 50edce64-128c-48fb-84ab-6536ddd742a4))
  (pad "242" smd roundrect (at 30.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp d65a2a38-2c1f-485c-b9d3-c143dd94fc41))
  (pad "243" smd roundrect (at 30.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp eb2720a7-b4be-4043-b721-ea0f0cbaee81))
  (pad "244" smd roundrect (at 30.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 224cce63-5c28-47d2-9c9b-f8040a2bb5be))
  (pad "245" smd roundrect (at 31 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp a7775ccf-fe3b-4e65-b479-9004fd5fb580))
  (pad "246" smd roundrect (at 31.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp b69ae63f-8f1d-49bf-8db3-fe5fc9772caa))
  (pad "247" smd roundrect (at 31.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp baf94c2f-56e1-4a8e-aa62-d636e09bcd21))
  (pad "248" smd roundrect (at 31.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp ae7229e1-609d-4279-bc89-09b30bc98685))
  (pad "249" smd roundrect (at 32 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 171bed1c-b434-49e3-97f1-23855b194f52))
  (pad "250" smd roundrect (at 32.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp d4e7dba2-e650-4fdc-994c-c522010a94b0))
  (pad "251" smd roundrect (at 32.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp a02eb5fc-a1b5-47c3-8332-505edf7dfc59))
  (pad "252" smd roundrect (at 32.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp ef9d9c9e-e338-4924-b0bd-000913a768a4))
  (pad "253" smd roundrect (at 33 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 05e222a8-eb2f-4241-a975-71c917d53b5e))
  (pad "254" smd roundrect (at 33.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp a611a67a-cb66-47b6-a89a-011729a51067))
  (pad "255" smd roundrect (at 33.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 28e02c58-b6df-4638-8ff7-f80531ba7b41))
  (pad "256" smd roundrect (at 33.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 11a6331c-175d-4aa2-84e5-59580f69a5be))
  (pad "257" smd roundrect (at 34 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 26a91a11-cf1c-4138-bfd2-7ba657745cdc))
  (pad "258" smd roundrect (at 34.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp e8b9ff03-812a-4076-aad9-c7707fd57237))
  (pad "259" smd roundrect (at 34.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 77c42690-cb41-481e-b6f2-837911615731))
  (pad "260" smd roundrect (at 34.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 964853c6-ecc5-4c4e-8646-f59a45e91c1d))
  (pad "261" smd roundrect (at 35 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 452a5c49-4e08-48db-8dc6-8d198bb19607))
  (pad "262" smd roundrect (at 35.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 305f6359-75c3-4a02-8265-c8379ccfaa26))
  (pad "263" smd roundrect (at 35.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp e8d3f7ff-1872-4bb9-a208-4b62239ac14d))
  (pad "264" smd roundrect (at 35.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp a6b89808-b140-4b69-9f08-83a5038206b7))
  (pad "265" smd roundrect (at 36 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp e6065940-e50f-48f9-ad36-7fc537322394))
  (pad "266" smd roundrect (at 36.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 5c85a3a7-0e20-4a8a-901d-53340f8eed09))
  (pad "267" smd roundrect (at 36.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 8a5f6b01-5a15-4a83-86bb-c00e4bbcb699))
  (pad "268" smd roundrect (at 36.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp eee1d6bf-b7de-45b2-8289-0dce7af4aaf9))
  (pad "269" smd roundrect (at 37 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 1d2672b8-2516-4037-b152-ca36531f55f7))
  (pad "270" smd roundrect (at 37.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 4823fd38-055c-4781-a76d-500a1761f4ac))
  (pad "271" smd roundrect (at 37.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 3e01ed7b-c04f-495f-a750-b5dc5413ecfb))
  (pad "272" smd roundrect (at 37.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp c0a4e0d6-954a-42b3-ba7b-54023707ad00))
  (pad "273" smd roundrect (at 38 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 5da2445c-8abe-4aa4-8484-a89ec37cf6bd))
  (pad "274" smd roundrect (at 38.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp a8c9c475-524e-41d4-8ac5-1b596eaffeb2))
  (pad "275" smd roundrect (at 38.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp e6727d07-df35-42f1-a5cf-79fe85363b1c))
  (pad "276" smd roundrect (at 38.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp a171bcba-d8c8-4811-a920-32af4f81c216))
  (pad "277" smd roundrect (at 39 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 18851b1d-4587-4ba0-a4c7-22c03b97a5df))
  (pad "278" smd roundrect (at 39.25 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 55a831cb-540d-438e-aa67-d6aef55bfee6))
  (pad "279" smd roundrect (at 39.5 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 2b8c9823-60be-4cbe-9675-87e0dab87523))
  (pad "280" smd roundrect (at 39.75 -3.5) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp 897db5dd-ff1c-4ce1-b987-d28533f3f10a))
  (pad "281" smd roundrect (at 40 3.75) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125) (tstamp a45a0e9e-812d-480f-acac-978f654975fb))
  (pad "E1" smd roundrect (at -37.75 3.75) (size 4.82 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.05)
    (zone_connect 2) (tstamp ad838f87-3c65-429a-a76d-39a5c9728c6a))
  (pad "E2" smd roundrect (at -37.5 -3.5) (size 4.82 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.05)
    (zone_connect 2) (tstamp 38c2ffad-c41b-436d-a42e-03f4b23dbb8b))
  (pad "E3" smd roundrect (at -32.75 3.75) (size 4.82 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.05)
    (zone_connect 2) (tstamp 01759697-8d66-46e8-b331-0bd879a6e9b6))
  (pad "E4" smd roundrect (at -32.5 -3.5) (size 4.82 2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.05)
    (zone_connect 2) (tstamp 20748ca7-5782-4652-bd99-12d554ba37c8))
)
