(module "QFN-24-1EP_5x5mm_P0.65mm_EP3.2x3.2mm" (layer F.Cu) (tedit 5D7DD242)
  (descr "QFN, 24 Pin (https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-qfn/(UH24)%20QFN%2005-08-1747%20Rev%20A.pdf), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
  (tags "QFN DFN_QFN")
  (attr smd)
  (fp_text reference "U1" (at 0 -3.475) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text value "Broadcom_AEAT-8800-Q24" (at 0 3.82 -180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user "%R" (at 0 0 -180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 3.12 -3.12) (end -3.12 -3.12) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.12 3.12) (end 3.12 -3.12) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.12 3.12) (end 3.12 3.12) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.12 -3.12) (end -3.12 3.12) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.5 -1.5) (end -1.5 -2.5) (layer F.Fab) (width 0.1))
  (fp_line (start -2.5 2.5) (end -2.5 -1.5) (layer F.Fab) (width 0.1))
  (fp_line (start 2.5 2.5) (end -2.5 2.5) (layer F.Fab) (width 0.1))
  (fp_line (start 2.5 -2.5) (end 2.5 2.5) (layer F.Fab) (width 0.1))
  (fp_line (start -1.5 -2.5) (end 2.5 -2.5) (layer F.Fab) (width 0.1))
  (fp_line (start -2.05 -2.625) (end -2.625 -2.625) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.625 2.625) (end 2.625 2.05) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.05 2.625) (end 2.625 2.625) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.625 2.625) (end -2.625 2.05) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.05 2.625) (end -2.625 2.625) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.625 -2.625) (end 2.625 -2.05) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.05 -2.625) (end 2.625 -2.625) (layer F.SilkS) (width 0.15))
  (pad "2" smd roundrect (at -1.625 -2.5 270) (size 0.55 0.3) (layers "F.Paste") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at -0.975 -2.5 270) (size 0.55 0.3) (layers "F.Paste") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at -0.325 -2.5 270) (size 0.55 0.3) (layers "F.Paste") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at 0.325 -2.5 270) (size 0.55 0.3) (layers "F.Paste") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at 0.975 -2.5 270) (size 0.55 0.3) (layers "F.Paste") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at 1.625 -2.5 270) (size 0.55 0.3) (layers "F.Paste") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at 2.5 -1.625 180) (size 0.55 0.3) (layers "F.Paste") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at 2.5 -0.975 180) (size 0.55 0.3) (layers "F.Paste") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at 2.5 -0.325 180) (size 0.55 0.3) (layers "F.Paste") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at 2.5 0.325 180) (size 0.55 0.3) (layers "F.Paste") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at 2.5 0.975 180) (size 0.55 0.3) (layers "F.Paste") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at 2.5 1.625 180) (size 0.55 0.3) (layers "F.Paste") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at 1.625 2.5 90) (size 0.55 0.3) (layers "F.Paste") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at 0.975 2.5 90) (size 0.55 0.3) (layers "F.Paste") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at 0.325 2.5 90) (size 0.55 0.3) (layers "F.Paste") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at -0.325 2.5 90) (size 0.55 0.3) (layers "F.Paste") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at -0.975 2.5 90) (size 0.55 0.3) (layers "F.Paste") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at -1.625 2.5 90) (size 0.55 0.3) (layers "F.Paste") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at -2.5 1.625) (size 0.55 0.3) (layers "F.Paste") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at -2.5 0.975) (size 0.55 0.3) (layers "F.Paste") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at -2.5 0.325) (size 0.55 0.3) (layers "F.Paste") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at -2.5 -0.325) (size 0.55 0.3) (layers "F.Paste") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at -2.5 -1.625) (size 0.55 0.3) (layers "F.Paste") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at -2.5 -0.975) (size 0.55 0.3) (layers "F.Paste") (roundrect_rratio 0.25))
  (pad "25" smd roundrect (at 0 0) (size 3.2 3.2) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.078125))
  (pad "" smd roundrect (at -0.8 -0.8) (size 1.29 1.29) (layers "F.Paste") (roundrect_rratio 0.193798))
  (pad "" smd roundrect (at -0.8 0.8) (size 1.29 1.29) (layers "F.Paste") (roundrect_rratio 0.193798))
  (pad "" smd roundrect (at 0.8 -0.8) (size 1.29 1.29) (layers "F.Paste") (roundrect_rratio 0.193798))
  (pad "" smd roundrect (at 0.8 0.8) (size 1.29 1.29) (layers "F.Paste") (roundrect_rratio 0.193798))
  (pad "1" smd custom (at -2.3625 -1.625) (size 0.193934 0.193934) (layers "F.Cu" "F.Mask")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.4375 -0.075) (xy 0.331434 -0.075) (xy 0.4375 0.031066) (xy 0.4375 0.075) (xy -0.4375 0.075)
) (width 0.15))
    ))
  (pad "2" smd roundrect (at -2.3625 -0.975) (size 1.025 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25))
  (pad "3" smd roundrect (at -2.3625 -0.325) (size 1.025 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25))
  (pad "4" smd roundrect (at -2.3625 0.325) (size 1.025 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25))
  (pad "5" smd roundrect (at -2.3625 0.975) (size 1.025 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25))
  (pad "6" smd custom (at -2.3625 1.625) (size 0.193934 0.193934) (layers "F.Cu" "F.Mask")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.4375 -0.075) (xy 0.4375 -0.075) (xy 0.4375 -0.031066) (xy 0.331434 0.075) (xy -0.4375 0.075)
) (width 0.15))
    ))
  (pad "7" smd custom (at -1.625 2.3625) (size 0.193934 0.193934) (layers "F.Cu" "F.Mask")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.075 -0.331434) (xy 0.031066 -0.4375) (xy 0.075 -0.4375) (xy 0.075 0.4375) (xy -0.075 0.4375)
) (width 0.15))
    ))
  (pad "8" smd roundrect (at -0.975 2.3625) (size 0.3 1.025) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25))
  (pad "9" smd roundrect (at -0.325 2.3625) (size 0.3 1.025) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25))
  (pad "10" smd roundrect (at 0.325 2.3625) (size 0.3 1.025) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25))
  (pad "11" smd roundrect (at 0.975 2.3625) (size 0.3 1.025) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25))
  (pad "12" smd custom (at 1.625 2.3625) (size 0.193934 0.193934) (layers "F.Cu" "F.Mask")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.075 -0.4375) (xy -0.031066 -0.4375) (xy 0.075 -0.331434) (xy 0.075 0.4375) (xy -0.075 0.4375)
) (width 0.15))
    ))
  (pad "13" smd custom (at 2.3625 1.625) (size 0.193934 0.193934) (layers "F.Cu" "F.Mask")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.4375 -0.075) (xy 0.4375 -0.075) (xy 0.4375 0.075) (xy -0.331434 0.075) (xy -0.4375 -0.031066)
) (width 0.15))
    ))
  (pad "14" smd roundrect (at 2.3625 0.975) (size 1.025 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25))
  (pad "15" smd roundrect (at 2.3625 0.325) (size 1.025 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25))
  (pad "16" smd roundrect (at 2.3625 -0.325) (size 1.025 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25))
  (pad "17" smd roundrect (at 2.3625 -0.975) (size 1.025 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25))
  (pad "18" smd custom (at 2.3625 -1.625) (size 0.193934 0.193934) (layers "F.Cu" "F.Mask")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.4375 0.031066) (xy -0.331434 -0.075) (xy 0.4375 -0.075) (xy 0.4375 0.075) (xy -0.4375 0.075)
) (width 0.15))
    ))
  (pad "19" smd custom (at 1.625 -2.3625) (size 0.193934 0.193934) (layers "F.Cu" "F.Mask")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.075 -0.4375) (xy 0.075 -0.4375) (xy 0.075 0.331434) (xy -0.031066 0.4375) (xy -0.075 0.4375)
) (width 0.15))
    ))
  (pad "20" smd roundrect (at 0.975 -2.3625) (size 0.3 1.025) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25))
  (pad "21" smd roundrect (at 0.325 -2.3625) (size 0.3 1.025) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25))
  (pad "22" smd roundrect (at -0.325 -2.3625) (size 0.3 1.025) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25))
  (pad "23" smd roundrect (at -0.975 -2.3625) (size 0.3 1.025) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25))
  (pad "24" smd custom (at -1.625 -2.3625) (size 0.193934 0.193934) (layers "F.Cu" "F.Mask")
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.075 -0.4375) (xy 0.075 -0.4375) (xy 0.075 0.4375) (xy 0.031066 0.4375) (xy -0.075 0.331434)
) (width 0.15))
    ))
  (model "${KICAD7_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-24-1EP_5x5mm_P0.65mm_EP3.2x3.2mm.wrl"
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
