(footprint "Heatsink_44x44x12mm_M2_40x40mm" (version 20220427) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -21 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp aad085f0-6deb-4309-95a9-cc04dc00c910)
  )
  (fp_text value "Heatsink_44x44x12mm_M2_40x40mm" (at 0 19 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d24218ad-25c9-45d3-aad8-16ba3a4d63d1)
  )
  (fp_text user "${REFERENCE}" (at 0 20.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4fe9ac5f-eb47-4fe7-bf44-d9f1bba94165)
  )
  (fp_line (start -22 -22) (end -20 -22)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 61aa6036-74f7-4d4f-b2ed-b77f85655836))
  (fp_line (start -22 -20) (end -22 -22)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 69ea8297-7d4b-43ef-9874-22c56e50192b))
  (fp_line (start -22 20) (end -22 22)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 14d27fda-1825-4836-a753-0e4fb08a461c))
  (fp_line (start -22 22) (end -20 22)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp c8e51e0a-c97d-47f9-b310-77786551d573))
  (fp_line (start 20 -22) (end 22 -22)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 227ee017-7ca8-4ba8-b0bd-d4c754298309))
  (fp_line (start 20 22) (end 22 22)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 32b8cc6f-2367-4137-b33f-ccd698c91b9a))
  (fp_line (start 22 -22) (end 22 -20)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp d53ee3e6-25d8-4769-872f-467514c9e194))
  (fp_line (start 22 22) (end 22 20)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 465095af-59a0-487a-9524-e3475dbdb9c8))
  (fp_rect (start -22 -22) (end 22 22)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 01bb1768-f0df-48cd-b97c-baa21a8003ce))
  (pad "1" thru_hole circle (at -20 -20) (size 2.5 2.5) (drill 2.2) (layers *.Cu *.Mask) (remove_unused_layers) (tstamp 7cb0d65a-7ae1-41a3-b359-9e7857bf52f9))
  (pad "1" connect circle (at -20 -20) (size 4.2 4.2) (layers "B.Cu" "B.Mask") (tstamp 432c9272-67d6-43c4-b10b-cddcba85f37b))
  (pad "1" thru_hole circle (at -20 20) (size 2.5 2.5) (drill 2.2) (layers *.Cu *.Mask) (remove_unused_layers) (tstamp de1f0a23-eb08-465f-8acb-262038183456))
  (pad "1" connect circle (at -20 20) (size 4.2 4.2) (layers "B.Cu" "B.Mask") (tstamp dfc04629-12e2-4b26-a1b2-0f31c416303f))
  (pad "1" thru_hole circle (at 20 -20) (size 2.5 2.5) (drill 2.2) (layers *.Cu *.Mask) (remove_unused_layers) (tstamp 1759a289-3bf4-477e-8c43-d07216cbe4c3))
  (pad "1" connect circle (at 20 -20) (size 4.2 4.2) (layers "B.Cu" "B.Mask") (tstamp 163b0871-24b6-4f8d-97ae-c689cc91b0c3))
  (pad "1" thru_hole circle (at 20 20) (size 2.5 2.5) (drill 2.2) (layers *.Cu *.Mask) (remove_unused_layers) (tstamp c0eaf094-4e70-4e23-9fe0-b5835377cb72))
  (pad "1" connect circle (at 20 20) (size 4.2 4.2) (layers "B.Cu" "B.Mask") (tstamp 11d5d93b-f4d1-4a89-8036-2c96123df3aa))
  (model "${KICAD7_3DMODEL_DIR}/Heatsink.3dshapes/Heatsink 44x44x12.step"
    (offset (xyz 0 0 2.7))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
