(module "4P_3x1.75_P2.0" (layer "F.Cu") (tedit 5FB912E2)
  (property "Sheet file" "/home/stefan/Projects/Current/USBtoCANFD/USBtoCANFD.kicad_sch")
  (property "Sheet name" "")
  (attr through_hole)
  (fp_text reference "J3" (at 0 -4.525 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 625001ec-16d4-4cd0-b1eb-2e175fdde6ca)
  )
  (fp_text value "SWD" (at 2.375 0 90 unlocked) (layer "F.Fab") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 75bffcbd-9212-417f-8feb-2ca70bdd04f1)
  )
  (fp_text user "${REF}" (at -0.1 -7.175 unlocked) (layer "F.Fab") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp dca89be9-55be-4fe8-88ee-e92cc44329da)
  )
  (fp_poly (pts (xy -1.6 -3)
    (xy -1.85 -2.8)
    (xy -1.85 -3.2)) (layer "F.SilkS") (width 0) (fill yes) (tstamp d5e9a0fb-4f60-46c2-9f5a-7907c4228b78))
  (fp_line (start -1.65 -3.625) (end -1.65 3.625) (layer "F.CrtYd") (width 0.05) (tstamp 052e9df3-7964-4211-a669-d86683f63c19))
  (fp_line (start -1.25 4.025) (end 1.25 4.025) (layer "F.CrtYd") (width 0.05) (tstamp 0890f4a4-1268-474d-988d-e14f06b60568))
  (fp_line (start 1.65 3.625) (end 1.65 -3.625) (layer "F.CrtYd") (width 0.05) (tstamp 37df83c5-6c23-4d72-8bb6-1090494f5c25))
  (fp_line (start 1.25 -4.025) (end -1.25 -4.025) (layer "F.CrtYd") (width 0.05) (tstamp bc8a47c5-a3a4-46ed-b9f8-381ced57c148))
  (fp_arc (start -1.25 3.625) (end -1.65 3.625) (angle -90) (layer "F.CrtYd") (width 0.05) (tstamp 7e02d4d1-9707-43d5-83d0-633b37f19379))
  (fp_arc (start -1.25 -3.625) (end -1.25 -4.025) (angle -90) (layer "F.CrtYd") (width 0.05) (tstamp 969ee8c0-8666-489d-933c-28f3bee39422))
  (fp_arc (start 1.25 3.625) (end 1.25 4.025) (angle -90) (layer "F.CrtYd") (width 0.05) (tstamp 9eaac276-6116-4bd7-9dba-ac5ff6b6d75a))
  (fp_arc (start 1.25 -3.625) (end 1.65 -3.625) (angle -90) (layer "F.CrtYd") (width 0.05) (tstamp b65a738f-a93f-405b-8287-65fdd5286d24))
  (pad "1" connect roundrect (at 0 -3) (size 3 1.75) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.143) (tstamp d013dd43-3dbe-4e40-9269-a0e03b3e87b5))
  (pad "2" connect roundrect (at 0 -1) (size 3 1.75) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.143) (tstamp cf54a143-2dcd-4eab-ae5d-3371c2bc8116))
  (pad "3" connect roundrect (at 0 1) (size 3 1.75) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.143) (tstamp e14d551d-5f5a-42f4-85b2-63b375c5dad7))
  (pad "4" connect roundrect (at 0 3) (size 3 1.75) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.143) (tstamp 4d85e044-dd09-4bd2-b09f-421db16fdda1))
)
