(module 8P_Oval_3x1_1.25mm (layer F.Cu) (tedit 5647B8EF)
  (solder_mask_margin 0.01)
  (attr virtual)
  (fp_text reference REF** (at -5.475 0 90) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value 8P_Oval_3x1_1.25mm (at 0 2.1) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_circle (center -5.1 1.675) (end -5 1.675) (layer F.SilkS) (width 0.2))
  (pad 1 connect rect (at -4.375 0) (size 1 3) (layers F.Cu F.Mask))
  (pad 2 connect oval (at -3.125 0) (size 1 3) (layers F.Cu F.Mask))
  (pad 3 connect oval (at -1.875 0) (size 1 3) (layers F.Cu F.Mask))
  (pad 4 connect oval (at -0.625 0) (size 1 3) (layers F.Cu F.Mask))
  (pad 5 connect oval (at 0.625 0) (size 1 3) (layers F.Cu F.Mask))
  (pad 6 connect oval (at 1.875 0) (size 1 3) (layers F.Cu F.Mask))
  (pad 7 connect oval (at 3.125 0) (size 1 3) (layers F.Cu F.Mask))
  (pad 8 connect oval (at 4.375 0) (size 1 3) (layers F.Cu F.Mask))
)
