(footprint "1608_C_KA" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (tags "0603 1608 Capacitor")
  (property "LCSC" "C2286")
  (property "MFG" "KENTO")
  (property "MPN" "KT-0603R")
  (property "Sheetfile" "NeedleGripperDriver.kicad_sch")
  (property "Sheetname" "")
  (solder_mask_margin 0.02)
  (solder_paste_margin -0.03)
  (attr smd)
  (fp_text reference "D5" (at 0.95 0 unlocked) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15) bold) (justify left))
    (tstamp 7d9a38ef-641e-4b3f-be7b-7a3cdd8d5fab)
  )
  (fp_text value "24V" (at 1.05 0.6 unlocked) (layer "F.Fab")
      (effects (font (size 0.2 0.2) (thickness 0.05)) (justify left))
    (tstamp 32d1b65d-eacc-43bb-b6e6-25657a45be33)
  )
  (fp_arc (start -1.1 -0.275) (mid -1.019454 -0.469454) (end -0.825 -0.55)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 3b1202c2-0092-4bbd-93ee-a914eaa07b9f))
  (fp_arc (start -0.825 0.55) (mid -1.019454 0.469454) (end -1.1 0.275)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 2c7e661d-b671-4fc2-91b0-c461a5e3f64e))
  (fp_poly
    (pts
      (xy -1.025 -0.275)
      (xy -1.025 0.275)
      (xy -1.175 0.275)
      (xy -1.175 -0.275)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 7c5033f8-412a-47bf-b03d-5cc52aea45ea))
  (fp_poly
    (pts
      (xy 0.325 -0.475)
      (xy -0.825 -0.475)
      (xy -0.825 -0.625)
      (xy 0.325 -0.625)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 8e11eabf-6b94-47c8-873c-0f38960a04e3))
  (fp_poly
    (pts
      (xy 0.325 0.625)
      (xy -0.825 0.625)
      (xy -0.825 0.475)
      (xy 0.325 0.475)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 792f032f-9aee-46c7-bd70-4a5df0cbb216))
  (fp_line (start -1.05 0.275) (end -1.05 -0.275)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 176bfb8d-42c6-44d9-a458-f2254b99ba0c))
  (fp_line (start -0.825 -0.5) (end 0.825 -0.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a1c7779f-508d-41ed-9ed9-8aa061fb9ed0))
  (fp_line (start 0.825 0.5) (end -0.825 0.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c1529704-ca78-4d07-aea0-0b7e82531414))
  (fp_line (start 1.05 -0.275) (end 1.05 0.275)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 15a15623-0d06-4788-b5da-90d9c8ebcc5a))
  (fp_arc (start -1.05 -0.275) (mid -0.984099 -0.434099) (end -0.825 -0.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e5418873-451d-4e14-9ecd-2fa3f6b5ea05))
  (fp_arc (start -0.825 0.5) (mid -0.984099 0.434099) (end -1.05 0.275)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 492094d9-dc4d-418f-a682-86a7e2f2cd79))
  (fp_arc (start 0.825 -0.5) (mid 0.984099 -0.434099) (end 1.05 -0.275)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 5259d730-eabd-43c7-a012-833d86040960))
  (fp_arc (start 1.05 0.275) (mid 0.984099 0.434099) (end 0.825 0.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1314a9aa-0514-4b11-aa36-7a76de35d3a2))
  (fp_line (start -0.8 -0.4) (end 0.8 -0.4)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 9a64b94a-2d49-4a0b-96b8-c93749bf4daa))
  (fp_line (start -0.8 0.4) (end -0.8 -0.4)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 73c27f0d-4ed5-42d3-bb7e-a17a3a276368))
  (fp_line (start 0.8 -0.4) (end 0.8 0.4)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 3b924c2f-c26d-4dd2-ae67-6a457b56f7ee))
  (fp_line (start 0.8 0.4) (end -0.8 0.4)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 833c1a49-b54a-424d-b1c4-4ec4f90e5e15))
  (pad "" smd oval (at -0.675 0) (size 0.4 0.6) (layers "F.Paste") (tstamp e1b95ddf-067d-4fe8-8e4a-23b8c6181b44))
  (pad "" smd oval (at 0.675 0) (size 0.4 0.6) (layers "F.Paste") (tstamp 7b3f9a0b-cc5f-4f1f-afeb-6b5e9f042519))
  (pad "A" smd roundrect (at 0.675 0) (size 0.55 0.8) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2)
    (chamfer_ratio 0.05) (chamfer top_left bottom_left) (tstamp 1448ae02-1e93-4624-9894-8c783c035619))
  (pad "K" smd roundrect (at -0.675 0) (size 0.55 0.8) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2)
    (chamfer_ratio 0.05) (chamfer top_right bottom_right) (tstamp 598157c6-f4d3-448a-b042-9ca006a79519))
  (model "${KICAD7_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
