(module Coded_Rotary_Switch_Apem_P25SMT103 (layer F.Cu) (tedit 5B4B636A)
  (solder_mask_margin 0.001)
  (solder_paste_margin -0.05)
  (attr smd)
  (fp_text reference REF** (at 0 -4.2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Coded_Rotary_Switch_Apem_P25SMT103 (at 0 3.2) (layer F.Fab)
    (effects (font (size 0.2 0.2) (thickness 0.05)))
  )
  (fp_line (start -3.5 -3.5) (end 3.5 -3.5) (layer F.Fab) (width 0.05))
  (fp_line (start 3.5 -3.5) (end 3.5 3.5) (layer F.Fab) (width 0.05))
  (fp_line (start 3.5 3.5) (end -3.5 3.5) (layer F.Fab) (width 0.05))
  (fp_line (start -3.5 3.5) (end -3.5 -3.5) (layer F.Fab) (width 0.05))
  (fp_line (start -3.7 -3.7) (end -3.7 -3.3) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.7 -3.7) (end -2.7 -3.7) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.7 -3.7) (end 3.7 -3.3) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.7 -3.7) (end 2.7 -3.7) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.7 3.7) (end -3.7 3.3) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.7 3.7) (end -2.7 3.7) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.7 3.7) (end 3.7 3.3) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.7 3.7) (end 2.7 3.7) (layer F.SilkS) (width 0.15))
  (fp_line (start -5.7 0) (end -5.9 -0.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -5.9 -0.1) (end -5.9 0.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -5.9 0.1) (end -5.7 0) (layer F.SilkS) (width 0.15))
  (pad C smd roundrect (at -4 -2.54) (size 3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 1 smd roundrect (at -4 0) (size 3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 2 smd roundrect (at -4 2.54) (size 3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 4 smd roundrect (at 4 2.54) (size 3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 8 smd roundrect (at 4 0) (size 3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad C smd roundrect (at 4 -2.54) (size 3 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (model ${KICAD7_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/P25SMT_103x.stp
    (offset (xyz 0 0 0.15))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 -90))
  )
)
