(module InvenSense_ICS-40300 (layer F.Cu) (tedit 57518F8E)
  (solder_mask_margin 0.025)
  (solder_paste_margin -0.025)
  (attr smd)
  (fp_text reference U4 (at -0.9 -2.4) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value InvenSense_ICS-40300 (at -1 2.4) (layer F.Fab)
    (effects (font (size 0.25 0.25) (thickness 0.0625)))
  )
  (fp_text user Microphone (at -1 0 90) (layer B.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)) (justify mirror))
  )
  (fp_circle (center -3.4 2.4) (end -3.4 2.5) (layer F.SilkS) (width 0.125))
  (fp_line (start -3.5 2.1) (end -3 2.1) (layer F.SilkS) (width 0.125))
  (fp_line (start -3.5 2.1) (end -3.5 1.6) (layer F.SilkS) (width 0.125))
  (fp_line (start 1.6 2.1) (end 1.1 2.1) (layer F.SilkS) (width 0.125))
  (fp_line (start 1.6 2.1) (end 1.6 1.6) (layer F.SilkS) (width 0.125))
  (fp_line (start 1.6 -2.1) (end 1.6 -1.6) (layer F.SilkS) (width 0.125))
  (fp_line (start 1.6 -2.1) (end 1.1 -2.1) (layer F.SilkS) (width 0.125))
  (fp_line (start -3.5 -2.1) (end -3 -2.1) (layer F.SilkS) (width 0.125))
  (fp_line (start -3.5 -2.1) (end -3.5 -1.6) (layer F.SilkS) (width 0.125))
  (fp_line (start -3.3 -1.88) (end 1.42 -1.88) (layer F.Fab) (width 0.125))
  (fp_line (start 1.42 -1.88) (end 1.42 1.88) (layer F.Fab) (width 0.125))
  (fp_line (start 1.42 1.88) (end -3.3 1.88) (layer F.Fab) (width 0.125))
  (fp_line (start -3.3 -1.88) (end -3.3 1.88) (layer F.Fab) (width 0.125))
  (fp_circle (center 0 0) (end 0.695 0) (layer F.Mask) (width 0.35))
  (fp_circle (center 0 0) (end 0.695 0) (layer F.Cu) (width 0.29))
  (pad "" np_thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask)
    (solder_mask_margin 0.05))
  (pad 1 smd circle (at -2.62 1.2) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd circle (at -2.62 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd circle (at -2.62 -1.2) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd circle (at 0.79 1.27) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd circle (at 0.79 -1.27) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd circle (at -0.695 0) (size 0.29 0.29) (layers F.Cu F.Paste))
  (pad 3 smd circle (at 0 -0.695) (size 0.29 0.29) (layers F.Cu F.Paste))
  (pad 3 smd circle (at 0.695 0) (size 0.29 0.29) (layers F.Cu F.Paste))
  (pad 3 smd circle (at 0 0.695) (size 0.29 0.29) (layers F.Cu F.Paste))
  (pad 3 smd circle (at -0.601888 -0.3475) (size 0.29 0.29) (layers F.Cu F.Paste))
  (pad 3 smd circle (at -0.601888 0.3475) (size 0.29 0.29) (layers F.Cu F.Paste))
  (pad 3 smd circle (at 0.601888 -0.3475) (size 0.29 0.29) (layers F.Cu F.Paste))
  (pad 3 smd circle (at 0.601888 0.3475) (size 0.29 0.29) (layers F.Cu F.Paste))
  (pad 3 smd circle (at -0.3475 -0.601888) (size 0.29 0.29) (layers F.Cu F.Paste))
  (pad 3 smd circle (at 0.3475 -0.601888) (size 0.29 0.29) (layers F.Cu F.Paste))
  (pad 3 smd circle (at 0.3475 0.601888) (size 0.29 0.29) (layers F.Cu F.Paste))
  (pad 3 smd circle (at -0.3475 0.601888) (size 0.29 0.29) (layers F.Cu F.Paste))
)
