(footprint "Arc_12x_Ri_1.2" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (zone_connect 0)
  (attr board_only exclude_from_pos_files exclude_from_bom)
  (fp_text reference "REF**" (at 0 -8.075 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2c79dc91-7d87-4312-a8b9-19715fd00ffa)
  )
  (fp_text value "Arc_12x_Ri_1.2" (at 0 -6.575 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 5beec144-4cc1-474b-a704-c5bb50798690)
  )
  (fp_text user "${REFERENCE}" (at 0 -5.075 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 329fd6c7-7418-4566-b934-69bde1aafa29)
  )
  (fp_circle (center 0 0) (end 0.6 0)
    (stroke (width 0) (type solid)) (fill solid) (layer "Dwgs.User") (tstamp 16722dac-af92-4300-b5c4-294d0b161305))
  (pad "1" smd custom (at -0.925 0) (size 0.15 0.15) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 0.925 -0.925) (end 1.85 0) (width 0.15))
    ) (tstamp 8c616d0e-77cb-4e2c-a29e-056569a9adb6))
  (pad "1" smd custom (at 0.925 0) (size 0.15 0.15) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -1.85 0) (mid -0.925 -0.925) (end 0 0) (width 0.15))
    ) (tstamp ff126c43-c66e-474b-9638-f98ef6b53d5e))
  (pad "2" smd custom (at -1.225 0) (size 0.15 0.15) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 1.225 -1.225) (end 2.45 0) (width 0.15))
    ) (tstamp f6ebe360-74e6-40be-86d2-4e7306b4ade5))
  (pad "2" smd custom (at 1.225 0) (size 0.15 0.15) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -2.45 0) (mid -1.225 -1.225) (end 0 0) (width 0.15))
    ) (tstamp 89812f32-6ea5-4842-9df6-c5be30d79eb1))
  (pad "3" smd custom (at -1.525 0) (size 0.15 0.15) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 1.525 -1.525) (end 3.05 0) (width 0.15))
    ) (tstamp d8e7a367-e428-44a5-b33d-768579c1924a))
  (pad "3" smd custom (at 1.525 0) (size 0.15 0.15) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -3.05 0) (mid -1.525 -1.525) (end 0 0) (width 0.15))
    ) (tstamp b11722d2-865b-411c-91ae-1cd4a2465e5c))
  (pad "4" smd custom (at -1.825 0) (size 0.15 0.15) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 1.825 -1.825) (end 3.65 0) (width 0.15))
    ) (tstamp 62795957-7ffd-4884-9092-9647848c6a51))
  (pad "4" smd custom (at 1.825 0) (size 0.15 0.15) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -3.65 0) (mid -1.825 -1.825) (end 0 0) (width 0.15))
    ) (tstamp fe01bc1c-1611-472c-8bde-089720c85808))
  (pad "5" smd custom (at -2.125 0) (size 0.15 0.15) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 2.125 -2.125) (end 4.25 0) (width 0.15))
    ) (tstamp da359632-d1d3-44c7-b3f6-f14b7b5afe6e))
  (pad "5" smd custom (at 2.125 0) (size 0.15 0.15) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -4.25 0) (mid -2.125 -2.125) (end 0 0) (width 0.15))
    ) (tstamp 0485f9d0-8d81-4ed0-bd3f-80c43d2848a9))
  (pad "6" smd custom (at -2.425 0) (size 0.15 0.15) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 2.425 -2.425) (end 4.85 0) (width 0.15))
    ) (tstamp 910dfb7d-d72a-41d6-844c-2825995e36b7))
  (pad "6" smd custom (at 2.425 0) (size 0.15 0.15) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -4.85 0) (mid -2.425 -2.425) (end 0 0) (width 0.15))
    ) (tstamp 9251f532-f193-4003-8f2a-b1f0effaf13d))
  (pad "7" smd custom (at -2.725 0) (size 0.15 0.15) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 2.725 -2.725) (end 5.45 0) (width 0.15))
    ) (tstamp 36f99933-305d-4b8b-a471-31128f144de3))
  (pad "7" smd custom (at 2.725 0) (size 0.15 0.15) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -5.45 0) (mid -2.725 -2.725) (end 0 0) (width 0.15))
    ) (tstamp 7a706acf-6ac4-44c3-945e-5b6db412a70e))
  (pad "8" smd custom (at -3.025 0) (size 0.15 0.15) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 3.025 -3.025) (end 6.05 0) (width 0.15))
    ) (tstamp ca5e2673-301f-4271-b07c-b3fdf7f00ade))
  (pad "8" smd custom (at 3.025 0) (size 0.15 0.15) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -6.05 0) (mid -3.025 -3.025) (end 0 0) (width 0.15))
    ) (tstamp 0ab5cc5a-0c73-4d37-a669-2f2f7160c38d))
  (pad "9" smd custom (at -3.325 0) (size 0.15 0.15) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 3.325 -3.325) (end 6.65 0) (width 0.15))
    ) (tstamp 5d425463-e96f-4343-9ada-2004ca904cfd))
  (pad "9" smd custom (at 3.325 0) (size 0.15 0.15) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -6.65 0) (mid -3.325 -3.325) (end 0 0) (width 0.15))
    ) (tstamp 7b34fce3-9f42-4a77-8b7d-57c634eb8856))
  (pad "10" smd custom (at -3.625 0) (size 0.15 0.15) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 3.625 -3.625) (end 7.25 0) (width 0.15))
    ) (tstamp 2f7ab0c3-1fc2-4d10-a4a9-a58e1abc9524))
  (pad "10" smd custom (at 3.625 0) (size 0.15 0.15) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -7.25 0) (mid -3.625 -3.625) (end 0 0) (width 0.15))
    ) (tstamp b9dfcde4-3abe-47e6-a4bd-778221dd058e))
  (pad "11" smd custom (at -3.925 0) (size 0.15 0.15) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 3.925 -3.925) (end 7.85 0) (width 0.15))
    ) (tstamp faa76b6a-b751-4708-a160-0c334d0ad5bf))
  (pad "11" smd custom (at 3.925 0) (size 0.15 0.15) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -7.85 0) (mid -3.925 -3.925) (end 0 0) (width 0.15))
    ) (tstamp 2f83c781-95b2-4019-95f0-6c5563a32614))
  (pad "12" smd custom (at -4.225 0) (size 0.15 0.15) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start 0 0) (mid 4.225 -4.225) (end 8.45 0) (width 0.15))
    ) (tstamp 53ec1f51-3fdd-4260-a4bd-25b8e151f18b))
  (pad "12" smd custom (at 4.225 0) (size 0.15 0.15) (layers "F.Cu")
    (thermal_bridge_angle 45)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_arc (start -8.45 0) (mid -4.225 -4.225) (end 0 0) (width 0.15))
    ) (tstamp dd4ed375-2752-44ad-8e75-f9b4df0a72d1))
)
