(footprint "SOT-23-3_GSD" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (tags "SOT-23 SOT-23-3 SOT23")
  (property "LCSC" "C2910165")
  (property "MFG" "Changjing")
  (property "MPN" "2N7002K")
  (property "Sheetfile" "../../library/blocks/Ultrasonic Distance Sensor.kicad_sch")
  (property "Sheetname" "Ultrasonic")
  (solder_mask_margin 0.01)
  (solder_paste_margin -0.04)
  (attr smd)
  (fp_text reference "Q9" (at 1.25 -1.25 -90) (layer "F.SilkS") hide
      (effects (font (size 0.6 0.6) (thickness 0.125)))
    (tstamp 4344b3cb-c579-4f2b-8deb-d43658d15094)
  )
  (fp_text value "MOSFET_N" (at 0 0.4 -180) (layer "F.Fab")
      (effects (font (size 0.15 0.15) (thickness 0.02)))
    (tstamp b6311b33-3cb6-48c2-8bbf-b57c3b420b16)
  )
  (fp_line (start -1.7 -0.65) (end -1.7 0.65)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1e7ba79f-459f-4df7-b40e-0452a94956e1))
  (fp_line (start -1.55 1.25) (end -1.551535 0.878453)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp eb07ce06-afc9-4114-8dfd-81f4dc2a04fc))
  (fp_line (start -1.45 -0.9) (end -0.55 -0.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f57a2df2-3682-40e0-a595-a60a9e4d8e20))
  (fp_line (start -1.2 1.6) (end -0.8 1.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 05e8f291-d9c8-48e7-b929-75938496e210))
  (fp_line (start -0.55 -0.9) (end -0.55 -1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 686e34d5-1252-4386-890b-113fe8bbd1c6))
  (fp_line (start -0.45 0.9) (end 0.45 0.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 3d1377dd-df00-430b-bbfe-fa2b34b9b20f))
  (fp_line (start -0.45 1.25) (end -0.45 0.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp de52b5de-b9ef-4c9f-a9d1-70e6fd2ee737))
  (fp_line (start 0.2 -1.6) (end -0.2 -1.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2c441817-40c2-413e-a050-8fbfb76da780))
  (fp_line (start 0.45 1.25) (end 0.45 0.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 8ae6c30f-460e-4f77-bbc7-56c23a15eb1c))
  (fp_line (start 0.55 -0.9) (end 0.55 -1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 5abe12c7-8535-416f-a5ef-37f88b3ea24f))
  (fp_line (start 1.2 1.6) (end 0.8 1.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 41a0f8d2-95da-4530-bf81-6b88a5c1eceb))
  (fp_line (start 1.45 -0.9) (end 0.55 -0.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ffba60ce-e1e9-474b-b7a8-ee32de5e24bf))
  (fp_line (start 1.55 1.25) (end 1.551535 0.878453)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f5f339bf-c692-44c4-82de-f80a76748447))
  (fp_line (start 1.7 -0.65) (end 1.7 0.65)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c038415c-ae31-4bf1-9113-dad25c0beaec))
  (fp_arc (start -1.7 -0.65) (mid -1.626777 -0.826777) (end -1.45 -0.9)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0336e97b-c2ae-48a7-ae58-f1c0065a1868))
  (fp_arc (start -1.551535 0.878453) (mid -1.659623 0.786228) (end -1.7 0.65)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp abda0956-eb87-4b8c-b83b-9778ad43f5a1))
  (fp_arc (start -1.2 1.6) (mid -1.447487 1.497487) (end -1.55 1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 589289ef-ab72-4bbe-a1d2-776b7c507a4d))
  (fp_arc (start -0.55 -1.25) (mid -0.447487 -1.497487) (end -0.2 -1.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 15668e8b-2b5e-4055-9601-2ea023ee87ba))
  (fp_arc (start -0.45 1.25) (mid -0.552513 1.497487) (end -0.8 1.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 79e3bbaa-ac3d-4721-a67b-61efa7da3728))
  (fp_arc (start 0.2 -1.6) (mid 0.447487 -1.497487) (end 0.55 -1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 660f267c-9cc8-4ee2-91c0-5a311ceebbf0))
  (fp_arc (start 0.8 1.6) (mid 0.552513 1.497487) (end 0.45 1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6f298bad-f49b-40b9-b26c-cdcd273b4342))
  (fp_arc (start 1.45 -0.9) (mid 1.626777 -0.826777) (end 1.7 -0.65)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 5d39389f-5552-4264-80dd-cee4db6f15fd))
  (fp_arc (start 1.55 1.25) (mid 1.447487 1.497487) (end 1.2 1.6)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 8eda1b71-8df4-495f-838f-a359285739a0))
  (fp_arc (start 1.7 0.65) (mid 1.659623 0.786228) (end 1.551535 0.878453)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 61d47960-728c-4c1e-aa56-6742ebe6845f))
  (fp_line (start -1.45 -0.65) (end -1.45 0.65)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 64e1e0c4-12c0-40e0-9eda-b4e30d1d374e))
  (fp_line (start -1.45 -0.65) (end 1.45 -0.65)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp fb2f988c-d884-4e55-afc9-8cb0306f55b3))
  (fp_line (start 1.45 -0.65) (end 1.45 0.65)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 77b78c52-3cd4-42ee-855a-70c8c47b4e46))
  (fp_line (start 1.45 0.65) (end -1.45 0.65)
    (stroke (width 0.05) (type solid)) (layer "F.Fab") (tstamp 592374f7-5cf1-46cf-9812-1d7dea8bf179))
  (fp_circle (center -1.3 0.5) (end -1.3 0.65)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.Fab") (tstamp 297cb59b-a8d1-40f6-986d-f41dfec613f6))
  (pad "D" smd roundrect (at 0 -1) (size 0.8 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b62df80b-9dc3-4a8a-bb1f-f6e8074f468d))
  (pad "G" smd roundrect (at -1 1) (size 0.8 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp f52111b5-c58e-4928-b018-d9dd51021753))
  (pad "S" smd roundrect (at 1 1) (size 0.8 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp bab67d5d-1bbb-4c43-bca8-5e40acce33e1))
  (model "${KICAD7_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 -90))
  )
)
