(footprint "WSON-10-1EP_2.5x2.5mm_P0.5mm_EP1.2x2mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "WSON, 10 Pin (http://www.ti.com/lit/gpn/tps63030#page=24), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "WSON NoLead")
	(property "Reference" "U3"
		(at 0 -2.05 0)
		(layer "F.SilkS")
		(uuid "f79c3a84-dec9-445e-a505-5684922ba921")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "TPS7A90"
		(at 0 2.05 0)
		(layer "F.Fab")
		(uuid "ac6986a4-1c26-4344-9b8f-4f4fc8a580a0")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.0625)
			)
		)
	)
	(property "Footprint" "Package_SON:WSON-10-1EP_2.5x2.5mm_P0.5mm_EP1.2x2mm"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "30b3b47d-a5ec-4ac8-82ee-50f496ed5531")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps7a90.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4b6693d6-535b-4b6e-82b6-416c9de85795")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "0.5A, High-Accuracy, Low-Noise LDO Voltage Regulator, Texas S-PDSO-N10"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "226c1c74-8021-4d11-a52e-1ad42f16e420")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" "C840111"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6bef7dc8-b9a8-44c2-a5d7-52255c3ad2fc")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "TI"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "dcdbb5a2-769c-400d-aaae-b9bba7f73822")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "TPS7A9001DSKR"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "01be7ddd-bfe2-4951-ae9a-fe061745d376")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Sim.Enable" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "35a90f99-2c62-42bd-a90c-da76c10f95ac")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start -1.25 -1.5)
		(end 1.25 -1.35)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "8c439c96-8c0e-4494-96e7-3a7372baebcb")
	)
	(fp_rect
		(start -1.25 1.35)
		(end 1.25 1.5)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "ddb42242-15e5-4697-8803-10dd65ba51fd")
	)
	(fp_poly
		(pts
			(xy -1.525 -1) (xy -1.675 -1.15) (xy -1.675 -0.85)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "c259fc6a-7bd9-4e34-a1a5-b030e78bef0a")
	)
	(fp_line
		(start -1.6 -1.025)
		(end -1.6 1.025)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "aa81a75e-52c1-4fe5-9ed0-72dbc81f4709")
	)
	(fp_line
		(start -1.5 -1.25)
		(end -1.5 -1.225)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "328aef94-d16f-4624-988e-b42c4db901c3")
	)
	(fp_line
		(start -1.5 1.25)
		(end -1.5 1.225)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "40e4cdf2-5b7a-4df1-92fa-2037855610fe")
	)
	(fp_line
		(start -1.25 1.5)
		(end 1.25 1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "38c5a466-d701-4357-8e9a-0e5c22942080")
	)
	(fp_line
		(start 1.25 -1.5)
		(end -1.25 -1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "870333a4-a136-46a4-bf68-e5231c537303")
	)
	(fp_line
		(start 1.5 -1.25)
		(end 1.5 -1.225)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "5e9b95e2-1674-403c-a874-4e8f8a308199")
	)
	(fp_line
		(start 1.5 1.25)
		(end 1.5 1.225)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "d1ce59e5-547b-4ec6-8869-2e34a5fac576")
	)
	(fp_line
		(start 1.6 1.025)
		(end 1.6 -1.025)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "c2199c40-f51b-4e6a-93ff-e0cc3cd6a973")
	)
	(fp_arc
		(start -1.6 -1.025)
		(mid -1.573607 -1.136803)
		(end -1.5 -1.225)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "cdf58f12-0b2b-404c-8c8b-05f3b0ffceb6")
	)
	(fp_arc
		(start -1.5 -1.25)
		(mid -1.426777 -1.426777)
		(end -1.25 -1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "53e25b6d-0cba-4ac4-9aac-f11b1ac382a3")
	)
	(fp_arc
		(start -1.5 1.225)
		(mid -1.573607 1.136803)
		(end -1.6 1.025)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "749d8e66-e481-4616-a4b4-11bd2e2fb453")
	)
	(fp_arc
		(start -1.25 1.5)
		(mid -1.426777 1.426777)
		(end -1.5 1.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "851b1cd7-cb97-47b1-aae0-5332775de03f")
	)
	(fp_arc
		(start 1.25 -1.5)
		(mid 1.426777 -1.426777)
		(end 1.5 -1.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "113d0c33-2c57-4e41-bcec-7438946f361c")
	)
	(fp_arc
		(start 1.5 -1.225)
		(mid 1.573607 -1.136803)
		(end 1.6 -1.025)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "29e45875-48cc-4a66-9ecc-f3d2f54431be")
	)
	(fp_arc
		(start 1.5 1.25)
		(mid 1.426777 1.426777)
		(end 1.25 1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9075a779-2202-442a-b71f-07258643c5cc")
	)
	(fp_arc
		(start 1.6 1.025)
		(mid 1.573607 1.136803)
		(end 1.5 1.225)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "b7d0f404-f9f2-40f4-8273-3f67afb073d8")
	)
	(fp_rect
		(start -1.25 -1.25)
		(end 1.25 1.25)
		(stroke
			(width 0.025)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "07771dca-6b9a-46f5-b8eb-10fbf0881f7c")
	)
	(fp_text user "${REFERENCE}"
		(at -0.025 1.7 0)
		(layer "F.Fab")
		(uuid "28b41d71-5fa0-4e34-88a0-91775a799ab4")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.05)
				(bold yes)
			)
		)
	)
	(pad "" smd oval
		(at -1.15 -1)
		(size 0.45 0.2)
		(layers "F.Paste")
		(uuid "b8d7df08-270c-4d08-b768-f383b4ffab88")
	)
	(pad "" smd oval
		(at -1.15 -0.5)
		(size 0.45 0.2)
		(layers "F.Paste")
		(uuid "6e9f4d48-c33c-48f5-8114-a7d4d15a5978")
	)
	(pad "" smd oval
		(at -1.15 0)
		(size 0.45 0.2)
		(layers "F.Paste")
		(uuid "775d021a-8b42-46f6-a317-5b557df81942")
	)
	(pad "" smd oval
		(at -1.15 0.5)
		(size 0.45 0.2)
		(layers "F.Paste")
		(uuid "d2bbac54-6880-45b4-af8f-ed0108feed1f")
	)
	(pad "" smd oval
		(at -1.15 1)
		(size 0.45 0.2)
		(layers "F.Paste")
		(uuid "4bca76a9-a565-4bf3-b293-f84d8d236685")
	)
	(pad "" smd roundrect
		(at -0.3 -0.5)
		(size 0.48 0.81)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "d3e92193-7a35-42b3-86de-e369cc97eaf4")
	)
	(pad "" smd roundrect
		(at -0.3 0.5)
		(size 0.48 0.81)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "e0ca2bf0-56d9-4533-a8ea-7dbdd8a643b2")
	)
	(pad "" smd roundrect
		(at 0.3 -0.5)
		(size 0.48 0.81)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "11f64a4f-0fd5-4f10-9fcf-b7c0258536d2")
	)
	(pad "" smd roundrect
		(at 0.3 0.5)
		(size 0.48 0.81)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "eafc13ce-8beb-405f-aaff-2467a097434f")
	)
	(pad "" smd oval
		(at 1.15 -1)
		(size 0.45 0.2)
		(layers "F.Paste")
		(uuid "2da448da-9dcf-49ad-912c-f4d14770fc91")
	)
	(pad "" smd oval
		(at 1.15 -0.5)
		(size 0.45 0.2)
		(layers "F.Paste")
		(uuid "5bffbe69-95d9-43aa-b933-caaab6fd4b49")
	)
	(pad "" smd oval
		(at 1.15 0)
		(size 0.45 0.2)
		(layers "F.Paste")
		(uuid "a561b2b7-067f-4663-afe4-4fdd12337aae")
	)
	(pad "" smd oval
		(at 1.15 0.5)
		(size 0.45 0.2)
		(layers "F.Paste")
		(uuid "97b4b9bd-f3e3-454b-9a24-b962f17b97a0")
	)
	(pad "" smd oval
		(at 1.15 1)
		(size 0.45 0.2)
		(layers "F.Paste")
		(uuid "aafcb49e-067e-4c7a-87a2-04803c28e2fb")
	)
	(pad "1" smd roundrect
		(at -1.15 -1)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "3990f566-715b-472d-9e6d-3bbf3f8a508e")
	)
	(pad "2" smd roundrect
		(at -1.15 -0.5)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "72cd36b6-aaa2-4c37-a17f-814f228eb389")
	)
	(pad "3" smd roundrect
		(at -1.15 0)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "5978effa-bf39-4b98-9874-83dffebf5a16")
	)
	(pad "4" smd roundrect
		(at -1.15 0.5)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "44ad0295-643e-4223-bb7e-bab6ef57151a")
	)
	(pad "5" smd roundrect
		(at -1.15 1)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "134e090d-e446-4e98-af79-5c0cdf339a41")
	)
	(pad "6" smd roundrect
		(at 1.15 1 180)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "5b708934-15e2-47f4-b3df-aa83c7a6f6de")
	)
	(pad "7" smd roundrect
		(at 1.15 0.5 180)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "e921ace8-d491-4648-9380-344d8144179b")
	)
	(pad "8" smd roundrect
		(at 1.15 0 180)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "34234a5d-8ef3-4a2d-be5e-b7985427451d")
	)
	(pad "9" smd roundrect
		(at 1.15 -0.5 180)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "a1344f6c-1a6b-4ede-ae12-14d42d853f8c")
	)
	(pad "10" smd roundrect
		(at 1.15 -1 180)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "7b3268fa-a376-42ee-8851-b6be218f8a05")
	)
	(pad "11" smd roundrect
		(at 0 0)
		(size 1.2 2)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.04166666667)
		(zone_connect 2)
		(uuid "9ca67fb4-1905-4772-a5ba-447eb07149fd")
	)
	(model "${KICAD8_3DMODEL_DIR}/Package_SON.3dshapes/WSON-10-1EP_2.5x2.5mm_P0.5mm_EP1.2x2mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
